Enumerations
HAL AES State
Peripheral Driver » HAL Driver » AES » Enumerations

## Enumerations
enum | hal_aes_state_t { HAL_AES_STATE_RESET = 0x00, HAL_AES_STATE_READY = 0x01, HAL_AES_STATE_BUSY = 0x02 }
| HAL AES State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_aes_state_t

enum hal_aes_state_t

HAL AES State Enumerations definition.

Enumerator
HAL_AES_STATE_RESET | Peripheral not initialized
HAL_AES_STATE_READY | Peripheral initialized and ready for use
HAL_AES_STATE_BUSY | Peripheral in indirect mode and busy

Definition at line 77 of file hal_aes.h.