ble_id.h
Go to the documentation of this file.
1 /**
2 ****************************************************************************************
3 *
4 * @file ble_id.h
5 *
6 * @brief define ble message id
7 *
8 ****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE
40 * @{
41 */
42
43 /**
44 * @addtogroup BLE_ID
45 * @{
46 * @brief Message ID and hci cmd/evt opcode defines.
47 */
48
49 #ifndef __BLE_ID_H__
50 #define __BLE_ID_H__
51
52 #include <stdint.h>
53
54 /** @addtogroup BLE_ID_DEFINES Defines
55 * @{ */
56
57 /// Message identifier index
58 #define MSG_ID(task, idx) (TASK_FIRST_MSG((TASK_ID_ ## task)) + idx)
59
60 /// Build the first message ID of a task. (in fact a ke_msg_id_t)
61 #define TASK_FIRST_MSG(task) ((uint16_t)((task) << 8))
62
63 /// Default message ID
64 #define KE_MSG_DEFAULT_HANDLER (0xFFFF)
65
66 /// Number of L2CC TASK Deprecated messages
67 #define L2CC_NB_DEPRECATED_MSG (4)
68
69 /**@} */
70
71 /** @addtogroup BLE_ID_ENUMS Enums
72 * @{ */
73
74 enum hci_opcode
75 {
76 HCI_NO_OPERATION_CMD_OPCODE = 0x0000,
77
78 //Link Control Commands
79 HCI_INQ_CMD_OPCODE = 0x0401,
80 HCI_INQ_CANCEL_CMD_OPCODE = 0x0402,
81 HCI_PER_INQ_MODE_CMD_OPCODE = 0x0403,
82 HCI_EXIT_PER_INQ_MODE_CMD_OPCODE = 0x0404,
83 HCI_CREATE_CON_CMD_OPCODE = 0x0405,
84 HCI_DISCONNECT_CMD_OPCODE = 0x0406,
85 HCI_CREATE_CON_CANCEL_CMD_OPCODE = 0x0408,
86 HCI_ACCEPT_CON_REQ_CMD_OPCODE = 0x0409,
87 HCI_REJECT_CON_REQ_CMD_OPCODE = 0x040A,
88 HCI_LK_REQ_REPLY_CMD_OPCODE = 0x040B,
89 HCI_LK_REQ_NEG_REPLY_CMD_OPCODE = 0x040C,
90 HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE = 0x040D,
91 HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE = 0x040E,
92 HCI_CHG_CON_PKT_TYPE_CMD_OPCODE = 0x040F,
93 HCI_AUTH_REQ_CMD_OPCODE = 0x0411,
94 HCI_SET_CON_ENC_CMD_OPCODE = 0x0413,
95 HCI_CHG_CON_LK_CMD_OPCODE = 0x0415,
96 HCI_MASTER_LK_CMD_OPCODE = 0x0417,
97 HCI_REM_NAME_REQ_CMD_OPCODE = 0x0419,
98 HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE = 0x041A,
99 HCI_RD_REM_SUPP_FEATS_CMD_OPCODE = 0x041B,
100 HCI_RD_REM_EXT_FEATS_CMD_OPCODE = 0x041C,
101 HCI_RD_REM_VER_INFO_CMD_OPCODE = 0x041D,
102 HCI_RD_CLK_OFF_CMD_OPCODE = 0x041F,
103 HCI_RD_LMP_HDL_CMD_OPCODE = 0x0420,
104 HCI_SETUP_SYNC_CON_CMD_OPCODE = 0x0428,
105 HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE = 0x0429,
106 HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE = 0x042A,
107 HCI_IO_CAP_REQ_REPLY_CMD_OPCODE = 0x042B,
108 HCI_USER_CFM_REQ_REPLY_CMD_OPCODE = 0x042C,
109 HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE = 0x042D,
110 HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE = 0x042E,
111 HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE = 0x042F,
112 HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE = 0x0430,
113 HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE = 0x0433,
114 HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE = 0x0434,
115 HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE = 0x043D,
116 HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE = 0x043E,
117 HCI_TRUNC_PAGE_CMD_OPCODE = 0x043F,
118 HCI_TRUNC_PAGE_CAN_CMD_OPCODE = 0x0440,
119 HCI_SET_CON_SLV_BCST_CMD_OPCODE = 0x0441,
120 HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE = 0x0442,
121 HCI_START_SYNC_TRAIN_CMD_OPCODE = 0x0443,
122 HCI_REC_SYNC_TRAIN_CMD_OPCODE = 0x0444,
123 HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE = 0x0445,
124
125 //Link Policy Commands
126 HCI_HOLD_MODE_CMD_OPCODE = 0x0801,
127 HCI_SNIFF_MODE_CMD_OPCODE = 0x0803,
128 HCI_EXIT_SNIFF_MODE_CMD_OPCODE = 0x0804,
129 HCI_PARK_STATE_CMD_OPCODE = 0x0805,
130 HCI_EXIT_PARK_STATE_CMD_OPCODE = 0x0806,
131 HCI_QOS_SETUP_CMD_OPCODE = 0x0807,
132 HCI_ROLE_DISCOVERY_CMD_OPCODE = 0x0809,
133 HCI_SWITCH_ROLE_CMD_OPCODE = 0x080B,
134 HCI_RD_LINK_POL_STG_CMD_OPCODE = 0x080C,
135 HCI_WR_LINK_POL_STG_CMD_OPCODE = 0x080D,
136 HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE = 0x080E,
137 HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE = 0x080F,
138 HCI_FLOW_SPEC_CMD_OPCODE = 0x0810,
139 HCI_SNIFF_SUB_CMD_OPCODE = 0x0811,
140
141 //Controller and Baseband Commands
142 HCI_SET_EVT_MASK_CMD_OPCODE = 0x0C01,
143 HCI_RESET_CMD_OPCODE = 0x0C03,
144 HCI_SET_EVT_FILTER_CMD_OPCODE = 0x0C05,
145 HCI_FLUSH_CMD_OPCODE = 0x0C08,
146 HCI_RD_PIN_TYPE_CMD_OPCODE = 0x0C09,
147 HCI_WR_PIN_TYPE_CMD_OPCODE = 0x0C0A,
148 HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE = 0x0C0B,
149 HCI_RD_STORED_LK_CMD_OPCODE = 0x0C0D,
150 HCI_WR_STORED_LK_CMD_OPCODE = 0x0C11,
151 HCI_DEL_STORED_LK_CMD_OPCODE = 0x0C12,
152 HCI_WR_LOCAL_NAME_CMD_OPCODE = 0x0C13,
153 HCI_RD_LOCAL_NAME_CMD_OPCODE = 0x0C14,
154 HCI_RD_CON_ACCEPT_TO_CMD_OPCODE = 0x0C15,
155 HCI_WR_CON_ACCEPT_TO_CMD_OPCODE = 0x0C16,
156 HCI_RD_PAGE_TO_CMD_OPCODE = 0x0C17,
157 HCI_WR_PAGE_TO_CMD_OPCODE = 0x0C18,
158 HCI_RD_SCAN_EN_CMD_OPCODE = 0x0C19,
159 HCI_WR_SCAN_EN_CMD_OPCODE = 0x0C1A,
160 HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE = 0x0C1B,
161 HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE = 0x0C1C,
162 HCI_RD_INQ_SCAN_ACT_CMD_OPCODE = 0x0C1D,
163 HCI_WR_INQ_SCAN_ACT_CMD_OPCODE = 0x0C1E,
164 HCI_RD_AUTH_EN_CMD_OPCODE = 0x0C1F,
165 HCI_WR_AUTH_EN_CMD_OPCODE = 0x0C20,
166 HCI_RD_CLASS_OF_DEV_CMD_OPCODE = 0x0C23,
167 HCI_WR_CLASS_OF_DEV_CMD_OPCODE = 0x0C24,
168 HCI_RD_VOICE_STG_CMD_OPCODE = 0x0C25,
169 HCI_WR_VOICE_STG_CMD_OPCODE = 0x0C26,
170 HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE = 0x0C27,
171 HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE = 0x0C28,
172 HCI_RD_NB_BDCST_RETX_CMD_OPCODE = 0x0C29,
173 HCI_WR_NB_BDCST_RETX_CMD_OPCODE = 0x0C2A,
174 HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE = 0x0C2B,
175 HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE = 0x0C2C,
176 HCI_RD_TX_PWR_LVL_CMD_OPCODE = 0x0C2D,
177 HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE = 0x0C2E,
178 HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE = 0x0C2F,
179 HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE = 0x0C31,
180 HCI_HOST_BUF_SIZE_CMD_OPCODE = 0x0C33,
181 HCI_HOST_NB_CMP_PKTS_CMD_OPCODE = 0x0C35,
182 HCI_RD_LINK_SUPV_TO_CMD_OPCODE = 0x0C36,
183 HCI_WR_LINK_SUPV_TO_CMD_OPCODE = 0x0C37,
184 HCI_RD_NB_SUPP_IAC_CMD_OPCODE = 0x0C38,
185 HCI_RD_CURR_IAC_LAP_CMD_OPCODE = 0x0C39,
186 HCI_WR_CURR_IAC_LAP_CMD_OPCODE = 0x0C3A,
187 HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE = 0x0C3F,
188 HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE = 0x0C42,
189 HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE = 0x0C43,
190 HCI_RD_INQ_MODE_CMD_OPCODE = 0x0C44,
191 HCI_WR_INQ_MODE_CMD_OPCODE = 0x0C45,
192 HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE = 0x0C46,
193 HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE = 0x0C47,
194 HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE = 0x0C48,
195 HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE = 0x0C49,
196 HCI_RD_EXT_INQ_RSP_CMD_OPCODE = 0x0C51,
197 HCI_WR_EXT_INQ_RSP_CMD_OPCODE = 0x0C52,
198 HCI_REFRESH_ENC_KEY_CMD_OPCODE = 0x0C53,
199 HCI_RD_SP_MODE_CMD_OPCODE = 0x0C55,
200 HCI_WR_SP_MODE_CMD_OPCODE = 0x0C56,
201 HCI_RD_LOC_OOB_DATA_CMD_OPCODE = 0x0C57,
202 HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE = 0x0C58,
203 HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE = 0x0C59,
204 HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE = 0x0C5A,
205 HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE = 0x0C5B,
206 HCI_ENH_FLUSH_CMD_OPCODE = 0x0C5F,
207 HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE = 0x0C60,
208 HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE = 0x0C63,
209 HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE = 0x0C66,
210 HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE = 0x0C67,
211 HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE = 0x0C68,
212 HCI_RD_LE_HOST_SUPP_CMD_OPCODE = 0x0C6C,
213 HCI_WR_LE_HOST_SUPP_CMD_OPCODE = 0x0C6D,
214 HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE = 0x0C6E,
215 HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE = 0x0C6F,
216 HCI_SET_MWS_SIGNALING_CMD_OPCODE = 0x0C70,
217 HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE = 0x0C71,
218 HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE = 0x0C72,
219 HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE = 0x0C73,
220 HCI_SET_RES_LT_ADDR_CMD_OPCODE = 0x0C74,
221 HCI_DEL_RES_LT_ADDR_CMD_OPCODE = 0x0C75,
222 HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE = 0x0C76,
223 HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE = 0x0C77,
224 HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE = 0x0C78,
225 HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE = 0x0C79,
226 HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE = 0x0C7A,
227 HCI_RD_AUTH_PAYL_TO_CMD_OPCODE = 0x0C7B,
228 HCI_WR_AUTH_PAYL_TO_CMD_OPCODE = 0x0C7C,
229 HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE = 0x0C7D,
230 HCI_RD_EXT_PAGE_TO_CMD_OPCODE = 0x0C7E,
231 HCI_WR_EXT_PAGE_TO_CMD_OPCODE = 0x0C7F,
232 HCI_RD_EXT_INQ_LEN_CMD_OPCODE = 0x0C80,
233 HCI_WR_EXT_INQ_LEN_CMD_OPCODE = 0x0C81,
234 HCI_SET_ECO_BASE_INTV_CMD_OPCODE = 0x0C82,
235 HCI_CONFIG_DATA_PATH_CMD_OPCODE = 0x0C83,
236
237 //Info Params
238 HCI_RD_LOCAL_VER_INFO_CMD_OPCODE = 0x1001,
239 HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE = 0x1002,
240 HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE = 0x1003,
241 HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE = 0x1004,
242 HCI_RD_BUF_SIZE_CMD_OPCODE = 0x1005,
243 HCI_RD_BD_ADDR_CMD_OPCODE = 0x1009,
244 HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE = 0x100A,
245 HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE = 0x100B,
246 HCI_RD_LOCAL_SP_OPT_CMD_OPCODE = 0x100C,
247 HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE = 0x100D,
248 HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE = 0x100E,
249 HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE = 0x100F,
250
251 //Status Params
252 HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE = 0x1401,
253 HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE = 0x1402,
254 HCI_RD_LINK_QUAL_CMD_OPCODE = 0x1403,
255 HCI_RD_RSSI_CMD_OPCODE = 0x1405,
256 HCI_RD_AFH_CH_MAP_CMD_OPCODE = 0x1406,
257 HCI_RD_CLK_CMD_OPCODE = 0x1407,
258 HCI_RD_ENC_KEY_SIZE_CMD_OPCODE = 0x1408,
259 HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE = 0x140C,
260
261 //Testing Commands
262 HCI_RD_LOOPBACK_MODE_CMD_OPCODE = 0x1801,
263 HCI_WR_LOOPBACK_MODE_CMD_OPCODE = 0x1802,
264 HCI_EN_DUT_MODE_CMD_OPCODE = 0x1803,
265 HCI_WR_SP_DBG_MODE_CMD_OPCODE = 0x1804,
266 HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE = 0x180A,
267
268 /// LE Commands Opcodes
269 HCI_LE_SET_EVT_MASK_CMD_OPCODE = 0x2001,
270 HCI_LE_RD_BUF_SIZE_CMD_OPCODE = 0x2002,
271 HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE = 0x2003,
272 HCI_LE_SET_RAND_ADDR_CMD_OPCODE = 0x2005,
273 HCI_LE_SET_ADV_PARAM_CMD_OPCODE = 0x2006,
274 HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE = 0x2007,
275 HCI_LE_SET_ADV_DATA_CMD_OPCODE = 0x2008,
276 HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE = 0x2009,
277 HCI_LE_SET_ADV_EN_CMD_OPCODE = 0x200A,
278 HCI_LE_SET_SCAN_PARAM_CMD_OPCODE = 0x200B,
279 HCI_LE_SET_SCAN_EN_CMD_OPCODE = 0x200C,
280 HCI_LE_CREATE_CON_CMD_OPCODE = 0x200D,
281 HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE = 0x200E,
282 HCI_LE_RD_WLST_SIZE_CMD_OPCODE = 0x200F,
283 HCI_LE_CLEAR_WLST_CMD_OPCODE = 0x2010,
284 HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE = 0x2011,
285 HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE = 0x2012,
286 HCI_LE_CON_UPDATE_CMD_OPCODE = 0x2013,
287 HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE = 0x2014,
288 HCI_LE_RD_CHNL_MAP_CMD_OPCODE = 0x2015,
289 HCI_LE_RD_REM_FEATS_CMD_OPCODE = 0x2016,
290 HCI_LE_ENC_CMD_OPCODE = 0x2017,
291 HCI_LE_RAND_CMD_OPCODE = 0x2018,
292 HCI_LE_EN_ENC_CMD_OPCODE = 0x2019,
293 HCI_LE_LTK_REQ_REPLY_CMD_OPCODE = 0x201A,
294 HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE = 0x201B,
295 HCI_LE_RD_SUPP_STATES_CMD_OPCODE = 0x201C,
296 HCI_LE_RX_TEST_V1_CMD_OPCODE = 0x201D,
297 HCI_LE_TX_TEST_V1_CMD_OPCODE = 0x201E,
298 HCI_LE_TEST_END_CMD_OPCODE = 0x201F,
299 HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE = 0x2020,
300 HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE = 0x2021,
301 HCI_LE_SET_DATA_LEN_CMD_OPCODE = 0x2022,
302 HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE = 0x2023,
303 HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE = 0x2024,
304 HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE = 0x2025,
305 HCI_LE_GEN_DHKEY_V1_CMD_OPCODE = 0x2026,
306 HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE = 0x2027,
307 HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE = 0x2028,
308 HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE = 0x2029,
309 HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE = 0x202A,
310 HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE = 0x202B,
311 HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE = 0x202C,
312 HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE = 0x202D,
313 HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE = 0x202E,
314 HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE = 0x202F,
315 HCI_LE_RD_PHY_CMD_OPCODE = 0x2030,
316 HCI_LE_SET_DFT_PHY_CMD_OPCODE = 0x2031,
317 HCI_LE_SET_PHY_CMD_OPCODE = 0x2032,
318 HCI_LE_RX_TEST_V2_CMD_OPCODE = 0x2033,
319 HCI_LE_TX_TEST_V2_CMD_OPCODE = 0x2034,
320 HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE = 0x2035,
321 HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE = 0x2036,
322 HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE = 0x2037,
323 HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE = 0x2038,
324 HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE = 0x2039,
325 HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE = 0x203A,
326 HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE = 0x203B,
327 HCI_LE_RMV_ADV_SET_CMD_OPCODE = 0x203C,
328 HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE = 0x203D,
329 HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE = 0x203E,
330 HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE = 0x203F,
331 HCI_LE_SET_PER_ADV_EN_CMD_OPCODE = 0x2040,
332 HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE = 0x2041,
333 HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE = 0x2042,
334 HCI_LE_EXT_CREATE_CON_CMD_OPCODE = 0x2043,
335 HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE = 0x2044,
336 HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE = 0x2045,
337 HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE = 0x2046,
338 HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE = 0x2047,
339 HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE = 0x2048,
340 HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE = 0x2049,
341 HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE = 0x204A,
342 HCI_LE_RD_TX_PWR_CMD_OPCODE = 0x204B,
343 HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE = 0x204C,
344 HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE = 0x204D,
345 HCI_LE_SET_PRIV_MODE_CMD_OPCODE = 0x204E,
346 HCI_LE_RX_TEST_V3_CMD_OPCODE = 0x204F,
347 HCI_LE_TX_TEST_V3_CMD_OPCODE = 0x2050,
348 HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE = 0x2051,
349 HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE = 0x2052,
350 HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE = 0x2053,
351 HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE = 0x2054,
352 HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE = 0x2055,
353 HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE = 0x2056,
354 HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE = 0x2057,
355 HCI_LE_RD_ANTENNA_INF_CMD_OPCODE = 0x2058,
356 HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE = 0x2059,
357 HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE = 0x205A,
358 HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE = 0x205B,
359 HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE = 0x205C,
360 HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE = 0x205D,
361 HCI_LE_GEN_DHKEY_V2_CMD_OPCODE = 0x205E,
362 HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE = 0x205F,
363 HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE = 0x2060,
364 HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE = 0x2061,
365 HCI_LE_SET_CIG_PARAMS_CMD_OPCODE = 0x2062,
366 HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE = 0x2063,
367 HCI_LE_CREATE_CIS_CMD_OPCODE = 0x2064,
368 HCI_LE_REMOVE_CIG_CMD_OPCODE = 0x2065,
369 HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE = 0x2066,
370 HCI_LE_REJECT_CIS_REQ_CMD_OPCODE = 0x2067,
371 HCI_LE_CREATE_BIG_CMD_OPCODE = 0x2068,
372 HCI_LE_CREATE_BIG_TEST_CMD_OPCODE = 0x2069,
373 HCI_LE_TERMINATE_BIG_CMD_OPCODE = 0x206A,
374 HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE = 0x206B,
375 HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE = 0x206C,
376 HCI_LE_REQ_PEER_SCA_CMD_OPCODE = 0x206D,
377 HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE = 0x206E,
378 HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE = 0x206F,
379 HCI_LE_ISO_TX_TEST_CMD_OPCODE = 0x2070,
380 HCI_LE_ISO_RX_TEST_CMD_OPCODE = 0x2071,
381 HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE = 0x2072,
382 HCI_LE_ISO_TEST_END_CMD_OPCODE = 0x2073,
383 HCI_LE_SET_HOST_FEATURE_CMD_OPCODE = 0x2074,
384 HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE = 0x2075,
385 HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE = 0x2076,
386 HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE = 0x2077,
387 HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE = 0x2078,
388 HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE = 0x2079,
389 HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE = 0x207A,
390 HCI_LE_TX_TEST_V4_CMD_OPCODE = 0x207B,
391 HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE = 0x20F9,
392 HCI_LE_START_RANGING_CMD_OPCODE = 0x20FA,
393 HCI_PUBLIC_ADDR_SET_CMD_OPCODE = 0x20FB,
394 HCI_LE_TIME_SYNC_EN_CMD_OPCODE = 0x20FC,
395
396 ///Debug commands - OGF = 0x3F (spec)
397 HCI_DBG_RD_MEM_CMD_OPCODE = 0xFC01,
398 HCI_DBG_WR_MEM_CMD_OPCODE = 0xFC02,
399 HCI_DBG_DEL_PAR_CMD_OPCODE = 0xFC03,
400 HCI_DBG_ID_FLASH_CMD_OPCODE = 0xFC05,
401 HCI_DBG_ER_FLASH_CMD_OPCODE = 0xFC06,
402 HCI_DBG_WR_FLASH_CMD_OPCODE = 0xFC07,
403 HCI_DBG_RD_FLASH_CMD_OPCODE = 0xFC08,
404 HCI_DBG_RD_PAR_CMD_OPCODE = 0xFC09,
405 HCI_DBG_WR_PAR_CMD_OPCODE = 0xFC0A,
406 HCI_DBG_WLAN_COEX_CMD_OPCODE = 0xFC0B,
407 HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE = 0xFC0D,
408 HCI_DBG_BT_SEND_LMP_CMD_OPCODE = 0xFC0E,
409 HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE = 0xFC0F,
410 HCI_DBG_RD_KE_STATS_CMD_OPCODE = 0xFC10,
411 HCI_DBG_PLF_RESET_CMD_OPCODE = 0xFC11,
412 HCI_DBG_RD_MEM_INFO_CMD_OPCODE = 0xFC12,
413 HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE = 0xFC13,
414 HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE = 0xFC14,
415 HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE = 0xFC15,
416
417 HCI_DBG_BLE_REG_RD_CMD_OPCODE = 0xFC30,
418 HCI_DBG_BLE_REG_WR_CMD_OPCODE = 0xFC31,
419 HCI_DBG_SEND_LLCP_CMD_OPCODE = 0xFC35,
420 HCI_DBG_LLCP_DISCARD_CMD_OPCODE = 0xFC36,
421 HCI_DBG_RF_REG_RD_CMD_OPCODE = 0xFC39,
422 HCI_DBG_RF_REG_WR_CMD_OPCODE = 0xFC3A,
423 HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE = 0xFC3C,
424 HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE = 0xFC3D,
425 HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE = 0xFC3E,
426 HCI_DBG_RF_CNTL_TX_CMD_OPCODE = 0xFC3F,
427 };
428
429 enum hci_evt_code
430 {
431 HCI_INQ_CMP_EVT_CODE = 0x01,
432 HCI_INQ_RES_EVT_CODE = 0x02,
433 HCI_CON_CMP_EVT_CODE = 0x03,
434 HCI_CON_REQ_EVT_CODE = 0x04,
435 HCI_DISC_CMP_EVT_CODE = 0x05,
436 HCI_AUTH_CMP_EVT_CODE = 0x06,
437 HCI_REM_NAME_REQ_CMP_EVT_CODE = 0x07,
438 HCI_ENC_CHG_EVT_CODE = 0x08,
439 HCI_CHG_CON_LK_CMP_EVT_CODE = 0x09,
440 HCI_MASTER_LK_CMP_EVT_CODE = 0x0A,
441 HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE = 0x0B,
442 HCI_RD_REM_VER_INFO_CMP_EVT_CODE = 0x0C,
443 HCI_QOS_SETUP_CMP_EVT_CODE = 0x0D,
444 HCI_CMD_CMP_EVT_CODE = 0x0E,
445 HCI_CMD_STATUS_EVT_CODE = 0x0F,
446 HCI_HW_ERR_EVT_CODE = 0x10,
447 HCI_FLUSH_OCCURRED_EVT_CODE = 0x11,
448 HCI_ROLE_CHG_EVT_CODE = 0x12,
449 HCI_NB_CMP_PKTS_EVT_CODE = 0x13,
450 HCI_MODE_CHG_EVT_CODE = 0x14,
451 HCI_RETURN_LINK_KEYS_EVT_CODE = 0x15,
452 HCI_PIN_CODE_REQ_EVT_CODE = 0x16,
453 HCI_LK_REQ_EVT_CODE = 0x17,
454 HCI_LK_NOTIF_EVT_CODE = 0x18,
455 HCI_DATA_BUF_OVFLW_EVT_CODE = 0x1A,
456 HCI_MAX_SLOT_CHG_EVT_CODE = 0x1B,
457 HCI_RD_CLK_OFF_CMP_EVT_CODE = 0x1C,
458 HCI_CON_PKT_TYPE_CHG_EVT_CODE = 0x1D,
459 HCI_QOS_VIOL_EVT_CODE = 0x1E,
460 HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE = 0x20,
461 HCI_FLOW_SPEC_CMP_EVT_CODE = 0x21,
462 HCI_INQ_RES_WITH_RSSI_EVT_CODE = 0x22,
463 HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE = 0x23,
464 HCI_SYNC_CON_CMP_EVT_CODE = 0x2C,
465 HCI_SYNC_CON_CHG_EVT_CODE = 0x2D,
466 HCI_SNIFF_SUB_EVT_CODE = 0x2E,
467 HCI_EXT_INQ_RES_EVT_CODE = 0x2F,
468 HCI_ENC_KEY_REFRESH_CMP_EVT_CODE = 0x30,
469 HCI_IO_CAP_REQ_EVT_CODE = 0x31,
470 HCI_IO_CAP_RSP_EVT_CODE = 0x32,
471 HCI_USER_CFM_REQ_EVT_CODE = 0x33,
472 HCI_USER_PASSKEY_REQ_EVT_CODE = 0x34,
473 HCI_REM_OOB_DATA_REQ_EVT_CODE = 0x35,
474 HCI_SP_CMP_EVT_CODE = 0x36,
475 HCI_LINK_SUPV_TO_CHG_EVT_CODE = 0x38,
476 HCI_ENH_FLUSH_CMP_EVT_CODE = 0x39,
477 HCI_USER_PASSKEY_NOTIF_EVT_CODE = 0x3B,
478 HCI_KEYPRESS_NOTIF_EVT_CODE = 0x3C,
479 HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE = 0x3D,
480 HCI_LE_META_EVT_CODE = 0x3E,
481 HCI_MAX_EVT_MSK_PAGE_1_CODE = 0x40,
482 HCI_SYNC_TRAIN_CMP_EVT_CODE = 0x4F,
483 HCI_SYNC_TRAIN_REC_EVT_CODE = 0x50,
484 HCI_CON_SLV_BCST_REC_EVT_CODE = 0x51,
485 HCI_CON_SLV_BCST_TO_EVT_CODE = 0x52,
486 HCI_TRUNC_PAGE_CMP_EVT_CODE = 0x53,
487 HCI_SLV_PAGE_RSP_TO_EVT_CODE = 0x54,
488 HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE = 0x55,
489 HCI_AUTH_PAYL_TO_EXP_EVT_CODE = 0x57,
490 HCI_SAM_STATUS_CHANGE_EVT_CODE = 0x58,
491 HCI_MAX_EVT_MSK_PAGE_2_CODE = 0x59,
492 HCI_DBG_META_EVT_CODE = 0xFF,
493 };
494
495 enum hci_le_evt_subcode
496 {
497 HCI_LE_CON_CMP_EVT_SUBCODE = 0x01,
498 HCI_LE_ADV_REPORT_EVT_SUBCODE = 0x02,
499 HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE = 0x03,
500 HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE = 0x04,
501 HCI_LE_LTK_REQUEST_EVT_SUBCODE = 0x05,
502 HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE = 0x06,
503 HCI_LE_DATA_LEN_CHG_EVT_SUBCODE = 0x07,
504 HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE = 0x08,
505 HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE = 0x09,
506 HCI_LE_ENH_CON_CMP_EVT_SUBCODE = 0x0A,
507 HCI_LE_DIR_ADV_REP_EVT_SUBCODE = 0x0B,
508 HCI_LE_PHY_UPD_CMP_EVT_SUBCODE = 0x0C,
509 HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE = 0x0D,
510 HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE = 0x0E,
511 HCI_LE_PER_ADV_REPORT_EVT_SUBCODE = 0x0F,
512 HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE = 0x10,
513 HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE = 0x11,
514 HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE = 0x12,
515 HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE = 0x13,
516 HCI_LE_CH_SEL_ALGO_EVT_SUBCODE = 0x14,
517 HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE = 0x15,
518 HCI_LE_CON_IQ_REPORT_EVT_SUBCODE = 0x16,
519 HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE = 0x17,
520 HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE = 0x18,
521 HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE = 0x19,
522 HCI_LE_CIS_REQUEST_EVT_SUBCODE = 0x1A,
523 HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE = 0x1B,
524 HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE = 0x1C,
525 HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE = 0x1D,
526 HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE = 0x1E,
527 HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE = 0x1F,
528 HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE = 0x20,
529 HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE = 0x21,
530 HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE = 0x22,
531
532 HCI_LE_RANGING_IND_EVT_SUBCODE = 0x31,
533 HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE = 0x32,
534 HCI_LE_RANGING_CMP_EVT_SUBCODE = 0x33,
535 };
536
537 /****** RANGING CODE START ******/
538 enum hci_vs_opcode
539 {
540 // DK command
541 HCI_VS_LE_SET_DK_DEVICE_INFO_CMD_OPCODE = 0xFC70,
542
543 HCI_VS_LE_GET_LINK_INFO_CMD_OPCODE = 0xFC73,
544 HCI_VS_LE_CREATE_SNIFFER_CMD_OPCODE = 0xFC74,
545 HCI_VS_LE_DISCONNECT_SNIFFER_CMD_OPCODE = 0xFC75,
546 HCI_VS_LE_UPDATE_SNIFFER_CON_PARAM_CMD_OPCODE = 0xFC76,
547 HCI_VS_LE_UPDATE_SNIFFER_CH_MAP_PARAM_CMD_OPCODE = 0xFC77,
548 HCI_VS_LE_UPDATE_SNIFFER_PHY_PARAM_CMD_OPCODE = 0xFC78,
549
550 HCI_VS_LE_RSSI_ENABLE_RANGING_CMD_OPCODE = 0xFC79,
551 HCI_VS_LE_RSSI_UPDATE_RANGING_TYPE_CMD_OPCODE = 0xFC7A,
552 HCI_VS_LE_EVENT_NOTIFICATION_EN_CMD_OPCODE = 0xFC7D, // KEEP the same as GR5410
553 };
554
555 enum hci_vs_dbg_evt_subcode
556 {
557 HCI_VS_LE_GET_LINK_INFO_CMP_EVT_SUBCODE = 0x10,
558 HCI_VS_LE_SNIFFER_DISC_CMP_EVT_SUBCODE = 0x11,
559 HCI_VS_LE_REQ_BLE_CLOCK_SYNC_EVT_SUBCODE = 0x12,
560 HCI_VS_LE_CON_PARAM_NOTIF_EVT_SUBCODE = 0x13,
561 HCI_VS_LE_CH_MAP_PARAM_NOTIF_EVT_SUBCODE = 0x14,
562 HCI_VS_LE_PHY_PARAM_NOTIF_EVT_SUBCODE = 0x15,
563 HCI_VS_LE_RSSI_REPORT_INFO_EVT_SUBCODE = 0x16,
564 HCI_VS_LE_RSSI_RANGING_TYPE_NOTIF_EVT_SUBCODE = 0x17,
565 HCI_VS_LE_EVENT_NOTIFICATION_REPORT_INFO_EVT_SUBCODE = 0x18,
566 };
567 /****** RANGING CODE END ******/
568
569 enum TASK_API_ID
570 {
571 // -----------------------------------------------------------------------------------
572 // ---------------------- Controller Task identifer ----------------------------------
573 // -----------------------------------------------------------------------------------
574 // Link Layer Tasks
575 TASK_ID_LLM = 0, // BLE Link manager
576 TASK_ID_LLC = 1, // BLE Link controller
577 TASK_ID_LLD = 2, // BLE Link driver
578 TASK_ID_LLI = 3, // BLE Link ISO
579
580 TASK_ID_DBG = 4, // Debug task
581
582 // BT Controller Tasks
583 TASK_ID_LM = 5, // BT Link manager
584 TASK_ID_LC = 6, // BT Link controller
585 TASK_ID_LB = 7, // BT Broadcast
586 TASK_ID_LD = 8, // BT Link driver
587
588 // -----------------------------------------------------------------------------------
589 // --------------------- BLE HL TASK API Identifiers ---------------------------------
590 // --------------------- SHALL NOT BE CHANGED ---------------------------------
591 // -----------------------------------------------------------------------------------
592 TASK_ID_SDK = 9, //SDK Task
593
594 TASK_ID_L2CC = 10, // L2CAP Controller Task
595 TASK_ID_GATTM = 11, // Generic Attribute Profile Manager Task
596 TASK_ID_GATTC = 12, // Generic Attribute Profile Controller Task
597 TASK_ID_GAPM = 13, // Generic Access Profile Manager
598 TASK_ID_GAPC = 14, // Generic Access Profile Controller
599 TASK_ID_APP = 15, // Application API
600 TASK_ID_AHI = 16, // Application Host Interface
601 TASK_ID_HCI = 17, // Host to Control Interface
602 TASK_ID_DISPLAY = 19, // LCD/Display task
603 TASK_ID_MESH = 200, // Mesh Task
604 TASK_ID_RTLS = 250, // RTLS Task
605
606 TASK_ID_INVALID = 0xFF, // Invalid Task Identifier
607 };
608
609 /// HCI task Message ID
610 /*@TRACE*/
611 enum hci_msg_id
612 {
613 HCI_MSG_ID_FIRST = TASK_FIRST_MSG(TASK_ID_HCI),
614
615 HCI_CMD_CMP_EVENT,
616 HCI_CMD_STAT_EVENT,
617 HCI_EVENT,
618 HCI_LE_EVENT,
619 HCI_COMMAND,
620 HCI_ACL_DATA,
621 HCI_VS_EVENT,
622 HCI_MSG_ID_LAST
623 };
624
625 /**
626 * @brief SDK_TASK Message ID.
627 */
628 enum sdk_msg_id
629 {
630 /// Timeout indication to sdk
631 SDK_COMMON_TIMEOUT_TIMER_0 = TASK_FIRST_MSG(TASK_ID_SDK),
632 SDK_COMMON_TIMEOUT_TIMER_1,
633 SDK_COMMON_TIMEOUT_TIMER_2,
634 SDK_COMMON_TIMEOUT_TIMER_3,
635 SDK_COMMON_TIMEOUT_TIMER_4,
636 SDK_COMMON_TIMEOUT_TIMER_5,
637 SDK_COMMON_TIMEOUT_TIMER_6,
638 SDK_COMMON_TIMEOUT_TIMER_7,
639 SDK_COMMON_TIMEOUT_TIMER_8,
640 SDK_COMMON_TIMEOUT_TIMER_9, // Message number for SDK_COMMON_TIMEOUT_TIMER shall be equal to SDK_TIMER_MAX_NUM.
641
642 /****** RANGING CODE START ******/
643 SDK_RANGING_INTER_NODE_COMM_RX_DATA, // Localization ranging: inter-node comm has received data.
644 SDK_RANGING_INTER_NODE_COMM_TX_DATA_CMP, // Localization ranging: inter-node comm has completed to transmit data.
645 SDK_RANGING_INTER_NODE_COMM_ABORT_TX_CMP, // Localization ranging: inter-node comm has completed to abort all data transmission.
646 SDK_RANGING_INTER_NODE_COMM_ERR_OCCUR, // Localization ranging: inter-node comm has error occurred.
647
648 SDK_RANGING_SLEEP_RANGING, // Localization ranging: sleep ranging.
649 SDK_RANGING_WAKEUP_RANGING, // Localization ranging: wakeup ranging.
650 SDK_RANGING_START_RANGING, // Localization ranging: start ranging.
651 SDK_RANGING_STOP_RANGING, // Localization ranging: stop ranging.
652 SDK_RANGING_ANCHOR_START_RANGING, // Localization ranging: anchor start ranging.
653 SDK_RANGING_ANCHOR_STOP_RANGING, // Localization ranging: anchor stop ranging.
654 SDK_RANGING_UPDATE_CI, // Localization ranging: update connection interval.
655 SDK_RANGING_TIMEOUT_DISPATCH, // Localization ranging: dispatch timer timeout.
656
657 SDK_APP_SET_SCAN_ADDR, // User sets target address to scan.
658 /****** RANGING CODE END ******/
659 };
660
661 /**
662 * @brief GAPC_TASK Message ID.
663 */
664 enum gapc_msg_id
665 {
666 GAPC_CMP_EVT = MSG_ID(GAPC, 0x00),
667 GAPC_CONNECTION_REQ_IND = MSG_ID(GAPC, 0x01),
668 GAPC_CONNECTION_CFM = MSG_ID(GAPC, 0x02),
669 GAPC_DISCONNECT_IND = MSG_ID(GAPC, 0x03),
670 GAPC_DISCONNECT_CMD = MSG_ID(GAPC, 0x04),
671 GAPC_GET_INFO_CMD = MSG_ID(GAPC, 0x05),
672 GAPC_PEER_ATT_INFO_IND = MSG_ID(GAPC, 0x06),
673 GAPC_PEER_VERSION_IND = MSG_ID(GAPC, 0x07),
674 GAPC_PEER_FEATURES_IND = MSG_ID(GAPC, 0x08),
675 GAPC_CON_RSSI_IND = MSG_ID(GAPC, 0x09),
676 GAPC_GET_DEV_INFO_REQ_IND = MSG_ID(GAPC, 0x0A),
677 GAPC_GET_DEV_INFO_CFM = MSG_ID(GAPC, 0x0B),
678 GAPC_SET_DEV_INFO_REQ_IND = MSG_ID(GAPC, 0x0C),
679 GAPC_SET_DEV_INFO_CFM = MSG_ID(GAPC, 0x0D),
680 GAPC_PARAM_UPDATE_CMD = MSG_ID(GAPC, 0x0E),
681 GAPC_PARAM_UPDATE_REQ_IND = MSG_ID(GAPC, 0x0F),
682 GAPC_PARAM_UPDATE_CFM = MSG_ID(GAPC, 0x10),
683 GAPC_PARAM_UPDATED_IND = MSG_ID(GAPC, 0x11),
684 GAPC_BOND_CMD = MSG_ID(GAPC, 0x12),
685 GAPC_BOND_REQ_IND = MSG_ID(GAPC, 0x13),
686 GAPC_BOND_CFM = MSG_ID(GAPC, 0x14),
687 GAPC_BOND_IND = MSG_ID(GAPC, 0x15),
688 GAPC_ENCRYPT_CMD = MSG_ID(GAPC, 0x16),
689 GAPC_ENCRYPT_REQ_IND = MSG_ID(GAPC, 0x17),
690 GAPC_ENCRYPT_CFM = MSG_ID(GAPC, 0x18),
691 GAPC_ENCRYPT_IND = MSG_ID(GAPC, 0x19),
692 GAPC_SECURITY_CMD = MSG_ID(GAPC, 0x1A),
693 GAPC_SECURITY_IND = MSG_ID(GAPC, 0x1B),
694 GAPC_SIGN_COUNTER_IND = MSG_ID(GAPC, 0x1C),
695 GAPC_CON_CHANNEL_MAP_IND = MSG_ID(GAPC, 0x1D),
696 GAPC_SEC_REQ_TIMEOUT_IND = MSG_ID(GAPC, 0x1E),
697 GAPC_SET_LE_PING_TO_CMD = MSG_ID(GAPC, 0x28),
698 GAPC_LE_PING_TO_VAL_IND = MSG_ID(GAPC, 0x29),
699 GAPC_LE_PING_TO_IND = MSG_ID(GAPC, 0x2A),
700 GAPC_SET_LE_PKT_SIZE_CMD = MSG_ID(GAPC, 0x2B),
701 GAPC_LE_PKT_SIZE_IND = MSG_ID(GAPC, 0x2C),
702 GAPC_KEY_PRESS_NOTIFICATION_CMD = MSG_ID(GAPC, 0x2D),
703 GAPC_KEY_PRESS_NOTIFICATION_IND = MSG_ID(GAPC, 0x2E),
704 GAPC_SET_PHY_CMD = MSG_ID(GAPC, 0x2F),
705 GAPC_LE_PHY_IND = MSG_ID(GAPC, 0x30),
706 GAPC_CHAN_SEL_ALGO_IND = MSG_ID(GAPC, 0x31),
707 GAPC_SET_PREF_SLAVE_LATENCY_CMD = MSG_ID(GAPC, 0x32),
708 GAPC_SET_PREF_SLAVE_EVT_DUR_CMD = MSG_ID(GAPC, 0x33),
709 GAPC_UNKNOWN_MSG_IND = MSG_ID(GAPC, 0x34),
710 GAPC_PER_ADV_SYNC_TRANS_CMD = MSG_ID(GAPC, 0x35),
711 GAPC_CTE_TX_CFG_CMD = MSG_ID(GAPC, 0x38),
712 GAPC_CTE_RX_CFG_CMD = MSG_ID(GAPC, 0x39),
713 GAPC_CTE_REQ_CTRL_CMD = MSG_ID(GAPC, 0x3A),
714 GAPC_CTE_RSP_CTRL_CMD = MSG_ID(GAPC, 0x3B),
715 GAPC_CTE_IQ_REPORT_IND = MSG_ID(GAPC, 0x3C),
716 GAPC_READ_LOCAL_TX_PWR_CMD = MSG_ID(GAPC, 0x3D),
717 GAPC_READ_REMOTE_TX_PWR_CMD = MSG_ID(GAPC, 0x3E),
718 GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD = MSG_ID(GAPC, 0x3F),
719 GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD = MSG_ID(GAPC, 0x40),
720 GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD = MSG_ID(GAPC, 0x41),
721 GAPC_READ_LOCAL_TX_PWR_IND = MSG_ID(GAPC, 0x42),
722 GAPC_READ_REMOTE_TX_PWR_IND = MSG_ID(GAPC, 0x43),
723 GAPC_TX_PWR_CHANGE_REPORT_IND = MSG_ID(GAPC, 0x44),
724 GAPC_PATH_LOSS_THRESHOLD_REPORT_IND = MSG_ID(GAPC, 0x45),
725 GAPC_RANGING_START_CMD = MSG_ID(GAPC, 0x46),
726 GAPC_RANGING_IND = MSG_ID(GAPC, 0x47),
727 GAPC_RANGING_SAMPLE_REPORT_IND = MSG_ID(GAPC, 0x48),
728 GAPC_RANGING_CMP_IND = MSG_ID(GAPC, 0x49),
729 GAPC_SIGN_CMD = MSG_ID(GAPC, 0xF0),
730 GAPC_SIGN_IND = MSG_ID(GAPC, 0xF1),
731 GAPC_PARAM_UPDATE_TO_IND = MSG_ID(GAPC, 0xF2),
732 GAPC_SMP_TIMEOUT_TIMER_IND = MSG_ID(GAPC, 0xF3),
733 GAPC_SMP_REP_ATTEMPTS_TIMER_IND = MSG_ID(GAPC, 0xF4),
734 };
735
736 /**
737 * @brief GAPM_TASK Message ID.
738 */
739 enum gapm_msg_id
740 {
741 GAPM_CMP_EVT = MSG_ID(GAPM, 0x00),
742 GAPM_RESET_CMD = MSG_ID(GAPM, 0x02),
743 GAPM_SET_DEV_CONFIG_CMD = MSG_ID(GAPM, 0x04),
744 GAPM_SET_CHANNEL_MAP_CMD = MSG_ID(GAPM, 0x05),
745 GAPM_GET_DEV_INFO_CMD = MSG_ID(GAPM, 0x06),
746 GAPM_DEV_VERSION_IND = MSG_ID(GAPM, 0x07),
747 GAPM_DEV_BDADDR_IND = MSG_ID(GAPM, 0x08),
748 GAPM_DEV_ADV_TX_POWER_IND = MSG_ID(GAPM, 0x09),
749 GAPM_DBG_MEM_INFO_IND = MSG_ID(GAPM, 0x0A),
750 GAPM_ANTENNA_INF_IND = MSG_ID(GAPM, 0x0B),
751 GAPM_RESOLV_ADDR_CMD = MSG_ID(GAPM, 0x14),
752 GAPM_ADDR_SOLVED_IND = MSG_ID(GAPM, 0x15),
753 GAPM_GEN_RAND_ADDR_CMD = MSG_ID(GAPM, 0x16),
754 GAPM_USE_ENC_BLOCK_CMD = MSG_ID(GAPM, 0x17),
755 GAPM_USE_ENC_BLOCK_IND = MSG_ID(GAPM, 0x18),
756 GAPM_GEN_RAND_NB_CMD = MSG_ID(GAPM, 0x19),
757 GAPM_GEN_RAND_NB_IND = MSG_ID(GAPM, 0x1A),
758 GAPM_PROFILE_TASK_ADD_CMD = MSG_ID(GAPM, 0x1B),
759 GAPM_PROFILE_ADDED_IND = MSG_ID(GAPM, 0x1C),
760 GAPM_UNKNOWN_TASK_IND = MSG_ID(GAPM, 0x1D),
761 GAPM_SUGG_DFLT_DATA_LEN_IND = MSG_ID(GAPM, 0x1E),
762 GAPM_MAX_DATA_LEN_IND = MSG_ID(GAPM, 0x1F),
763 GAPM_RAL_ADDR_IND = MSG_ID(GAPM, 0x22),
764 GAPM_SET_IRK_CMD = MSG_ID(GAPM, 0x23),
765 GAPM_LEPSM_REGISTER_CMD = MSG_ID(GAPM, 0x24),
766 GAPM_LEPSM_UNREGISTER_CMD = MSG_ID(GAPM, 0x25),
767 GAPM_LE_TEST_MODE_CTRL_CMD = MSG_ID(GAPM, 0x26),
768 GAPM_LE_TEST_END_IND = MSG_ID(GAPM, 0x27),
769 GAPM_LE_TEST_IQ_REPORT_IND = MSG_ID(GAPM, 0x2D),
770 GAPM_ISO_STAT_IND = MSG_ID(GAPM, 0x28),
771 GAPM_GEN_DH_KEY_CMD = MSG_ID(GAPM, 0x29),
772 GAPM_GEN_DH_KEY_IND = MSG_ID(GAPM, 0x2A),
773 GAPM_GET_PUB_KEY_CMD = MSG_ID(GAPM, 0x2B),
774 GAPM_PUB_KEY_IND = MSG_ID(GAPM, 0x2C),
775 GAPM_GET_RAL_ADDR_CMD = MSG_ID(GAPM, 0x90),
776 GAPM_LIST_SET_CMD = MSG_ID(GAPM, 0x91),
777 GAPM_LIST_SIZE_IND = MSG_ID(GAPM, 0x92),
778 GAPM_ACTIVITY_CREATE_CMD = MSG_ID(GAPM, 0xA0),
779 GAPM_ACTIVITY_START_CMD = MSG_ID(GAPM, 0xA1),
780 GAPM_ACTIVITY_STOP_CMD = MSG_ID(GAPM, 0xA2),
781 GAPM_ACTIVITY_DELETE_CMD = MSG_ID(GAPM, 0xA3),
782 GAPM_ACTIVITY_CREATED_IND = MSG_ID(GAPM, 0xA4),
783 GAPM_ACTIVITY_STOPPED_IND = MSG_ID(GAPM, 0xA5),
784 GAPM_SET_ADV_DATA_CMD = MSG_ID(GAPM, 0xA6),
785 GAPM_EXT_ADV_REPORT_IND = MSG_ID(GAPM, 0xA7),
786 GAPM_SCAN_REQUEST_IND = MSG_ID(GAPM, 0xA8),
787 GAPM_SYNC_ESTABLISHED_IND = MSG_ID(GAPM, 0xA9),
788 GAPM_MAX_ADV_DATA_LEN_IND = MSG_ID(GAPM, 0xAA),
789 GAPM_NB_ADV_SETS_IND = MSG_ID(GAPM, 0xAB),
790 GAPM_DEV_TX_PWR_IND = MSG_ID(GAPM, 0xAC),
791 GAPM_DEV_RF_PATH_COMP_IND = MSG_ID(GAPM, 0xAD),
792 GAPM_UNKNOWN_MSG_IND = MSG_ID(GAPM, 0xAE),
793 GAPM_PER_ADV_REPORT_CTRL_CMD = MSG_ID(GAPM, 0xAF),
794 GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD = MSG_ID(GAPM, 0xB0),
795 GAPM_PER_ADV_IQ_REPORT_IND = MSG_ID(GAPM, 0xB1),
796 GAPM_PER_ADV_CTE_TX_CTL_CMD = MSG_ID(GAPM, 0xB2),
797 GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD = MSG_ID(GAPM, 0xB3),
798 GAPM_DBG_IQGEN_CFG_CMD = MSG_ID(GAPM, 0x50),
799 GAPM_UNKNOWN_TASK_MSG = MSG_ID(GAPM, 0xF0),
800 GAPM_ADDR_RENEW_TO_IND = MSG_ID(GAPM, 0xF1),
801 GAPM_AUTO_CONN_TO_IND = MSG_ID(GAPM, 0xF2),
802 GAPM_ADDR_RENEW_CMD = MSG_ID(GAPM, 0xF3),
803 GAPM_PUBLIC_ADDR_SET_CMD = MSG_ID(GAPM, 0xF4),
804 GAPM_SET_GDX_RANGING_PARAM_CMD = MSG_ID(GAPM, 0xF5),
805 GAPM_ADV_SCAN_MONITOR_EVT_REPORT_IND = MSG_ID(GAPM, 0xF6),
806 };
807
808 /**
809 * @brief GATTC_TASK Message ID.
810 */
811 enum gattc_msg_id
812 {
813 GATTC_CMP_EVT = TASK_FIRST_MSG(TASK_ID_GATTC),
814 GATTC_EXC_MTU_CMD,
815 GATTC_MTU_CHANGED_IND,
816 GATTC_DISC_CMD,
817 GATTC_DISC_SVC_IND,
818 GATTC_DISC_SVC_INCL_IND,
819 GATTC_DISC_CHAR_IND,
820 GATTC_DISC_CHAR_DESC_IND,
821 GATTC_READ_CMD,
822 GATTC_READ_IND,
823 GATTC_WRITE_CMD,
824 GATTC_EXECUTE_WRITE_CMD,
825 GATTC_EVENT_IND,
826 GATTC_EVENT_REQ_IND,
827 GATTC_EVENT_CFM,
828 GATTC_REG_TO_PEER_EVT_CMD,
829 GATTC_SEND_EVT_CMD,
830 GATTC_SEND_SVC_CHANGED_CMD,
831 GATTC_SVC_CHANGED_CFG_IND,
832 GATTC_READ_REQ_IND,
833 GATTC_READ_CFM,
834 GATTC_WRITE_REQ_IND,
835 GATTC_WRITE_CFM,
836 GATTC_ATT_INFO_REQ_IND,
837 GATTC_ATT_INFO_CFM,
838 GATTC_SDP_SVC_DISC_CMD,
839 GATTC_SDP_SVC_IND,
840 GATTC_TRANSACTION_TO_ERROR_IND,
841 GATTC_UNKNOWN_MSG_IND,
842 GATTC_CLIENT_RTX_IND,
843 GATTC_SERVER_RTX_IND,
844 };
845
846 /**
847 * @brief GATTC_TASK Message ID.
848 */
849 enum l2cc_msg_id
850 {
851 L2CC_CMP_EVT = TASK_FIRST_MSG(TASK_ID_L2CC) + L2CC_NB_DEPRECATED_MSG,
852 L2CC_LECB_CONNECT_CMD,
853 L2CC_LECB_CONNECT_REQ_IND,
854 L2CC_LECB_CONNECT_CFM,
855 L2CC_LECB_CONNECT_IND,
856 L2CC_LECB_DISCONNECT_CMD,
857 L2CC_LECB_DISCONNECT_IND,
858 L2CC_LECB_ADD_CMD,
859 L2CC_LECB_ADD_IND,
860 L2CC_LECB_SDU_SEND_CMD,
861 L2CC_LECB_SDU_RECV_IND,
862 L2CC_UNKNOWN_MSG_IND,
863 L2CC_DBG_PDU_SEND_CMD,
864 L2CC_DBG_PDU_RECV_IND,
865 L2CC_PDU_SEND_CMD,
866 L2CC_PDU_RECV_IND,
867 L2CC_SIGNALING_TRANS_TO_IND,
868 };
869
870 /** @} */
871 #endif // __BLE_ID_H__
872 /** @} */
873 /** @} */
874
HCI_IO_CAP_REQ_REPLY_CMD_OPCODE
@ HCI_IO_CAP_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:107
GAPM_ANTENNA_INF_IND
@ GAPM_ANTENNA_INF_IND
Definition: ble_id.h:750
GATTC_READ_CMD
@ GATTC_READ_CMD
Definition: ble_id.h:821
HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE
@ HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE
Definition: ble_id.h:519
HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE
@ HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE
Definition: ble_id.h:353
HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE
@ HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:386
GAPC_SMP_TIMEOUT_TIMER_IND
@ GAPC_SMP_TIMEOUT_TIMER_IND
Definition: ble_id.h:732
HCI_SETUP_SYNC_CON_CMD_OPCODE
@ HCI_SETUP_SYNC_CON_CMD_OPCODE
Definition: ble_id.h:104
GAPM_GET_PUB_KEY_CMD
@ GAPM_GET_PUB_KEY_CMD
Definition: ble_id.h:773
SDK_RANGING_INTER_NODE_COMM_ABORT_TX_CMP
@ SDK_RANGING_INTER_NODE_COMM_ABORT_TX_CMP
Definition: ble_id.h:645
GAPM_PER_ADV_IQ_REPORT_IND
@ GAPM_PER_ADV_IQ_REPORT_IND
Definition: ble_id.h:795
HCI_LE_SET_ADV_EN_CMD_OPCODE
@ HCI_LE_SET_ADV_EN_CMD_OPCODE
Definition: ble_id.h:277
HCI_REM_NAME_REQ_CMD_OPCODE
@ HCI_REM_NAME_REQ_CMD_OPCODE
Definition: ble_id.h:97
HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE
@ HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE
Definition: ble_id.h:423
HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE
Definition: ble_id.h:330
TASK_ID_INVALID
@ TASK_ID_INVALID
Definition: ble_id.h:606
HCI_LE_START_RANGING_CMD_OPCODE
@ HCI_LE_START_RANGING_CMD_OPCODE
Definition: ble_id.h:392
HCI_DBG_DEL_PAR_CMD_OPCODE
@ HCI_DBG_DEL_PAR_CMD_OPCODE
Definition: ble_id.h:399
HCI_LE_RD_ANTENNA_INF_CMD_OPCODE
@ HCI_LE_RD_ANTENNA_INF_CMD_OPCODE
Definition: ble_id.h:355
HCI_CHG_CON_PKT_TYPE_CMD_OPCODE
@ HCI_CHG_CON_PKT_TYPE_CMD_OPCODE
Definition: ble_id.h:92
GATTC_UNKNOWN_MSG_IND
@ GATTC_UNKNOWN_MSG_IND
Definition: ble_id.h:841
HCI_CHG_CON_LK_CMP_EVT_CODE
@ HCI_CHG_CON_LK_CMP_EVT_CODE
Definition: ble_id.h:439
HCI_LE_CLEAR_WLST_CMD_OPCODE
@ HCI_LE_CLEAR_WLST_CMD_OPCODE
Definition: ble_id.h:283
GATTC_WRITE_CMD
@ GATTC_WRITE_CMD
Definition: ble_id.h:823
HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE
@ HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE
Definition: ble_id.h:313
HCI_CMD_STAT_EVENT
@ HCI_CMD_STAT_EVENT
Definition: ble_id.h:616
HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE
@ HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE
Definition: ble_id.h:354
HCI_RD_PAGE_TO_CMD_OPCODE
@ HCI_RD_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:156
HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE
@ HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE
Definition: ble_id.h:115
HCI_LE_TEST_END_CMD_OPCODE
@ HCI_LE_TEST_END_CMD_OPCODE
Definition: ble_id.h:298
HCI_LE_RX_TEST_V2_CMD_OPCODE
@ HCI_LE_RX_TEST_V2_CMD_OPCODE
Definition: ble_id.h:318
TASK_ID_LC
@ TASK_ID_LC
Definition: ble_id.h:584
HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE
@ HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE
Definition: ble_id.h:217
HCI_LE_CREATE_BIG_CMD_OPCODE
@ HCI_LE_CREATE_BIG_CMD_OPCODE
Definition: ble_id.h:371
HCI_INQ_CANCEL_CMD_OPCODE
@ HCI_INQ_CANCEL_CMD_OPCODE
Definition: ble_id.h:80
HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE
@ HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE
Definition: ble_id.h:388
GAPC_PEER_VERSION_IND
@ GAPC_PEER_VERSION_IND
Definition: ble_id.h:673
L2CC_NB_DEPRECATED_MSG
#define L2CC_NB_DEPRECATED_MSG
Number of L2CC TASK Deprecated messages.
Definition: ble_id.h:67
GAPC_SECURITY_CMD
@ GAPC_SECURITY_CMD
Definition: ble_id.h:692
HCI_RD_AUTH_EN_CMD_OPCODE
@ HCI_RD_AUTH_EN_CMD_OPCODE
Definition: ble_id.h:164
HCI_LE_SET_CIG_PARAMS_CMD_OPCODE
@ HCI_LE_SET_CIG_PARAMS_CMD_OPCODE
Definition: ble_id.h:365
HCI_RD_LOCAL_SP_OPT_CMD_OPCODE
@ HCI_RD_LOCAL_SP_OPT_CMD_OPCODE
Definition: ble_id.h:246
HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE
@ HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE
Definition: ble_id.h:219
HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:300
GATTC_READ_IND
@ GATTC_READ_IND
Definition: ble_id.h:822
HCI_VS_LE_CREATE_SNIFFER_CMD_OPCODE
@ HCI_VS_LE_CREATE_SNIFFER_CMD_OPCODE
Definition: ble_id.h:544
GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD
@ GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD
Definition: ble_id.h:719
HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE
@ HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:299
GAPC_PARAM_UPDATE_TO_IND
@ GAPC_PARAM_UPDATE_TO_IND
Definition: ble_id.h:731
HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE
@ HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE
Definition: ble_id.h:287
HCI_IO_CAP_REQ_EVT_CODE
@ HCI_IO_CAP_REQ_EVT_CODE
Definition: ble_id.h:469
HCI_LE_EVENT
@ HCI_LE_EVENT
Definition: ble_id.h:618
HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE
@ HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE
Definition: ble_id.h:205
SDK_COMMON_TIMEOUT_TIMER_3
@ SDK_COMMON_TIMEOUT_TIMER_3
Definition: ble_id.h:634
HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE
@ HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE
Definition: ble_id.h:324
HCI_LE_META_EVT_CODE
@ HCI_LE_META_EVT_CODE
Definition: ble_id.h:480
HCI_MASTER_LK_CMD_OPCODE
@ HCI_MASTER_LK_CMD_OPCODE
Definition: ble_id.h:96
HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE
@ HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE
Definition: ble_id.h:309
HCI_LE_SET_SCAN_EN_CMD_OPCODE
@ HCI_LE_SET_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:279
HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE
@ HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE
Definition: ble_id.h:351
HCI_LE_SET_RAND_ADDR_CMD_OPCODE
@ HCI_LE_SET_RAND_ADDR_CMD_OPCODE
Definition: ble_id.h:272
HCI_RD_REM_VER_INFO_CMD_OPCODE
@ HCI_RD_REM_VER_INFO_CMD_OPCODE
Definition: ble_id.h:101
HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE
@ HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE
Definition: ble_id.h:527
HCI_DBG_BLE_REG_WR_CMD_OPCODE
@ HCI_DBG_BLE_REG_WR_CMD_OPCODE
Definition: ble_id.h:418
HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE
@ HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE
Definition: ble_id.h:344
HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE
@ HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE
Definition: ble_id.h:210
HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE
@ HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:193
GAPC_SET_LE_PKT_SIZE_CMD
@ GAPC_SET_LE_PKT_SIZE_CMD
Definition: ble_id.h:700
GAPM_GET_RAL_ADDR_CMD
@ GAPM_GET_RAL_ADDR_CMD
Definition: ble_id.h:775
L2CC_SIGNALING_TRANS_TO_IND
@ L2CC_SIGNALING_TRANS_TO_IND
Definition: ble_id.h:867
GAPM_LE_TEST_MODE_CTRL_CMD
@ GAPM_LE_TEST_MODE_CTRL_CMD
Definition: ble_id.h:767
hci_opcode
hci_opcode
Definition: ble_id.h:75
HCI_SAM_STATUS_CHANGE_EVT_CODE
@ HCI_SAM_STATUS_CHANGE_EVT_CODE
Definition: ble_id.h:490
HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE
@ HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE
Definition: ble_id.h:308
HCI_DBG_PLF_RESET_CMD_OPCODE
@ HCI_DBG_PLF_RESET_CMD_OPCODE
Definition: ble_id.h:411
GAPC_SET_DEV_INFO_REQ_IND
@ GAPC_SET_DEV_INFO_REQ_IND
Definition: ble_id.h:678
HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE
@ HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE
Definition: ble_id.h:310
HCI_RD_LE_HOST_SUPP_CMD_OPCODE
@ HCI_RD_LE_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:212
GAPM_LIST_SIZE_IND
@ GAPM_LIST_SIZE_IND
Definition: ble_id.h:777
GAPM_ACTIVITY_CREATED_IND
@ GAPM_ACTIVITY_CREATED_IND
Definition: ble_id.h:782
GATTC_EXECUTE_WRITE_CMD
@ GATTC_EXECUTE_WRITE_CMD
Definition: ble_id.h:824
HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE
@ HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE
Definition: ble_id.h:259
HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:111
GAPM_SET_DEV_CONFIG_CMD
@ GAPM_SET_DEV_CONFIG_CMD
Definition: ble_id.h:743
HCI_ACL_DATA
@ HCI_ACL_DATA
Definition: ble_id.h:620
GAPC_RANGING_SAMPLE_REPORT_IND
@ GAPC_RANGING_SAMPLE_REPORT_IND
Definition: ble_id.h:727
HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE
@ HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE
Definition: ble_id.h:499
HCI_DBG_SEND_LLCP_CMD_OPCODE
@ HCI_DBG_SEND_LLCP_CMD_OPCODE
Definition: ble_id.h:419
HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE
@ HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE
Definition: ble_id.h:241
GAPM_USE_ENC_BLOCK_CMD
@ GAPM_USE_ENC_BLOCK_CMD
Definition: ble_id.h:754
HCI_WR_SCAN_EN_CMD_OPCODE
@ HCI_WR_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:159
HCI_MASTER_LK_CMP_EVT_CODE
@ HCI_MASTER_LK_CMP_EVT_CODE
Definition: ble_id.h:440
HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE
@ HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:203
HCI_WR_STORED_LK_CMD_OPCODE
@ HCI_WR_STORED_LK_CMD_OPCODE
Definition: ble_id.h:150
HCI_LE_LTK_REQUEST_EVT_SUBCODE
@ HCI_LE_LTK_REQUEST_EVT_SUBCODE
Definition: ble_id.h:501
HCI_WR_EXT_INQ_LEN_CMD_OPCODE
@ HCI_WR_EXT_INQ_LEN_CMD_OPCODE
Definition: ble_id.h:233
HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE
@ HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE
Definition: ble_id.h:170
HCI_EXIT_PARK_STATE_CMD_OPCODE
@ HCI_EXIT_PARK_STATE_CMD_OPCODE
Definition: ble_id.h:130
HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE
@ HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE
Definition: ble_id.h:106
GAPM_ISO_STAT_IND
@ GAPM_ISO_STAT_IND
Definition: ble_id.h:770
HCI_VS_LE_UPDATE_SNIFFER_CON_PARAM_CMD_OPCODE
@ HCI_VS_LE_UPDATE_SNIFFER_CON_PARAM_CMD_OPCODE
Definition: ble_id.h:546
SDK_COMMON_TIMEOUT_TIMER_7
@ SDK_COMMON_TIMEOUT_TIMER_7
Definition: ble_id.h:638
SDK_RANGING_UPDATE_CI
@ SDK_RANGING_UPDATE_CI
Definition: ble_id.h:654
HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE
@ HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:189
HCI_WR_AUTH_EN_CMD_OPCODE
@ HCI_WR_AUTH_EN_CMD_OPCODE
Definition: ble_id.h:165
HCI_DBG_RD_MEM_CMD_OPCODE
@ HCI_DBG_RD_MEM_CMD_OPCODE
Debug commands - OGF = 0x3F (spec)
Definition: ble_id.h:397
HCI_LE_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:498
HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE
@ HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE
Definition: ble_id.h:348
HCI_WR_LOOPBACK_MODE_CMD_OPCODE
@ HCI_WR_LOOPBACK_MODE_CMD_OPCODE
Definition: ble_id.h:263
HCI_RD_CON_ACCEPT_TO_CMD_OPCODE
@ HCI_RD_CON_ACCEPT_TO_CMD_OPCODE
Definition: ble_id.h:154
HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE
@ HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:112
GAPM_LEPSM_UNREGISTER_CMD
@ GAPM_LEPSM_UNREGISTER_CMD
Definition: ble_id.h:766
GAPC_DISCONNECT_CMD
@ GAPC_DISCONNECT_CMD
Definition: ble_id.h:670
HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE
@ HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE
Definition: ble_id.h:533
HCI_LE_CH_SEL_ALGO_EVT_SUBCODE
@ HCI_LE_CH_SEL_ALGO_EVT_SUBCODE
Definition: ble_id.h:516
HCI_RD_CLK_OFF_CMD_OPCODE
@ HCI_RD_CLK_OFF_CMD_OPCODE
Definition: ble_id.h:102
HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE
@ HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE
Definition: ble_id.h:323
TASK_ID_GAPM
@ TASK_ID_GAPM
Definition: ble_id.h:597
HCI_LE_CREATE_BIG_TEST_CMD_OPCODE
@ HCI_LE_CREATE_BIG_TEST_CMD_OPCODE
Definition: ble_id.h:372
HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE
@ HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:160
HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE
@ HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE
Definition: ble_id.h:266
HCI_LE_DIR_ADV_REP_EVT_SUBCODE
@ HCI_LE_DIR_ADV_REP_EVT_SUBCODE
Definition: ble_id.h:507
HCI_INQ_RES_WITH_RSSI_EVT_CODE
@ HCI_INQ_RES_WITH_RSSI_EVT_CODE
Definition: ble_id.h:462
TASK_ID_LLC
@ TASK_ID_LLC
Definition: ble_id.h:576
HCI_RD_ENC_KEY_SIZE_CMD_OPCODE
@ HCI_RD_ENC_KEY_SIZE_CMD_OPCODE
Definition: ble_id.h:258
HCI_LE_SET_PRIV_MODE_CMD_OPCODE
@ HCI_LE_SET_PRIV_MODE_CMD_OPCODE
Definition: ble_id.h:345
HCI_LE_RD_PHY_CMD_OPCODE
@ HCI_LE_RD_PHY_CMD_OPCODE
Definition: ble_id.h:315
GAPM_LEPSM_REGISTER_CMD
@ GAPM_LEPSM_REGISTER_CMD
Definition: ble_id.h:765
HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE
@ HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE
Definition: ble_id.h:336
HCI_WR_LINK_POL_STG_CMD_OPCODE
@ HCI_WR_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:135
GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD
@ GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD
Definition: ble_id.h:720
GAPC_CHAN_SEL_ALGO_IND
@ GAPC_CHAN_SEL_ALGO_IND
Definition: ble_id.h:706
HCI_VS_LE_REQ_BLE_CLOCK_SYNC_EVT_SUBCODE
@ HCI_VS_LE_REQ_BLE_CLOCK_SYNC_EVT_SUBCODE
Definition: ble_id.h:559
HCI_LE_GEN_DHKEY_V1_CMD_OPCODE
@ HCI_LE_GEN_DHKEY_V1_CMD_OPCODE
Definition: ble_id.h:305
SDK_COMMON_TIMEOUT_TIMER_6
@ SDK_COMMON_TIMEOUT_TIMER_6
Definition: ble_id.h:637
GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD
@ GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD
Definition: ble_id.h:797
HCI_VS_LE_UPDATE_SNIFFER_CH_MAP_PARAM_CMD_OPCODE
@ HCI_VS_LE_UPDATE_SNIFFER_CH_MAP_PARAM_CMD_OPCODE
Definition: ble_id.h:547
HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE
@ HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE
Definition: ble_id.h:311
HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE
@ HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE
Definition: ble_id.h:98
HCI_RD_RSSI_CMD_OPCODE
@ HCI_RD_RSSI_CMD_OPCODE
Definition: ble_id.h:255
HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:91
SDK_APP_SET_SCAN_ADDR
@ SDK_APP_SET_SCAN_ADDR
Definition: ble_id.h:657
HCI_CMD_STATUS_EVT_CODE
@ HCI_CMD_STATUS_EVT_CODE
Definition: ble_id.h:445
HCI_DISC_CMP_EVT_CODE
@ HCI_DISC_CMP_EVT_CODE
Definition: ble_id.h:435
HCI_LE_TERMINATE_BIG_CMD_OPCODE
@ HCI_LE_TERMINATE_BIG_CMD_OPCODE
Definition: ble_id.h:373
TASK_ID_DISPLAY
@ TASK_ID_DISPLAY
Definition: ble_id.h:602
HCI_WR_EXT_INQ_RSP_CMD_OPCODE
@ HCI_WR_EXT_INQ_RSP_CMD_OPCODE
Definition: ble_id.h:197
HCI_QOS_SETUP_CMD_OPCODE
@ HCI_QOS_SETUP_CMD_OPCODE
Definition: ble_id.h:131
TASK_ID_DBG
@ TASK_ID_DBG
Definition: ble_id.h:580
HCI_RD_INQ_SCAN_ACT_CMD_OPCODE
@ HCI_RD_INQ_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:162
HCI_SNIFF_SUB_EVT_CODE
@ HCI_SNIFF_SUB_EVT_CODE
Definition: ble_id.h:466
GAPM_ADV_SCAN_MONITOR_EVT_REPORT_IND
@ GAPM_ADV_SCAN_MONITOR_EVT_REPORT_IND
Definition: ble_id.h:805
HCI_SP_CMP_EVT_CODE
@ HCI_SP_CMP_EVT_CODE
Definition: ble_id.h:474
HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE
@ HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE
Definition: ble_id.h:520
GATTC_EVENT_IND
@ GATTC_EVENT_IND
Definition: ble_id.h:825
GAPC_LE_PKT_SIZE_IND
@ GAPC_LE_PKT_SIZE_IND
Definition: ble_id.h:701
HCI_HOST_BUF_SIZE_CMD_OPCODE
@ HCI_HOST_BUF_SIZE_CMD_OPCODE
Definition: ble_id.h:180
HCI_LE_SET_DFT_PHY_CMD_OPCODE
@ HCI_LE_SET_DFT_PHY_CMD_OPCODE
Definition: ble_id.h:316
gattc_msg_id
gattc_msg_id
GATTC_TASK Message ID.
Definition: ble_id.h:812
HCI_EXIT_SNIFF_MODE_CMD_OPCODE
@ HCI_EXIT_SNIFF_MODE_CMD_OPCODE
Definition: ble_id.h:128
HCI_VS_LE_EVENT_NOTIFICATION_EN_CMD_OPCODE
@ HCI_VS_LE_EVENT_NOTIFICATION_EN_CMD_OPCODE
Definition: ble_id.h:552
HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE
@ HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE
Definition: ble_id.h:513
HCI_LINK_SUPV_TO_CHG_EVT_CODE
@ HCI_LINK_SUPV_TO_CHG_EVT_CODE
Definition: ble_id.h:475
HCI_DEL_RES_LT_ADDR_CMD_OPCODE
@ HCI_DEL_RES_LT_ADDR_CMD_OPCODE
Definition: ble_id.h:221
HCI_RD_INQ_MODE_CMD_OPCODE
@ HCI_RD_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:190
HCI_RD_NB_BDCST_RETX_CMD_OPCODE
@ HCI_RD_NB_BDCST_RETX_CMD_OPCODE
Definition: ble_id.h:172
HCI_WR_PIN_TYPE_CMD_OPCODE
@ HCI_WR_PIN_TYPE_CMD_OPCODE
Definition: ble_id.h:147
HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE
@ HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE
Definition: ble_id.h:521
HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE
Definition: ble_id.h:356
HCI_MODE_CHG_EVT_CODE
@ HCI_MODE_CHG_EVT_CODE
Definition: ble_id.h:450
HCI_RESET_CMD_OPCODE
@ HCI_RESET_CMD_OPCODE
Definition: ble_id.h:143
GATTC_WRITE_CFM
@ GATTC_WRITE_CFM
Definition: ble_id.h:835
SDK_RANGING_INTER_NODE_COMM_RX_DATA
@ SDK_RANGING_INTER_NODE_COMM_RX_DATA
Definition: ble_id.h:643
HCI_EXT_INQ_RES_EVT_CODE
@ HCI_EXT_INQ_RES_EVT_CODE
Definition: ble_id.h:467
GAPC_CTE_RX_CFG_CMD
@ GAPC_CTE_RX_CFG_CMD
Definition: ble_id.h:712
GAPC_BOND_CFM
@ GAPC_BOND_CFM
Definition: ble_id.h:686
HCI_VS_LE_SET_DK_DEVICE_INFO_CMD_OPCODE
@ HCI_VS_LE_SET_DK_DEVICE_INFO_CMD_OPCODE
Definition: ble_id.h:541
GAPM_PROFILE_TASK_ADD_CMD
@ GAPM_PROFILE_TASK_ADD_CMD
Definition: ble_id.h:758
GAPC_RANGING_IND
@ GAPC_RANGING_IND
Definition: ble_id.h:726
L2CC_LECB_DISCONNECT_CMD
@ L2CC_LECB_DISCONNECT_CMD
Definition: ble_id.h:856
L2CC_PDU_RECV_IND
@ L2CC_PDU_RECV_IND
Definition: ble_id.h:866
HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE
@ HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE
Definition: ble_id.h:526
GAPM_ACTIVITY_DELETE_CMD
@ GAPM_ACTIVITY_DELETE_CMD
Definition: ble_id.h:781
GAPC_GET_INFO_CMD
@ GAPC_GET_INFO_CMD
Definition: ble_id.h:671
HCI_WR_INQ_SCAN_ACT_CMD_OPCODE
@ HCI_WR_INQ_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:163
HCI_MSG_ID_LAST
@ HCI_MSG_ID_LAST
Definition: ble_id.h:622
HCI_REM_OOB_DATA_REQ_EVT_CODE
@ HCI_REM_OOB_DATA_REQ_EVT_CODE
Definition: ble_id.h:473
HCI_SET_EVT_MASK_CMD_OPCODE
@ HCI_SET_EVT_MASK_CMD_OPCODE
Definition: ble_id.h:142
GAPM_DEV_TX_PWR_IND
@ GAPM_DEV_TX_PWR_IND
Definition: ble_id.h:790
HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE
@ HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE
Definition: ble_id.h:500
HCI_LE_RANGING_IND_EVT_SUBCODE
@ HCI_LE_RANGING_IND_EVT_SUBCODE
Definition: ble_id.h:532
HCI_ENC_CHG_EVT_CODE
@ HCI_ENC_CHG_EVT_CODE
Definition: ble_id.h:438
HCI_LE_REJECT_CIS_REQ_CMD_OPCODE
@ HCI_LE_REJECT_CIS_REQ_CMD_OPCODE
Definition: ble_id.h:370
HCI_INQ_RES_EVT_CODE
@ HCI_INQ_RES_EVT_CODE
Definition: ble_id.h:432
HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE
@ HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE
Definition: ble_id.h:523
HCI_LE_CON_CMP_EVT_SUBCODE
@ HCI_LE_CON_CMP_EVT_SUBCODE
Definition: ble_id.h:497
HCI_ENH_FLUSH_CMP_EVT_CODE
@ HCI_ENH_FLUSH_CMP_EVT_CODE
Definition: ble_id.h:476
HCI_RD_VOICE_STG_CMD_OPCODE
@ HCI_RD_VOICE_STG_CMD_OPCODE
Definition: ble_id.h:168
TASK_FIRST_MSG
#define TASK_FIRST_MSG(task)
Build the first message ID of a task. (in fact a ke_msg_id_t)
Definition: ble_id.h:61
HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE
Definition: ble_id.h:239
HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE
@ HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:90
HCI_SET_CON_ENC_CMD_OPCODE
@ HCI_SET_CON_ENC_CMD_OPCODE
Definition: ble_id.h:94
L2CC_DBG_PDU_SEND_CMD
@ L2CC_DBG_PDU_SEND_CMD
Definition: ble_id.h:863
HCI_WR_CLASS_OF_DEV_CMD_OPCODE
@ HCI_WR_CLASS_OF_DEV_CMD_OPCODE
Definition: ble_id.h:167
HCI_CONFIG_DATA_PATH_CMD_OPCODE
@ HCI_CONFIG_DATA_PATH_CMD_OPCODE
Definition: ble_id.h:235
HCI_ACCEPT_CON_REQ_CMD_OPCODE
@ HCI_ACCEPT_CON_REQ_CMD_OPCODE
Definition: ble_id.h:86
SDK_RANGING_WAKEUP_RANGING
@ SDK_RANGING_WAKEUP_RANGING
Definition: ble_id.h:649
HCI_LE_ENH_CON_CMP_EVT_SUBCODE
@ HCI_LE_ENH_CON_CMP_EVT_SUBCODE
Definition: ble_id.h:506
HCI_LK_REQ_REPLY_CMD_OPCODE
@ HCI_LK_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:88
HCI_WR_VOICE_STG_CMD_OPCODE
@ HCI_WR_VOICE_STG_CMD_OPCODE
Definition: ble_id.h:169
GAPC_LE_PING_TO_IND
@ GAPC_LE_PING_TO_IND
Definition: ble_id.h:699
hci_evt_code
hci_evt_code
Definition: ble_id.h:430
HCI_VS_LE_RSSI_REPORT_INFO_EVT_SUBCODE
@ HCI_VS_LE_RSSI_REPORT_INFO_EVT_SUBCODE
Definition: ble_id.h:563
SDK_COMMON_TIMEOUT_TIMER_0
@ SDK_COMMON_TIMEOUT_TIMER_0
Timeout indication to sdk.
Definition: ble_id.h:631
GAPM_GEN_RAND_NB_IND
@ GAPM_GEN_RAND_NB_IND
Definition: ble_id.h:757
GAPM_PER_ADV_REPORT_CTRL_CMD
@ GAPM_PER_ADV_REPORT_CTRL_CMD
Definition: ble_id.h:793
HCI_ROLE_DISCOVERY_CMD_OPCODE
@ HCI_ROLE_DISCOVERY_CMD_OPCODE
Definition: ble_id.h:132
GAPC_CON_RSSI_IND
@ GAPC_CON_RSSI_IND
Definition: ble_id.h:675
TASK_ID_GATTM
@ TASK_ID_GATTM
Definition: ble_id.h:595
HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE
@ HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE
Definition: ble_id.h:120
L2CC_LECB_DISCONNECT_IND
@ L2CC_LECB_DISCONNECT_IND
Definition: ble_id.h:857
GATTC_DISC_CMD
@ GATTC_DISC_CMD
Definition: ble_id.h:816
HCI_REC_SYNC_TRAIN_CMD_OPCODE
@ HCI_REC_SYNC_TRAIN_CMD_OPCODE
Definition: ble_id.h:122
HCI_RD_PIN_TYPE_CMD_OPCODE
@ HCI_RD_PIN_TYPE_CMD_OPCODE
Definition: ble_id.h:146
HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE
@ HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE
Definition: ble_id.h:502
SDK_RANGING_STOP_RANGING
@ SDK_RANGING_STOP_RANGING
Definition: ble_id.h:651
HCI_DBG_RD_PAR_CMD_OPCODE
@ HCI_DBG_RD_PAR_CMD_OPCODE
Definition: ble_id.h:404
HCI_MAX_EVT_MSK_PAGE_1_CODE
@ HCI_MAX_EVT_MSK_PAGE_1_CODE
Definition: ble_id.h:481
HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE
@ HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE
Definition: ble_id.h:374
HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE
@ HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE
Definition: ble_id.h:204
GAPM_USE_ENC_BLOCK_IND
@ GAPM_USE_ENC_BLOCK_IND
Definition: ble_id.h:755
GAPM_PER_ADV_CTE_TX_CTL_CMD
@ GAPM_PER_ADV_CTE_TX_CTL_CMD
Definition: ble_id.h:796
GAPC_SET_LE_PING_TO_CMD
@ GAPC_SET_LE_PING_TO_CMD
Definition: ble_id.h:697
HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE
Definition: ble_id.h:329
HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:114
HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE
@ HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE
Definition: ble_id.h:105
HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE
@ HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE
Definition: ble_id.h:414
SDK_RANGING_SLEEP_RANGING
@ SDK_RANGING_SLEEP_RANGING
Definition: ble_id.h:648
HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE
@ HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE
Definition: ble_id.h:340
HCI_MAX_EVT_MSK_PAGE_2_CODE
@ HCI_MAX_EVT_MSK_PAGE_2_CODE
Definition: ble_id.h:491
TASK_ID_LLD
@ TASK_ID_LLD
Definition: ble_id.h:577
HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE
@ HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE
Definition: ble_id.h:339
GATTC_SERVER_RTX_IND
@ GATTC_SERVER_RTX_IND
Definition: ble_id.h:843
HCI_VS_LE_GET_LINK_INFO_CMD_OPCODE
@ HCI_VS_LE_GET_LINK_INFO_CMD_OPCODE
Definition: ble_id.h:543
HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE
@ HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE
Definition: ble_id.h:424
HCI_DBG_WR_MEM_CMD_OPCODE
@ HCI_DBG_WR_MEM_CMD_OPCODE
Definition: ble_id.h:398
HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE
@ HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE
Definition: ble_id.h:174
TASK_ID_GATTC
@ TASK_ID_GATTC
Definition: ble_id.h:596
HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE
@ HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE
Definition: ble_id.h:307
HCI_LE_ISO_TX_TEST_CMD_OPCODE
@ HCI_LE_ISO_TX_TEST_CMD_OPCODE
Definition: ble_id.h:379
HCI_FLUSH_CMD_OPCODE
@ HCI_FLUSH_CMD_OPCODE
Definition: ble_id.h:145
GAPM_ACTIVITY_CREATE_CMD
@ GAPM_ACTIVITY_CREATE_CMD
Definition: ble_id.h:778
GAPC_ENCRYPT_CMD
@ GAPC_ENCRYPT_CMD
Definition: ble_id.h:688
HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE
@ HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE
Definition: ble_id.h:328
GAPM_GEN_DH_KEY_IND
@ GAPM_GEN_DH_KEY_IND
Definition: ble_id.h:772
GATTC_EVENT_REQ_IND
@ GATTC_EVENT_REQ_IND
Definition: ble_id.h:826
HCI_DBG_BT_SEND_LMP_CMD_OPCODE
@ HCI_DBG_BT_SEND_LMP_CMD_OPCODE
Definition: ble_id.h:408
HCI_WR_LINK_SUPV_TO_CMD_OPCODE
@ HCI_WR_LINK_SUPV_TO_CMD_OPCODE
Definition: ble_id.h:183
GAPM_PROFILE_ADDED_IND
@ GAPM_PROFILE_ADDED_IND
Definition: ble_id.h:759
HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE
@ HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE
Definition: ble_id.h:214
GAPM_MAX_ADV_DATA_LEN_IND
@ GAPM_MAX_ADV_DATA_LEN_IND
Definition: ble_id.h:788
HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE
@ HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE
Definition: ble_id.h:252
SDK_RANGING_START_RANGING
@ SDK_RANGING_START_RANGING
Definition: ble_id.h:650
HCI_RD_TX_PWR_LVL_CMD_OPCODE
@ HCI_RD_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:176
HCI_RD_STORED_LK_CMD_OPCODE
@ HCI_RD_STORED_LK_CMD_OPCODE
Definition: ble_id.h:149
GAPC_SIGN_CMD
@ GAPC_SIGN_CMD
Definition: ble_id.h:729
HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE
@ HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE
Definition: ble_id.h:207
SDK_COMMON_TIMEOUT_TIMER_4
@ SDK_COMMON_TIMEOUT_TIMER_4
Definition: ble_id.h:635
GAPM_GEN_DH_KEY_CMD
@ GAPM_GEN_DH_KEY_CMD
Definition: ble_id.h:771
HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE
@ HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE
Definition: ble_id.h:364
HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE
@ HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE
Definition: ble_id.h:391
HCI_LE_RD_WLST_SIZE_CMD_OPCODE
@ HCI_LE_RD_WLST_SIZE_CMD_OPCODE
Definition: ble_id.h:282
L2CC_LECB_CONNECT_IND
@ L2CC_LECB_CONNECT_IND
Definition: ble_id.h:855
HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE
@ HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE
Definition: ble_id.h:441
HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE
@ HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE
Definition: ble_id.h:335
GAPM_SYNC_ESTABLISHED_IND
@ GAPM_SYNC_ESTABLISHED_IND
Definition: ble_id.h:787
GAPC_GET_DEV_INFO_CFM
@ GAPC_GET_DEV_INFO_CFM
Definition: ble_id.h:677
HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE
Definition: ble_id.h:245
HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE
@ HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE
Definition: ble_id.h:343
GAPM_ADDR_SOLVED_IND
@ GAPM_ADDR_SOLVED_IND
Definition: ble_id.h:752
HCI_CON_SLV_BCST_TO_EVT_CODE
@ HCI_CON_SLV_BCST_TO_EVT_CODE
Definition: ble_id.h:485
HCI_LE_TX_TEST_V3_CMD_OPCODE
@ HCI_LE_TX_TEST_V3_CMD_OPCODE
Definition: ble_id.h:347
HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
@ HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:271
TASK_ID_LD
@ TASK_ID_LD
Definition: ble_id.h:586
SDK_RANGING_INTER_NODE_COMM_ERR_OCCUR
@ SDK_RANGING_INTER_NODE_COMM_ERR_OCCUR
Definition: ble_id.h:646
HCI_LE_RMV_ADV_SET_CMD_OPCODE
@ HCI_LE_RMV_ADV_SET_CMD_OPCODE
Definition: ble_id.h:327
HCI_RD_CLK_CMD_OPCODE
@ HCI_RD_CLK_CMD_OPCODE
Definition: ble_id.h:257
TASK_ID_GAPC
@ TASK_ID_GAPC
Definition: ble_id.h:598
HCI_DBG_RF_REG_WR_CMD_OPCODE
@ HCI_DBG_RF_REG_WR_CMD_OPCODE
Definition: ble_id.h:422
HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE
@ HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE
Definition: ble_id.h:529
GAPM_UNKNOWN_TASK_IND
@ GAPM_UNKNOWN_TASK_IND
Definition: ble_id.h:760
L2CC_LECB_ADD_IND
@ L2CC_LECB_ADD_IND
Definition: ble_id.h:859
HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE
@ HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:225
GAPM_DEV_RF_PATH_COMP_IND
@ GAPM_DEV_RF_PATH_COMP_IND
Definition: ble_id.h:791
HCI_LE_CON_UPDATE_CMD_OPCODE
@ HCI_LE_CON_UPDATE_CMD_OPCODE
Definition: ble_id.h:286
TASK_ID_SDK
@ TASK_ID_SDK
Definition: ble_id.h:592
HCI_RD_LOCAL_NAME_CMD_OPCODE
@ HCI_RD_LOCAL_NAME_CMD_OPCODE
Definition: ble_id.h:153
HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE
@ HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE
Definition: ble_id.h:341
GAPC_BOND_REQ_IND
@ GAPC_BOND_REQ_IND
Definition: ble_id.h:685
HCI_RD_BUF_SIZE_CMD_OPCODE
@ HCI_RD_BUF_SIZE_CMD_OPCODE
Definition: ble_id.h:242
HCI_TRUNC_PAGE_CAN_CMD_OPCODE
@ HCI_TRUNC_PAGE_CAN_CMD_OPCODE
Definition: ble_id.h:118
HCI_VS_LE_RSSI_RANGING_TYPE_NOTIF_EVT_SUBCODE
@ HCI_VS_LE_RSSI_RANGING_TYPE_NOTIF_EVT_SUBCODE
Definition: ble_id.h:564
HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE
@ HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE
Definition: ble_id.h:322
HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
@ HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:302
GATTC_CMP_EVT
@ GATTC_CMP_EVT
Definition: ble_id.h:813
HCI_PUBLIC_ADDR_SET_CMD_OPCODE
@ HCI_PUBLIC_ADDR_SET_CMD_OPCODE
Definition: ble_id.h:393
HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
@ HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
Definition: ble_id.h:360
HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE
Definition: ble_id.h:359
HCI_SYNC_CON_CMP_EVT_CODE
@ HCI_SYNC_CON_CMP_EVT_CODE
Definition: ble_id.h:464
HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:294
HCI_IO_CAP_RSP_EVT_CODE
@ HCI_IO_CAP_RSP_EVT_CODE
Definition: ble_id.h:470
SDK_COMMON_TIMEOUT_TIMER_9
@ SDK_COMMON_TIMEOUT_TIMER_9
Definition: ble_id.h:640
HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE
@ HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE
Definition: ble_id.h:304
HCI_NB_CMP_PKTS_EVT_CODE
@ HCI_NB_CMP_PKTS_EVT_CODE
Definition: ble_id.h:449
GAPC_CTE_IQ_REPORT_IND
@ GAPC_CTE_IQ_REPORT_IND
Definition: ble_id.h:715
HCI_LE_REMOVE_CIG_CMD_OPCODE
@ HCI_LE_REMOVE_CIG_CMD_OPCODE
Definition: ble_id.h:368
HCI_CMD_CMP_EVENT
@ HCI_CMD_CMP_EVENT
Definition: ble_id.h:615
HCI_TRUNC_PAGE_CMD_OPCODE
@ HCI_TRUNC_PAGE_CMD_OPCODE
Definition: ble_id.h:117
HCI_KEYPRESS_NOTIF_EVT_CODE
@ HCI_KEYPRESS_NOTIF_EVT_CODE
Definition: ble_id.h:478
GAPM_SUGG_DFLT_DATA_LEN_IND
@ GAPM_SUGG_DFLT_DATA_LEN_IND
Definition: ble_id.h:761
HCI_RD_CLK_OFF_CMP_EVT_CODE
@ HCI_RD_CLK_OFF_CMP_EVT_CODE
Definition: ble_id.h:457
HCI_VS_LE_DISCONNECT_SNIFFER_CMD_OPCODE
@ HCI_VS_LE_DISCONNECT_SNIFFER_CMD_OPCODE
Definition: ble_id.h:545
GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD
@ GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD
Definition: ble_id.h:794
HCI_EXIT_PER_INQ_MODE_CMD_OPCODE
@ HCI_EXIT_PER_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:82
HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE
@ HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE
Definition: ble_id.h:338
GATTC_READ_CFM
@ GATTC_READ_CFM
Definition: ble_id.h:833
HCI_AUTH_CMP_EVT_CODE
@ HCI_AUTH_CMP_EVT_CODE
Definition: ble_id.h:436
HCI_DBG_WLAN_COEX_CMD_OPCODE
@ HCI_DBG_WLAN_COEX_CMD_OPCODE
Definition: ble_id.h:406
HCI_USER_PASSKEY_NOTIF_EVT_CODE
@ HCI_USER_PASSKEY_NOTIF_EVT_CODE
Definition: ble_id.h:477
HCI_DBG_WR_FLASH_CMD_OPCODE
@ HCI_DBG_WR_FLASH_CMD_OPCODE
Definition: ble_id.h:402
HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE
@ HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE
Definition: ble_id.h:281
HCI_LE_CON_IQ_REPORT_EVT_SUBCODE
@ HCI_LE_CON_IQ_REPORT_EVT_SUBCODE
Definition: ble_id.h:518
HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE
@ HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE
Definition: ble_id.h:285
HCI_RD_LOCAL_VER_INFO_CMD_OPCODE
@ HCI_RD_LOCAL_VER_INFO_CMD_OPCODE
Definition: ble_id.h:238
GAPM_GET_DEV_INFO_CMD
@ GAPM_GET_DEV_INFO_CMD
Definition: ble_id.h:745
HCI_WR_SP_DBG_MODE_CMD_OPCODE
@ HCI_WR_SP_DBG_MODE_CMD_OPCODE
Definition: ble_id.h:265
HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE
@ HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE
Definition: ble_id.h:177
HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE
@ HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:333
GAPM_DBG_MEM_INFO_IND
@ GAPM_DBG_MEM_INFO_IND
Definition: ble_id.h:749
GAPC_KEY_PRESS_NOTIFICATION_CMD
@ GAPC_KEY_PRESS_NOTIFICATION_CMD
Definition: ble_id.h:702
HCI_EN_DUT_MODE_CMD_OPCODE
@ HCI_EN_DUT_MODE_CMD_OPCODE
Definition: ble_id.h:264
GAPM_SET_ADV_DATA_CMD
@ GAPM_SET_ADV_DATA_CMD
Definition: ble_id.h:784
HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE
@ HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE
Definition: ble_id.h:505
HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE
@ HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE
Definition: ble_id.h:362
MSG_ID
#define MSG_ID(task, idx)
Message identifier index.
Definition: ble_id.h:58
HCI_WR_PAGE_TO_CMD_OPCODE
@ HCI_WR_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:157
HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE
@ HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE
Definition: ble_id.h:463
HCI_LE_CREATE_CIS_CMD_OPCODE
@ HCI_LE_CREATE_CIS_CMD_OPCODE
Definition: ble_id.h:367
HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE
@ HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE
Definition: ble_id.h:312
TASK_ID_L2CC
@ TASK_ID_L2CC
Definition: ble_id.h:594
HCI_LE_TX_TEST_V1_CMD_OPCODE
@ HCI_LE_TX_TEST_V1_CMD_OPCODE
Definition: ble_id.h:297
HCI_HOST_NB_CMP_PKTS_CMD_OPCODE
@ HCI_HOST_NB_CMP_PKTS_CMD_OPCODE
Definition: ble_id.h:181
HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE
@ HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE
Definition: ble_id.h:479
HCI_COMMAND
@ HCI_COMMAND
Definition: ble_id.h:619
sdk_msg_id
sdk_msg_id
SDK_TASK Message ID.
Definition: ble_id.h:629
HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE
@ HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:110
HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE
@ HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:137
GAPC_BOND_CMD
@ GAPC_BOND_CMD
Definition: ble_id.h:684
HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE
@ HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE
Definition: ble_id.h:332
HCI_DISCONNECT_CMD_OPCODE
@ HCI_DISCONNECT_CMD_OPCODE
Definition: ble_id.h:84
HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:240
HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE
@ HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE
Definition: ble_id.h:276
HCI_VS_LE_CON_PARAM_NOTIF_EVT_SUBCODE
@ HCI_VS_LE_CON_PARAM_NOTIF_EVT_SUBCODE
Definition: ble_id.h:560
HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE
@ HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE
Definition: ble_id.h:194
HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE
@ HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE
Definition: ble_id.h:350
GAPM_GEN_RAND_ADDR_CMD
@ GAPM_GEN_RAND_ADDR_CMD
Definition: ble_id.h:753
HCI_REFRESH_ENC_KEY_CMD_OPCODE
@ HCI_REFRESH_ENC_KEY_CMD_OPCODE
Definition: ble_id.h:198
GAPM_UNKNOWN_MSG_IND
@ GAPM_UNKNOWN_MSG_IND
Definition: ble_id.h:792
HCI_HOLD_MODE_CMD_OPCODE
@ HCI_HOLD_MODE_CMD_OPCODE
Definition: ble_id.h:126
L2CC_UNKNOWN_MSG_IND
@ L2CC_UNKNOWN_MSG_IND
Definition: ble_id.h:862
GAPC_BOND_IND
@ GAPC_BOND_IND
Definition: ble_id.h:687
HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE
Definition: ble_id.h:247
SDK_RANGING_ANCHOR_START_RANGING
@ SDK_RANGING_ANCHOR_START_RANGING
Definition: ble_id.h:652
GATTC_EVENT_CFM
@ GATTC_EVENT_CFM
Definition: ble_id.h:827
HCI_RD_SP_MODE_CMD_OPCODE
@ HCI_RD_SP_MODE_CMD_OPCODE
Definition: ble_id.h:199
GAPC_LE_PING_TO_VAL_IND
@ GAPC_LE_PING_TO_VAL_IND
Definition: ble_id.h:698
gapc_msg_id
gapc_msg_id
GAPC_TASK Message ID.
Definition: ble_id.h:665
GAPM_SCAN_REQUEST_IND
@ GAPM_SCAN_REQUEST_IND
Definition: ble_id.h:786
GAPM_DBG_IQGEN_CFG_CMD
@ GAPM_DBG_IQGEN_CFG_CMD
Definition: ble_id.h:798
HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE
@ HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE
Definition: ble_id.h:223
HCI_LE_RD_REM_FEATS_CMD_OPCODE
@ HCI_LE_RD_REM_FEATS_CMD_OPCODE
Definition: ble_id.h:289
HCI_QOS_SETUP_CMP_EVT_CODE
@ HCI_QOS_SETUP_CMP_EVT_CODE
Definition: ble_id.h:443
HCI_LE_GEN_DHKEY_V2_CMD_OPCODE
@ HCI_LE_GEN_DHKEY_V2_CMD_OPCODE
Definition: ble_id.h:361
HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE
@ HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:202
GAPM_DEV_VERSION_IND
@ GAPM_DEV_VERSION_IND
Definition: ble_id.h:746
HCI_WR_SP_MODE_CMD_OPCODE
@ HCI_WR_SP_MODE_CMD_OPCODE
Definition: ble_id.h:200
HCI_USER_CFM_REQ_EVT_CODE
@ HCI_USER_CFM_REQ_EVT_CODE
Definition: ble_id.h:471
HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE
@ HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE
Definition: ble_id.h:369
HCI_LE_CREATE_CON_CMD_OPCODE
@ HCI_LE_CREATE_CON_CMD_OPCODE
Definition: ble_id.h:280
GAPC_CTE_RSP_CTRL_CMD
@ GAPC_CTE_RSP_CTRL_CMD
Definition: ble_id.h:714
GAPC_SMP_REP_ATTEMPTS_TIMER_IND
@ GAPC_SMP_REP_ATTEMPTS_TIMER_IND
Definition: ble_id.h:733
GATTC_MTU_CHANGED_IND
@ GATTC_MTU_CHANGED_IND
Definition: ble_id.h:815
HCI_LE_DATA_LEN_CHG_EVT_SUBCODE
@ HCI_LE_DATA_LEN_CHG_EVT_SUBCODE
Definition: ble_id.h:503
HCI_SYNC_TRAIN_REC_EVT_CODE
@ HCI_SYNC_TRAIN_REC_EVT_CODE
Definition: ble_id.h:483
HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:530
SDK_COMMON_TIMEOUT_TIMER_1
@ SDK_COMMON_TIMEOUT_TIMER_1
Definition: ble_id.h:632
TASK_ID_APP
@ TASK_ID_APP
Definition: ble_id.h:599
GAPC_PARAM_UPDATE_CFM
@ GAPC_PARAM_UPDATE_CFM
Definition: ble_id.h:682
HCI_DBG_ID_FLASH_CMD_OPCODE
@ HCI_DBG_ID_FLASH_CMD_OPCODE
Definition: ble_id.h:400
HCI_CON_SLV_BCST_REC_EVT_CODE
@ HCI_CON_SLV_BCST_REC_EVT_CODE
Definition: ble_id.h:484
GAPC_READ_REMOTE_TX_PWR_IND
@ GAPC_READ_REMOTE_TX_PWR_IND
Definition: ble_id.h:722
HCI_CON_CMP_EVT_CODE
@ HCI_CON_CMP_EVT_CODE
Definition: ble_id.h:433
HCI_RD_EXT_INQ_LEN_CMD_OPCODE
@ HCI_RD_EXT_INQ_LEN_CMD_OPCODE
Definition: ble_id.h:232
GAPC_SET_PREF_SLAVE_EVT_DUR_CMD
@ GAPC_SET_PREF_SLAVE_EVT_DUR_CMD
Definition: ble_id.h:708
HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE
@ HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE
Definition: ble_id.h:244
HCI_VS_LE_RSSI_ENABLE_RANGING_CMD_OPCODE
@ HCI_VS_LE_RSSI_ENABLE_RANGING_CMD_OPCODE
Definition: ble_id.h:550
HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE
@ HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE
Definition: ble_id.h:253
HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE
@ HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE
Definition: ble_id.h:178
GATTC_TRANSACTION_TO_ERROR_IND
@ GATTC_TRANSACTION_TO_ERROR_IND
Definition: ble_id.h:840
GAPM_LE_TEST_IQ_REPORT_IND
@ GAPM_LE_TEST_IQ_REPORT_IND
Definition: ble_id.h:769
GAPM_CMP_EVT
@ GAPM_CMP_EVT
Definition: ble_id.h:741
GAPM_EXT_ADV_REPORT_IND
@ GAPM_EXT_ADV_REPORT_IND
Definition: ble_id.h:785
HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE
@ HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE
Definition: ble_id.h:215
HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE
@ HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE
Definition: ble_id.h:514
GAPM_UNKNOWN_TASK_MSG
@ GAPM_UNKNOWN_TASK_MSG
Definition: ble_id.h:799
HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE
@ HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE
Definition: ble_id.h:407
TASK_ID_MESH
@ TASK_ID_MESH
Definition: ble_id.h:603
HCI_LK_REQ_EVT_CODE
@ HCI_LK_REQ_EVT_CODE
Definition: ble_id.h:453
HCI_TRUNC_PAGE_CMP_EVT_CODE
@ HCI_TRUNC_PAGE_CMP_EVT_CODE
Definition: ble_id.h:486
HCI_RD_LOC_OOB_DATA_CMD_OPCODE
@ HCI_RD_LOC_OOB_DATA_CMD_OPCODE
Definition: ble_id.h:201
GAPC_ENCRYPT_CFM
@ GAPC_ENCRYPT_CFM
Definition: ble_id.h:690
GAPM_SET_CHANNEL_MAP_CMD
@ GAPM_SET_CHANNEL_MAP_CMD
Definition: ble_id.h:744
GAPC_CMP_EVT
@ GAPC_CMP_EVT
Definition: ble_id.h:666
HCI_DBG_RD_FLASH_CMD_OPCODE
@ HCI_DBG_RD_FLASH_CMD_OPCODE
Definition: ble_id.h:403
HCI_CON_PKT_TYPE_CHG_EVT_CODE
@ HCI_CON_PKT_TYPE_CHG_EVT_CODE
Definition: ble_id.h:458
HCI_VS_LE_CH_MAP_PARAM_NOTIF_EVT_SUBCODE
@ HCI_VS_LE_CH_MAP_PARAM_NOTIF_EVT_SUBCODE
Definition: ble_id.h:561
HCI_LE_RX_TEST_V3_CMD_OPCODE
@ HCI_LE_RX_TEST_V3_CMD_OPCODE
Definition: ble_id.h:346
HCI_LE_SET_EVT_MASK_CMD_OPCODE
@ HCI_LE_SET_EVT_MASK_CMD_OPCODE
LE Commands Opcodes.
Definition: ble_id.h:269
HCI_RD_LINK_POL_STG_CMD_OPCODE
@ HCI_RD_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:134
hci_msg_id
hci_msg_id
HCI task Message ID.
Definition: ble_id.h:612
GAPM_PUBLIC_ADDR_SET_CMD
@ GAPM_PUBLIC_ADDR_SET_CMD
Definition: ble_id.h:803
TASK_ID_HCI
@ TASK_ID_HCI
Definition: ble_id.h:601
HCI_CREATE_CON_CMD_OPCODE
@ HCI_CREATE_CON_CMD_OPCODE
Definition: ble_id.h:83
L2CC_LECB_CONNECT_REQ_IND
@ L2CC_LECB_CONNECT_REQ_IND
Definition: ble_id.h:853
GAPC_PEER_FEATURES_IND
@ GAPC_PEER_FEATURES_IND
Definition: ble_id.h:674
HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE
@ HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE
Definition: ble_id.h:321
HCI_LE_RD_TX_PWR_CMD_OPCODE
@ HCI_LE_RD_TX_PWR_CMD_OPCODE
Definition: ble_id.h:342
HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE
@ HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE
Definition: ble_id.h:415
gapm_msg_id
gapm_msg_id
GAPM_TASK Message ID.
Definition: ble_id.h:740
GATTC_DISC_CHAR_IND
@ GATTC_DISC_CHAR_IND
Definition: ble_id.h:819
HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE
Definition: ble_id.h:248
HCI_WR_CON_ACCEPT_TO_CMD_OPCODE
@ HCI_WR_CON_ACCEPT_TO_CMD_OPCODE
Definition: ble_id.h:155
GAPC_CON_CHANNEL_MAP_IND
@ GAPC_CON_CHANNEL_MAP_IND
Definition: ble_id.h:695
GAPC_PARAM_UPDATED_IND
@ GAPC_PARAM_UPDATED_IND
Definition: ble_id.h:683
HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE
@ HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE
Definition: ble_id.h:375
HCI_LK_NOTIF_EVT_CODE
@ HCI_LK_NOTIF_EVT_CODE
Definition: ble_id.h:454
HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE
@ HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE
Definition: ble_id.h:378
GATTC_SDP_SVC_IND
@ GATTC_SDP_SVC_IND
Definition: ble_id.h:839
SDK_RANGING_ANCHOR_STOP_RANGING
@ SDK_RANGING_ANCHOR_STOP_RANGING
Definition: ble_id.h:653
L2CC_PDU_SEND_CMD
@ L2CC_PDU_SEND_CMD
Definition: ble_id.h:865
HCI_SLV_PAGE_RSP_TO_EVT_CODE
@ HCI_SLV_PAGE_RSP_TO_EVT_CODE
Definition: ble_id.h:487
HCI_SET_EVT_FILTER_CMD_OPCODE
@ HCI_SET_EVT_FILTER_CMD_OPCODE
Definition: ble_id.h:144
GATTC_SEND_SVC_CHANGED_CMD
@ GATTC_SEND_SVC_CHANGED_CMD
Definition: ble_id.h:830
HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE
@ HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE
Definition: ble_id.h:349
GAPC_SIGN_IND
@ GAPC_SIGN_IND
Definition: ble_id.h:730
HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE
@ HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE
Definition: ble_id.h:504
HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE
@ HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE
Definition: ble_id.h:136
HCI_RD_BD_ADDR_CMD_OPCODE
@ HCI_RD_BD_ADDR_CMD_OPCODE
Definition: ble_id.h:243
HCI_LE_SET_ADV_PARAM_CMD_OPCODE
@ HCI_LE_SET_ADV_PARAM_CMD_OPCODE
Definition: ble_id.h:273
HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE
@ HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE
Definition: ble_id.h:488
SDK_COMMON_TIMEOUT_TIMER_2
@ SDK_COMMON_TIMEOUT_TIMER_2
Definition: ble_id.h:633
HCI_LE_EXT_CREATE_CON_CMD_OPCODE
@ HCI_LE_EXT_CREATE_CON_CMD_OPCODE
Definition: ble_id.h:334
HCI_SWITCH_ROLE_CMD_OPCODE
@ HCI_SWITCH_ROLE_CMD_OPCODE
Definition: ble_id.h:133
HCI_MSG_ID_FIRST
@ HCI_MSG_ID_FIRST
Definition: ble_id.h:613
HCI_WR_EXT_PAGE_TO_CMD_OPCODE
@ HCI_WR_EXT_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:231
hci_le_evt_subcode
hci_le_evt_subcode
Definition: ble_id.h:496
GATTC_EXC_MTU_CMD
@ GATTC_EXC_MTU_CMD
Definition: ble_id.h:814
HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE
@ HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE
Definition: ble_id.h:161
HCI_RD_CLASS_OF_DEV_CMD_OPCODE
@ HCI_RD_CLASS_OF_DEV_CMD_OPCODE
Definition: ble_id.h:166
HCI_LE_REQ_PEER_SCA_CMD_OPCODE
@ HCI_LE_REQ_PEER_SCA_CMD_OPCODE
Definition: ble_id.h:376
GAPC_PARAM_UPDATE_CMD
@ GAPC_PARAM_UPDATE_CMD
Definition: ble_id.h:680
GATTC_ATT_INFO_REQ_IND
@ GATTC_ATT_INFO_REQ_IND
Definition: ble_id.h:836
HCI_VS_LE_RSSI_UPDATE_RANGING_TYPE_CMD_OPCODE
@ HCI_VS_LE_RSSI_UPDATE_RANGING_TYPE_CMD_OPCODE
Definition: ble_id.h:551
HCI_LE_RANGING_CMP_EVT_SUBCODE
@ HCI_LE_RANGING_CMP_EVT_SUBCODE
Definition: ble_id.h:534
HCI_LE_SET_PER_ADV_EN_CMD_OPCODE
@ HCI_LE_SET_PER_ADV_EN_CMD_OPCODE
Definition: ble_id.h:331
HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE
@ HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE
Definition: ble_id.h:175
GAPC_READ_LOCAL_TX_PWR_CMD
@ GAPC_READ_LOCAL_TX_PWR_CMD
Definition: ble_id.h:716
GAPM_RESOLV_ADDR_CMD
@ GAPM_RESOLV_ADDR_CMD
Definition: ble_id.h:751
HCI_RD_REM_SUPP_FEATS_CMD_OPCODE
@ HCI_RD_REM_SUPP_FEATS_CMD_OPCODE
Definition: ble_id.h:99
HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE
@ HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE
Definition: ble_id.h:284
HCI_LE_ISO_TEST_END_CMD_OPCODE
@ HCI_LE_ISO_TEST_END_CMD_OPCODE
Definition: ble_id.h:382
HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:509
L2CC_LECB_CONNECT_CFM
@ L2CC_LECB_CONNECT_CFM
Definition: ble_id.h:854
HCI_HW_ERR_EVT_CODE
@ HCI_HW_ERR_EVT_CODE
Definition: ble_id.h:446
hci_vs_dbg_evt_subcode
hci_vs_dbg_evt_subcode
Definition: ble_id.h:556
HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE
@ HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE
Definition: ble_id.h:218
HCI_SYNC_CON_CHG_EVT_CODE
@ HCI_SYNC_CON_CHG_EVT_CODE
Definition: ble_id.h:465
HCI_LE_RAND_CMD_OPCODE
@ HCI_LE_RAND_CMD_OPCODE
Definition: ble_id.h:291
GATTC_DISC_SVC_IND
@ GATTC_DISC_SVC_IND
Definition: ble_id.h:817
SDK_COMMON_TIMEOUT_TIMER_5
@ SDK_COMMON_TIMEOUT_TIMER_5
Definition: ble_id.h:636
GAPC_READ_LOCAL_TX_PWR_IND
@ GAPC_READ_LOCAL_TX_PWR_IND
Definition: ble_id.h:721
HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE
@ HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:188
HCI_DBG_RF_REG_RD_CMD_OPCODE
@ HCI_DBG_RF_REG_RD_CMD_OPCODE
Definition: ble_id.h:421
HCI_LE_SET_SCAN_PARAM_CMD_OPCODE
@ HCI_LE_SET_SCAN_PARAM_CMD_OPCODE
Definition: ble_id.h:278
HCI_USER_CFM_REQ_REPLY_CMD_OPCODE
@ HCI_USER_CFM_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:108
HCI_DBG_RF_CNTL_TX_CMD_OPCODE
@ HCI_DBG_RF_CNTL_TX_CMD_OPCODE
Definition: ble_id.h:426
HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:113
GAPM_ACTIVITY_START_CMD
@ GAPM_ACTIVITY_START_CMD
Definition: ble_id.h:779
GAPC_GET_DEV_INFO_REQ_IND
@ GAPC_GET_DEV_INFO_REQ_IND
Definition: ble_id.h:676
HCI_LE_TX_TEST_V2_CMD_OPCODE
@ HCI_LE_TX_TEST_V2_CMD_OPCODE
Definition: ble_id.h:319
HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE
@ HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE
Definition: ble_id.h:306
HCI_SET_CON_SLV_BCST_CMD_OPCODE
@ HCI_SET_CON_SLV_BCST_CMD_OPCODE
Definition: ble_id.h:119
HCI_LE_TX_TEST_V4_CMD_OPCODE
@ HCI_LE_TX_TEST_V4_CMD_OPCODE
Definition: ble_id.h:390
HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE
@ HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:314
GAPM_DEV_ADV_TX_POWER_IND
@ GAPM_DEV_ADV_TX_POWER_IND
Definition: ble_id.h:748
HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE
@ HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE
Definition: ble_id.h:209
HCI_FLOW_SPEC_CMP_EVT_CODE
@ HCI_FLOW_SPEC_CMP_EVT_CODE
Definition: ble_id.h:461
HCI_RD_LINK_QUAL_CMD_OPCODE
@ HCI_RD_LINK_QUAL_CMD_OPCODE
Definition: ble_id.h:254
TASK_ID_LB
@ TASK_ID_LB
Definition: ble_id.h:585
HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE
@ HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE
Definition: ble_id.h:528
HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE
@ HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE
Definition: ble_id.h:116
GAPM_MAX_DATA_LEN_IND
@ GAPM_MAX_DATA_LEN_IND
Definition: ble_id.h:762
HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE
@ HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE
Definition: ble_id.h:381
L2CC_LECB_CONNECT_CMD
@ L2CC_LECB_CONNECT_CMD
Definition: ble_id.h:852
HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE
@ HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE
Definition: ble_id.h:274
HCI_RD_REM_VER_INFO_CMP_EVT_CODE
@ HCI_RD_REM_VER_INFO_CMP_EVT_CODE
Definition: ble_id.h:442
L2CC_LECB_SDU_RECV_IND
@ L2CC_LECB_SDU_RECV_IND
Definition: ble_id.h:861
HCI_INQ_CMP_EVT_CODE
@ HCI_INQ_CMP_EVT_CODE
Definition: ble_id.h:431
HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE
@ HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE
Definition: ble_id.h:357
HCI_CREATE_CON_CANCEL_CMD_OPCODE
@ HCI_CREATE_CON_CANCEL_CMD_OPCODE
Definition: ble_id.h:85
GAPC_PER_ADV_SYNC_TRANS_CMD
@ GAPC_PER_ADV_SYNC_TRANS_CMD
Definition: ble_id.h:710
HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE
@ HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE
Definition: ble_id.h:525
HCI_DBG_ER_FLASH_CMD_OPCODE
@ HCI_DBG_ER_FLASH_CMD_OPCODE
Definition: ble_id.h:401
L2CC_CMP_EVT
@ L2CC_CMP_EVT
Definition: ble_id.h:851
GAPM_ADDR_RENEW_CMD
@ GAPM_ADDR_RENEW_CMD
Definition: ble_id.h:802
HCI_RD_EXT_INQ_RSP_CMD_OPCODE
@ HCI_RD_EXT_INQ_RSP_CMD_OPCODE
Definition: ble_id.h:196
GAPC_TX_PWR_CHANGE_REPORT_IND
@ GAPC_TX_PWR_CHANGE_REPORT_IND
Definition: ble_id.h:723
HCI_NO_OPERATION_CMD_OPCODE
@ HCI_NO_OPERATION_CMD_OPCODE
Definition: ble_id.h:76
HCI_DBG_RD_KE_STATS_CMD_OPCODE
@ HCI_DBG_RD_KE_STATS_CMD_OPCODE
Definition: ble_id.h:410
SDK_RANGING_TIMEOUT_DISPATCH
@ SDK_RANGING_TIMEOUT_DISPATCH
Definition: ble_id.h:655
HCI_RD_LINK_SUPV_TO_CMD_OPCODE
@ HCI_RD_LINK_SUPV_TO_CMD_OPCODE
Definition: ble_id.h:182
GATTC_READ_REQ_IND
@ GATTC_READ_REQ_IND
Definition: ble_id.h:832
HCI_FLUSH_OCCURRED_EVT_CODE
@ HCI_FLUSH_OCCURRED_EVT_CODE
Definition: ble_id.h:447
L2CC_DBG_PDU_RECV_IND
@ L2CC_DBG_PDU_RECV_IND
Definition: ble_id.h:864
HCI_LE_SET_DATA_LEN_CMD_OPCODE
@ HCI_LE_SET_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:301
HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:109
HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE
@ HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE
Definition: ble_id.h:524
GAPM_RAL_ADDR_IND
@ GAPM_RAL_ADDR_IND
Definition: ble_id.h:763
HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE
@ HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE
Definition: ble_id.h:510
GAPM_LE_TEST_END_IND
@ GAPM_LE_TEST_END_IND
Definition: ble_id.h:768
HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE
@ HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE
Definition: ble_id.h:387
TASK_ID_LLI
@ TASK_ID_LLI
Definition: ble_id.h:578
HCI_DBG_META_EVT_CODE
@ HCI_DBG_META_EVT_CODE
Definition: ble_id.h:492
SDK_RANGING_INTER_NODE_COMM_TX_DATA_CMP
@ SDK_RANGING_INTER_NODE_COMM_TX_DATA_CMP
Definition: ble_id.h:644
GATTC_ATT_INFO_CFM
@ GATTC_ATT_INFO_CFM
Definition: ble_id.h:837
HCI_REM_NAME_REQ_CMP_EVT_CODE
@ HCI_REM_NAME_REQ_CMP_EVT_CODE
Definition: ble_id.h:437
HCI_WR_NB_BDCST_RETX_CMD_OPCODE
@ HCI_WR_NB_BDCST_RETX_CMD_OPCODE
Definition: ble_id.h:173
HCI_VS_LE_EVENT_NOTIFICATION_REPORT_INFO_EVT_SUBCODE
@ HCI_VS_LE_EVENT_NOTIFICATION_REPORT_INFO_EVT_SUBCODE
Definition: ble_id.h:565
HCI_DATA_BUF_OVFLW_EVT_CODE
@ HCI_DATA_BUF_OVFLW_EVT_CODE
Definition: ble_id.h:455
HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE
@ HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE
Definition: ble_id.h:148
HCI_FLOW_SPEC_CMD_OPCODE
@ HCI_FLOW_SPEC_CMD_OPCODE
Definition: ble_id.h:138
HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE
@ HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE
Definition: ble_id.h:249
HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE
@ HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE
Definition: ble_id.h:384
GAPC_PEER_ATT_INFO_IND
@ GAPC_PEER_ATT_INFO_IND
Definition: ble_id.h:672
HCI_ENC_KEY_REFRESH_CMP_EVT_CODE
@ HCI_ENC_KEY_REFRESH_CMP_EVT_CODE
Definition: ble_id.h:468
HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE
@ HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE
Definition: ble_id.h:413
GAPC_CTE_TX_CFG_CMD
@ GAPC_CTE_TX_CFG_CMD
Definition: ble_id.h:711
GATTC_DISC_SVC_INCL_IND
@ GATTC_DISC_SVC_INCL_IND
Definition: ble_id.h:818
HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE
@ HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:226
HCI_LE_SET_ADV_DATA_CMD_OPCODE
@ HCI_LE_SET_ADV_DATA_CMD_OPCODE
Definition: ble_id.h:275
HCI_START_SYNC_TRAIN_CMD_OPCODE
@ HCI_START_SYNC_TRAIN_CMD_OPCODE
Definition: ble_id.h:121
GAPC_SEC_REQ_TIMEOUT_IND
@ GAPC_SEC_REQ_TIMEOUT_IND
Definition: ble_id.h:696
HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE
@ HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE
Definition: ble_id.h:187
GATTC_SVC_CHANGED_CFG_IND
@ GATTC_SVC_CHANGED_CFG_IND
Definition: ble_id.h:831
HCI_LE_CIS_REQUEST_EVT_SUBCODE
@ HCI_LE_CIS_REQUEST_EVT_SUBCODE
Definition: ble_id.h:522
GAPM_RESET_CMD
@ GAPM_RESET_CMD
Definition: ble_id.h:742
HCI_SNIFF_MODE_CMD_OPCODE
@ HCI_SNIFF_MODE_CMD_OPCODE
Definition: ble_id.h:127
HCI_SET_ECO_BASE_INTV_CMD_OPCODE
@ HCI_SET_ECO_BASE_INTV_CMD_OPCODE
Definition: ble_id.h:234
TASK_ID_RTLS
@ TASK_ID_RTLS
Definition: ble_id.h:604
GAPC_PATH_LOSS_THRESHOLD_REPORT_IND
@ GAPC_PATH_LOSS_THRESHOLD_REPORT_IND
Definition: ble_id.h:724
GAPC_SET_PHY_CMD
@ GAPC_SET_PHY_CMD
Definition: ble_id.h:704
GAPC_PARAM_UPDATE_REQ_IND
@ GAPC_PARAM_UPDATE_REQ_IND
Definition: ble_id.h:681
HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE
@ HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE
Definition: ble_id.h:337
HCI_LK_REQ_NEG_REPLY_CMD_OPCODE
@ HCI_LK_REQ_NEG_REPLY_CMD_OPCODE
Definition: ble_id.h:89
HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE
@ HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE
Definition: ble_id.h:326
HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE
@ HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE
Definition: ble_id.h:320
HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE
@ HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:325
GAPC_READ_REMOTE_TX_PWR_CMD
@ GAPC_READ_REMOTE_TX_PWR_CMD
Definition: ble_id.h:717
HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE
@ HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:385
HCI_AUTH_PAYL_TO_EXP_EVT_CODE
@ HCI_AUTH_PAYL_TO_EXP_EVT_CODE
Definition: ble_id.h:489
hci_vs_opcode
hci_vs_opcode
Definition: ble_id.h:539
HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE
@ HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE
Definition: ble_id.h:460
GATTC_SEND_EVT_CMD
@ GATTC_SEND_EVT_CMD
Definition: ble_id.h:829
HCI_WR_LE_HOST_SUPP_CMD_OPCODE
@ HCI_WR_LE_HOST_SUPP_CMD_OPCODE
Definition: ble_id.h:213
HCI_RD_AFH_CH_MAP_CMD_OPCODE
@ HCI_RD_AFH_CH_MAP_CMD_OPCODE
Definition: ble_id.h:256
HCI_WR_INQ_MODE_CMD_OPCODE
@ HCI_WR_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:191
GAPM_AUTO_CONN_TO_IND
@ GAPM_AUTO_CONN_TO_IND
Definition: ble_id.h:801
HCI_SYNC_TRAIN_CMP_EVT_CODE
@ HCI_SYNC_TRAIN_CMP_EVT_CODE
Definition: ble_id.h:482
HCI_VS_LE_GET_LINK_INFO_CMP_EVT_SUBCODE
@ HCI_VS_LE_GET_LINK_INFO_CMP_EVT_SUBCODE
Definition: ble_id.h:557
GAPM_SET_GDX_RANGING_PARAM_CMD
@ GAPM_SET_GDX_RANGING_PARAM_CMD
Definition: ble_id.h:804
HCI_ROLE_CHG_EVT_CODE
@ HCI_ROLE_CHG_EVT_CODE
Definition: ble_id.h:448
HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE
@ HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE
Definition: ble_id.h:208
HCI_VS_LE_UPDATE_SNIFFER_PHY_PARAM_CMD_OPCODE
@ HCI_VS_LE_UPDATE_SNIFFER_PHY_PARAM_CMD_OPCODE
Definition: ble_id.h:548
HCI_RD_REM_EXT_FEATS_CMD_OPCODE
@ HCI_RD_REM_EXT_FEATS_CMD_OPCODE
Definition: ble_id.h:100
HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE
@ HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE
Definition: ble_id.h:222
HCI_CON_REQ_EVT_CODE
@ HCI_CON_REQ_EVT_CODE
Definition: ble_id.h:434
HCI_LE_LTK_REQ_REPLY_CMD_OPCODE
@ HCI_LE_LTK_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:293
HCI_WR_LOCAL_NAME_CMD_OPCODE
@ HCI_WR_LOCAL_NAME_CMD_OPCODE
Definition: ble_id.h:152
HCI_QOS_VIOL_EVT_CODE
@ HCI_QOS_VIOL_EVT_CODE
Definition: ble_id.h:459
HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE
@ HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE
Definition: ble_id.h:425
TASK_API_ID
TASK_API_ID
Definition: ble_id.h:570
GAPC_SECURITY_IND
@ GAPC_SECURITY_IND
Definition: ble_id.h:693
GAPC_SET_DEV_INFO_CFM
@ GAPC_SET_DEV_INFO_CFM
Definition: ble_id.h:679
HCI_LE_PER_ADV_REPORT_EVT_SUBCODE
@ HCI_LE_PER_ADV_REPORT_EVT_SUBCODE
Definition: ble_id.h:511
GAPC_LE_PHY_IND
@ GAPC_LE_PHY_IND
Definition: ble_id.h:705
HCI_VS_LE_PHY_PARAM_NOTIF_EVT_SUBCODE
@ HCI_VS_LE_PHY_PARAM_NOTIF_EVT_SUBCODE
Definition: ble_id.h:562
HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE
@ HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE
Definition: ble_id.h:179
GAPM_ADDR_RENEW_TO_IND
@ GAPM_ADDR_RENEW_TO_IND
Definition: ble_id.h:800
HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE
@ HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE
Definition: ble_id.h:517
GAPC_UNKNOWN_MSG_IND
@ GAPC_UNKNOWN_MSG_IND
Definition: ble_id.h:709
HCI_PARK_STATE_CMD_OPCODE
@ HCI_PARK_STATE_CMD_OPCODE
Definition: ble_id.h:129
HCI_PIN_CODE_REQ_EVT_CODE
@ HCI_PIN_CODE_REQ_EVT_CODE
Definition: ble_id.h:452
HCI_LE_RD_SUPP_STATES_CMD_OPCODE
@ HCI_LE_RD_SUPP_STATES_CMD_OPCODE
Definition: ble_id.h:295
HCI_RETURN_LINK_KEYS_EVT_CODE
@ HCI_RETURN_LINK_KEYS_EVT_CODE
Definition: ble_id.h:451
HCI_LE_EN_ENC_CMD_OPCODE
@ HCI_LE_EN_ENC_CMD_OPCODE
Definition: ble_id.h:292
HCI_LE_RX_TEST_V1_CMD_OPCODE
@ HCI_LE_RX_TEST_V1_CMD_OPCODE
Definition: ble_id.h:296
HCI_ENH_FLUSH_CMD_OPCODE
@ HCI_ENH_FLUSH_CMD_OPCODE
Definition: ble_id.h:206
HCI_USER_PASSKEY_REQ_EVT_CODE
@ HCI_USER_PASSKEY_REQ_EVT_CODE
Definition: ble_id.h:472
HCI_VS_EVENT
@ HCI_VS_EVENT
Definition: ble_id.h:621
HCI_DBG_WR_PAR_CMD_OPCODE
@ HCI_DBG_WR_PAR_CMD_OPCODE
Definition: ble_id.h:405
HCI_LE_SET_PHY_CMD_OPCODE
@ HCI_LE_SET_PHY_CMD_OPCODE
Definition: ble_id.h:317
GAPC_RANGING_START_CMD
@ GAPC_RANGING_START_CMD
Definition: ble_id.h:725
HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE
@ HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE
Definition: ble_id.h:389
GATTC_WRITE_REQ_IND
@ GATTC_WRITE_REQ_IND
Definition: ble_id.h:834
GAPM_LIST_SET_CMD
@ GAPM_LIST_SET_CMD
Definition: ble_id.h:776
GAPM_NB_ADV_SETS_IND
@ GAPM_NB_ADV_SETS_IND
Definition: ble_id.h:789
HCI_DEL_STORED_LK_CMD_OPCODE
@ HCI_DEL_STORED_LK_CMD_OPCODE
Definition: ble_id.h:151
HCI_RD_LOOPBACK_MODE_CMD_OPCODE
@ HCI_RD_LOOPBACK_MODE_CMD_OPCODE
Definition: ble_id.h:262
GAPM_SET_IRK_CMD
@ GAPM_SET_IRK_CMD
Definition: ble_id.h:764
HCI_RD_SCAN_EN_CMD_OPCODE
@ HCI_RD_SCAN_EN_CMD_OPCODE
Definition: ble_id.h:158
GAPC_ENCRYPT_REQ_IND
@ GAPC_ENCRYPT_REQ_IND
Definition: ble_id.h:689
L2CC_LECB_SDU_SEND_CMD
@ L2CC_LECB_SDU_SEND_CMD
Definition: ble_id.h:860
HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE
@ HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE
Definition: ble_id.h:352
HCI_MAX_SLOT_CHG_EVT_CODE
@ HCI_MAX_SLOT_CHG_EVT_CODE
Definition: ble_id.h:456
HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE
@ HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE
Definition: ble_id.h:229
HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE
@ HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE
Definition: ble_id.h:409
TASK_ID_LM
@ TASK_ID_LM
Definition: ble_id.h:583
HCI_SET_MWS_SIGNALING_CMD_OPCODE
@ HCI_SET_MWS_SIGNALING_CMD_OPCODE
Definition: ble_id.h:216
SDK_COMMON_TIMEOUT_TIMER_8
@ SDK_COMMON_TIMEOUT_TIMER_8
Definition: ble_id.h:639
HCI_RD_AUTH_PAYL_TO_CMD_OPCODE
@ HCI_RD_AUTH_PAYL_TO_CMD_OPCODE
Definition: ble_id.h:227
HCI_INQ_CMD_OPCODE
@ HCI_INQ_CMD_OPCODE
Definition: ble_id.h:79
GATTC_REG_TO_PEER_EVT_CMD
@ GATTC_REG_TO_PEER_EVT_CMD
Definition: ble_id.h:828
HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE
@ HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE
Definition: ble_id.h:512
TASK_ID_LLM
@ TASK_ID_LLM
Definition: ble_id.h:575
HCI_CHG_CON_LK_CMD_OPCODE
@ HCI_CHG_CON_LK_CMD_OPCODE
Definition: ble_id.h:95
GAPC_ENCRYPT_IND
@ GAPC_ENCRYPT_IND
Definition: ble_id.h:691
HCI_LE_TIME_SYNC_EN_CMD_OPCODE
@ HCI_LE_TIME_SYNC_EN_CMD_OPCODE
Definition: ble_id.h:394
GAPM_ACTIVITY_STOP_CMD
@ GAPM_ACTIVITY_STOP_CMD
Definition: ble_id.h:780
HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE
@ HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE
Definition: ble_id.h:224
GAPM_ACTIVITY_STOPPED_IND
@ GAPM_ACTIVITY_STOPPED_IND
Definition: ble_id.h:783
GATTC_CLIENT_RTX_IND
@ GATTC_CLIENT_RTX_IND
Definition: ble_id.h:842
HCI_DBG_BLE_REG_RD_CMD_OPCODE
@ HCI_DBG_BLE_REG_RD_CMD_OPCODE
Definition: ble_id.h:417
GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD
@ GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD
Definition: ble_id.h:718
HCI_EVENT
@ HCI_EVENT
Definition: ble_id.h:617
GAPC_CONNECTION_CFM
@ GAPC_CONNECTION_CFM
Definition: ble_id.h:668
GAPC_CTE_REQ_CTRL_CMD
@ GAPC_CTE_REQ_CTRL_CMD
Definition: ble_id.h:713
HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE
@ HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE
Definition: ble_id.h:358
HCI_PER_INQ_MODE_CMD_OPCODE
@ HCI_PER_INQ_MODE_CMD_OPCODE
Definition: ble_id.h:81
HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE
@ HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE
Definition: ble_id.h:171
HCI_SET_RES_LT_ADDR_CMD_OPCODE
@ HCI_SET_RES_LT_ADDR_CMD_OPCODE
Definition: ble_id.h:220
GATTC_DISC_CHAR_DESC_IND
@ GATTC_DISC_CHAR_DESC_IND
Definition: ble_id.h:820
HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE
@ HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE
Definition: ble_id.h:363
GAPM_GEN_RAND_NB_CMD
@ GAPM_GEN_RAND_NB_CMD
Definition: ble_id.h:756
HCI_RD_EXT_PAGE_TO_CMD_OPCODE
@ HCI_RD_EXT_PAGE_TO_CMD_OPCODE
Definition: ble_id.h:230
HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE
@ HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE
Definition: ble_id.h:211
HCI_RD_CURR_IAC_LAP_CMD_OPCODE
@ HCI_RD_CURR_IAC_LAP_CMD_OPCODE
Definition: ble_id.h:185
GATTC_SDP_SVC_DISC_CMD
@ GATTC_SDP_SVC_DISC_CMD
Definition: ble_id.h:838
HCI_WR_CURR_IAC_LAP_CMD_OPCODE
@ HCI_WR_CURR_IAC_LAP_CMD_OPCODE
Definition: ble_id.h:186
GAPC_SET_PREF_SLAVE_LATENCY_CMD
@ GAPC_SET_PREF_SLAVE_LATENCY_CMD
Definition: ble_id.h:707
HCI_LE_PHY_UPD_CMP_EVT_SUBCODE
@ HCI_LE_PHY_UPD_CMP_EVT_SUBCODE
Definition: ble_id.h:508
HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE
@ HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE
Definition: ble_id.h:195
l2cc_msg_id
l2cc_msg_id
GATTC_TASK Message ID.
Definition: ble_id.h:850
HCI_CMD_CMP_EVT_CODE
@ HCI_CMD_CMP_EVT_CODE
Definition: ble_id.h:444
HCI_LE_RD_CHNL_MAP_CMD_OPCODE
@ HCI_LE_RD_CHNL_MAP_CMD_OPCODE
Definition: ble_id.h:288
HCI_LE_ENC_CMD_OPCODE
@ HCI_LE_ENC_CMD_OPCODE
Definition: ble_id.h:290
GAPC_CONNECTION_REQ_IND
@ GAPC_CONNECTION_REQ_IND
Definition: ble_id.h:667
HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE
@ HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE
Definition: ble_id.h:515
HCI_VS_LE_SNIFFER_DISC_CMP_EVT_SUBCODE
@ HCI_VS_LE_SNIFFER_DISC_CMP_EVT_SUBCODE
Definition: ble_id.h:558
HCI_RD_NB_SUPP_IAC_CMD_OPCODE
@ HCI_RD_NB_SUPP_IAC_CMD_OPCODE
Definition: ble_id.h:184
HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE
@ HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE
Definition: ble_id.h:366
HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
@ HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE
Definition: ble_id.h:303
GAPC_DISCONNECT_IND
@ GAPC_DISCONNECT_IND
Definition: ble_id.h:669
HCI_LE_ISO_RX_TEST_CMD_OPCODE
@ HCI_LE_ISO_RX_TEST_CMD_OPCODE
Definition: ble_id.h:380
HCI_RD_LMP_HDL_CMD_OPCODE
@ HCI_RD_LMP_HDL_CMD_OPCODE
Definition: ble_id.h:103
TASK_ID_AHI
@ TASK_ID_AHI
Definition: ble_id.h:600
HCI_DBG_RD_MEM_INFO_CMD_OPCODE
@ HCI_DBG_RD_MEM_INFO_CMD_OPCODE
Definition: ble_id.h:412
HCI_WR_AUTH_PAYL_TO_CMD_OPCODE
@ HCI_WR_AUTH_PAYL_TO_CMD_OPCODE
Definition: ble_id.h:228
HCI_REJECT_CON_REQ_CMD_OPCODE
@ HCI_REJECT_CON_REQ_CMD_OPCODE
Definition: ble_id.h:87
HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE
@ HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE
Definition: ble_id.h:123
HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE
@ HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE
Definition: ble_id.h:192
HCI_AUTH_REQ_CMD_OPCODE
@ HCI_AUTH_REQ_CMD_OPCODE
Definition: ble_id.h:93
HCI_LE_SET_HOST_FEATURE_CMD_OPCODE
@ HCI_LE_SET_HOST_FEATURE_CMD_OPCODE
Definition: ble_id.h:383
HCI_LE_RD_BUF_SIZE_CMD_OPCODE
@ HCI_LE_RD_BUF_SIZE_CMD_OPCODE
Definition: ble_id.h:270
GAPM_PUB_KEY_IND
@ GAPM_PUB_KEY_IND
Definition: ble_id.h:774
GAPC_KEY_PRESS_NOTIFICATION_IND
@ GAPC_KEY_PRESS_NOTIFICATION_IND
Definition: ble_id.h:703
GAPC_RANGING_CMP_IND
@ GAPC_RANGING_CMP_IND
Definition: ble_id.h:728
HCI_SNIFF_SUB_CMD_OPCODE
@ HCI_SNIFF_SUB_CMD_OPCODE
Definition: ble_id.h:139
HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE
@ HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE
Definition: ble_id.h:377
GAPM_DEV_BDADDR_IND
@ GAPM_DEV_BDADDR_IND
Definition: ble_id.h:747
HCI_DBG_LLCP_DISCARD_CMD_OPCODE
@ HCI_DBG_LLCP_DISCARD_CMD_OPCODE
Definition: ble_id.h:420
GAPC_SIGN_COUNTER_IND
@ GAPC_SIGN_COUNTER_IND
Definition: ble_id.h:694
L2CC_LECB_ADD_CMD
@ L2CC_LECB_ADD_CMD
Definition: ble_id.h:858