Macros
Private Macro
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

## Macros
#define | LL_AON_GPIO_MODE_INPUT_POS ((uint32_t)0x0U)
#define | LL_AON_GPIO_MODE_OUTPUT_POS ((uint32_t)0x1U)
#define | LL_AON_GPIO_STRENGTH_DS0_MASK ((uint32_t)0x10U)
#define | LL_AON_GPIO_STRENGTH_DS1_MASK ((uint32_t)0x01U)
#define | LL_AON_GPIO_STRENGTH_DS0_POS ((uint32_t)0x04U)
#define | LL_AON_GPIO_STRENGTH_DS1_POS ((uint32_t)0x00U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_MODE_INPUT_POS

#define LL_AON_GPIO_MODE_INPUT_POS ((uint32_t)0x0U)

Input mode bit position AON_GPIO_LL_EC_MODE

Definition at line 132 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_MODE_OUTPUT_POS

#define LL_AON_GPIO_MODE_OUTPUT_POS ((uint32_t)0x1U)

Output mode bit position AON_GPIO_LL_EC_MODE

Definition at line 133 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_DS0_MASK

#define LL_AON_GPIO_STRENGTH_DS0_MASK ((uint32_t)0x10U)

DS0 mask in AON_GPIO_LL_EC_STRENGTH

Definition at line 134 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_DS0_POS

#define LL_AON_GPIO_STRENGTH_DS0_POS ((uint32_t)0x04U)

DS0 bit position in AON_GPIO_LL_EC_STRENGTH

Definition at line 136 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_DS1_MASK

#define LL_AON_GPIO_STRENGTH_DS1_MASK ((uint32_t)0x01U)

DS1 mask in AON_GPIO_LL_EC_STRENGTH

Definition at line 135 of file ll_aon_gpio.h.

## ◆ LL_AON_GPIO_STRENGTH_DS1_POS

#define LL_AON_GPIO_STRENGTH_DS1_POS ((uint32_t)0x00U)

DS1 bit position in AON_GPIO_LL_EC_STRENGTH

Definition at line 137 of file ll_aon_gpio.h.