Functions
Initialization and de-initialization functions
Peripheral Driver » LL Driver » MSIO » Functions

## Functions
void | ll_msio_init (msio_pad_t MSIOx, const ll_msio_init_t *p_msio_init)
| Initialize MSIO registers according to the specified. parameters in p_msio_init. More...

## Detailed Description

## Function Documentation

## ◆ ll_msio_init()

void ll_msio_init | ( | msio_pad_t | MSIOx,
|  | const ll_msio_init_t * | p_msio_init
| ) |  |

Initialize MSIO registers according to the specified. parameters in p_msio_init.

Parameters

  MSIOx | MSIO instance.
  p_msio_init | Pointer to a ll_msio_init_t structure that contains the configuration information for the specified MSIO peripheral.

Return values

  None |