Modules | Macros
COMP Exported Constants
Peripheral Driver » LL Driver » COMP » Defines

## Modules
| COMP INPUT SOURCE
| COMP REF SOURCE
| COMP

## Macros
#define | LL_COMP_RES_DEGENERATION_POSITIVE (1UL << AON_PMU_COMP_REG_1_CHANNEL_POSITIVE_RES_DEGENERATION_Pos )
#define | LL_COMP_RES_DEGENERATION_NEGATIVE (1UL << AON_PMU_COMP_REG_1_CHANNEL_NEGATIVE_RES_DEGENERATION_Pos )

## Detailed Description

## Macro Definition Documentation

## ◆ LL_COMP_RES_DEGENERATION_NEGATIVE

#define LL_COMP_RES_DEGENERATION_NEGATIVE (1UL << AON_PMU_COMP_REG_1_CHANNEL_NEGATIVE_RES_DEGENERATION_Pos )

Set negative side of calibration for the comparator

Definition at line 158 of file ll_comp.h.

## ◆ LL_COMP_RES_DEGENERATION_POSITIVE

#define LL_COMP_RES_DEGENERATION_POSITIVE (1UL << AON_PMU_COMP_REG_1_CHANNEL_POSITIVE_RES_DEGENERATION_Pos )

Set positive side of calibration for the comparator

Definition at line 157 of file ll_comp.h.