Modules | Macros
CGC Exported Constants
Peripheral Driver » LL Driver » CGC » Defines

## Modules
| Block0 Clock During WFI
| Block1 Clock During WFI
| Force Clock OFF
| Force Clock OFF
| Force Clock OFF
| Low Power Feature
| Turn the peripherals off during WFI/WFE
| Individual block's clock control inside security system
| Specify the default system clock when the system is initialized

## Macros
#define | LL_CGC_MCU_PERIPH_CG_LP ((uint32_t)0x00000D3BUL)
#define | LL_CGC_MCU_MISC_CLK_DEFAULT ((uint32_t)0x00000008U)
#define | LL_CGC_MCU_MISC_CLK ((uint32_t)0x0000000CU)
#define | LL_CGC_MCU_MISC_DMA_CLK ((uint32_t)0x00000008U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_MCU_MISC_CLK

#define LL_CGC_MCU_MISC_CLK ((uint32_t)0x0000000CU)

Hclk for msic all clock

Definition at line 186 of file ll_cgc.h.

## ◆ LL_CGC_MCU_MISC_CLK_DEFAULT

#define LL_CGC_MCU_MISC_CLK_DEFAULT ((uint32_t)0x00000008U)

Hclk for msic default clock

Definition at line 184 of file ll_cgc.h.

## ◆ LL_CGC_MCU_MISC_DMA_CLK

#define LL_CGC_MCU_MISC_DMA_CLK ((uint32_t)0x00000008U)

Hclk for msic dma clock

Definition at line 188 of file ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP

#define LL_CGC_MCU_PERIPH_CG_LP ((uint32_t)0x00000D3BUL)

All Low Power Feature

Definition at line 151 of file ll_cgc.h.