Macros | Functions
ll_cgc.h File Reference

Header file containing functions prototypes of CGC LL library. More...

`#include "gr5405.h"`

Go to the source code of this file.

## Macros
#define | LL_CGC_WFI_SECU_HCLK MCU_SUB_WFI_SECU_HCLK
#define | LL_CGC_WFI_HTB_HCLK MCU_SUB_WFI_HTB_HCLK
#define | LL_CGC_WFI_ROM_HCLK MCU_SUB_WFI_ROM_HCLK
#define | LL_CGC_WFI_SNSADC_HCLK MCU_SUB_WFI_SNSADC_HCLK
#define | LL_CGC_WFI_GPIO_HCLK MCU_SUB_WFI_GPIO_HCLK
#define | LL_CGC_WFI_BLE_BRG_HCLK MCU_SUB_WFI_BLE_BRG_HCLK
#define | LL_CGC_WFI_APB_SUB_HCLK MCU_SUB_WFI_APB_SUB_HCLK
#define | LL_CGC_WFI_SERIAL_HCLK MCU_SUB_WFI_SERIAL_HCLK
#define | LL_CGC_WFI_ALL_HCLK0 ((uint32_t)0x000007FFU)
#define | LL_CGC_WFI_AON_MCUSUB_HCLK MCU_SUB_WFI_AON_MCUSUB_HCLK
#define | LL_CGC_WFI_XF_XQSPI_HCLK MCU_SUB_WFI_XF_XQSPI_HCLK
#define | LL_CGC_WFI_SRAM_HCLK MCU_SUB_WFI_SRAM_HCLK
#define | LL_CGC_WFI_ALL_HCLK1 ((uint32_t)0x00000007U)
#define | LL_CGC_FRC_SECU_HCLK MCU_SUB_FORCE_SECU_HCLK
#define | LL_CGC_FRC_HTB_HCLK MCU_SUB_FORCE_HTB_HCLK
#define | LL_CGC_FRC_ROM_HCLK MCU_SUB_FORCE_ROM_HCLK
#define | LL_CGC_FRC_SNSADC_HCLK MCU_SUB_FORCE_SNSADC_HCLK
#define | LL_CGC_FRC_GPIO_HCLK MCU_SUB_FORCE_GPIO_HCLK
#define | LL_CGC_FRC_BLE_BRG_HCLK MCU_SUB_FORCE_BLE_BRG_HCLK
#define | LL_CGC_FRC_APB_SUB_HCLK MCU_SUB_FORCE_APB_SUB_HCLK
#define | LL_CGC_FRC_SERIAL_HCLK MCU_SUB_FORCE_SERIAL_HCLK
#define | LL_CGC_FRC_ALL_HCLK0 ((uint32_t)0x00000775U)
#define | LL_CGC_FRC_XF_XQSPI_HCLK MCU_SUB_FORCE_XF_XQSPI_HCLK
#define | LL_CGC_FRC_SRAM_HCLK MCU_SUB_FORCE_SRAM_HCLK
#define | LL_CGC_FRC_ALL_HCLK1 ((uint32_t)0x00060000U)
#define | LL_CGC_FRC_UART0_PCLK MCU_SUB_FORCE_UART0_PCLK
#define | LL_CGC_FRC_UART1_PCLK MCU_SUB_FORCE_UART1_PCLK
#define | LL_CGC_FRC_I2C0_PCLK MCU_SUB_FORCE_I2C0_PCLK
#define | LL_CGC_FRC_I2C1_PCLK MCU_SUB_FORCE_I2C1_PCLK
#define | LL_CGC_FRC_SPI_M_PCLK MCU_SUB_FORCE_SPI_M_PCLK
#define | LL_CGC_FRC_SPI_S_PCLK MCU_SUB_FORCE_SPI_S_PCLK
#define | LL_CGC_FRC_PWM_0_PCLK MCU_SUB_FORCE_PWM_0_PCLK
#define | LL_CGC_FRC_PWM_1_PCLK MCU_SUB_FORCE_PWM_1_PCLK
#define | LL_CGC_FRC_SERIALS_HCLK2 ((uint32_t)0x30063005UL)
#define | LL_CGC_FRC_ALL_HCLK2 ((uint32_t)0x30063005UL)
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_ASYNC_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_SYNC_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN MCU_SUB_PERIPH_CG_LP_EN_AHB_BUS_LP_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_PCLK_EN
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_SCLK_EN
#define | LL_CGC_MCU_PERIPH_CG_LP ((uint32_t)0x00000D3BUL)
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x00003CC3UL)
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x00003CC3UL)
#define | LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_FORCE_OFF
#define | LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_SLP_OFF
#define | LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_FORCE_OFF
#define | LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_SLP_OFF
#define | LL_CGC_MCU_SECU_FRC_OFF_HCLK ((uint32_t)0x00001400U)
#define | LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK ((uint32_t)0x00002800U)
#define | LL_CGC_MCU_SECU_FRC_OFF_ALL
#define | LL_CGC_MCU_MISC_CLK_DEFAULT ((uint32_t)0x00000008U)
#define | LL_CGC_MCU_MISC_CLK ((uint32_t)0x0000000CU)
#define | LL_CGC_MCU_MISC_DMA_CLK ((uint32_t)0x00000008U)
#define | LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK0
#define | LL_CGC_MCU_SUBSYS_DEFAULT_WFI_CLK1
#define | LL_CGC_MCU_SUBSYS_DEFAULT_CLK
#define | LL_CGC_MCU_PERIPH_CG_DEFAULT
#define | LL_CGC_MCU_PERIPH_SLP_CG_DEFAULT
#define | CGC_CLOCK_ENABLE (1)
#define | CGC_CLOCK_DISABLE (0)
#define | BIT_SEGMENT_VALUE BIT_ADDR

## Functions
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_0 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: Security/SIM/HTB/PWM/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_0 (void)
| Return to clock blocks that is turned off during WFI.(Include: Security/SIM/HTB/PWM/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_1 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_1 (void)
| Return to clock blocks that is turned off during WFI.(Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_2 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: SECU_DIV4/XQSPI_DIV4) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_2 (void)
| Return to clock blocks that is turned off during WFI.(Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_3 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: UART/DSPI.I2C/QSPI.etc) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_3 (void)
| Return to clock blocks that is turned off during WFI.(Include: UART/DSPI.I2C/QSPI.etc) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_4 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_4 (void)
| Return to clock blocks that is turned off during WFI.(Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_0 (uint32_t clk_mask)
| Some peripherals force turn off clock. (Include: Security/SIM/HTB/PWM/ROM/SNSADC/GPIO/ DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_0 (void)
| Return to clock blocks that was forcibly closed.(Include: Security/SIM/HTB/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_1 (uint32_t clk_mask)
| Some peripherals force turn off clock. (Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_1 (void)
| Return to clock blocks that was forcibly closed.(Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_2 (uint32_t clk_mask)
| Some peripherals force turn off clock. (Include: UART0_HCLK/UART1_HCLK/UART2_HCLK/UART3_HCLK/UART4_HCLK/UART5_HCLK/ I2C0_HCLK/I2C1_HCLK/SPIM_HCLK/SPIS_HCLK/QSPI0_HCLK/QSPI1_HCLK/I2S_HCLK/SECU_DIV4_PCLK/XQSPI_DIV4_PCLK/PWM0/PWM1) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_2 (void)
| Return to clock blocks that was forcibly closed.(Include: UART0_HCLK/UART1_HCLK/UART2_HCLK/UART3_HCLK/UART4_HCLK/UART5_HCLK/ I2C0_HCLK/I2C1_HCLK/SPIM_HCLK/SPIS_HCLK/QSPI0_HCLK/QSPI1_HCLK/I2S_HCLK/SECU_DIV4_PCLK/XQSPI_DIV4_PCLK/PWM0/PWM1) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_3 (uint32_t clk_mask)
| Some peripherals automatic turn off clock. (Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_3 (void)
| Return to clock blocks that is turned off.(Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_secu_hclk (void)
| Enable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_secu_hclk (void)
| Disable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_secu_hclk (void)
| Indicate whether the security blocks(including AES, PKC, Present, HMAC) automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_sim_hclk (void)
| Enable SIM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_sim_hclk (void)
| Disable SIM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_sim_hclk (void)
| Indicate whether the SIM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_htb_hclk (void)
| Enable Hopping Table automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_htb_hclk (void)
| Disable Hopping Table automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_htb_hclk (void)
| Indicate whether the Hopping Table automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_pwm_hclk (void)
| Enable PWM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_pwm_hclk (void)
| Disable PWM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_pwm_hclk (void)
| Indicate whether the PWM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_rom_hclk (void)
| Enable ROM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_rom_hclk (void)
| Disable ROM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_rom_hclk (void)
| Indicate whether the ROM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_snsadc_hclk (void)
| Enable SNSADC automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_snsadc_hclk (void)
| Disable SNSADC automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_snsadc_hclk (void)
| Indicate whether the SNSADC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_gpio_hclk (void)
| Enable GPIO automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_gpio_hclk (void)
| Disable GPIO automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_gpio_hclk (void)
| Indicate whether the GPIO automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_dma_hclk (void)
| Enable DMA automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_dma_hclk (void)
| Disable DMA automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_dma_hclk (void)
| Indicate whether the DMA automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_ble_brg_hclk (void)
| Enable BLE Bridge automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_ble_brg_hclk (void)
| Disable BLE Bridge automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_ble_brg_hclk (void)
| Indicate whether the BLE Bridge automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_apb_sub_hclk (void)
| Enable APB Subsystem automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_apb_sub_hclk (void)
| Disable APB Subsystem automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_apb_sub_hclk (void)
| Indicate whether the APB Subsystem automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_serial_hclk (void)
| Enable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_serial_hclk (void)
| Disable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_serial_hclk (void)
| Indicate whether the serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_aon_mcusub_hclk (void)
| Enable AON_MUCSUB automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_aon_mcusub_hclk (void)
| Disable AON_MUCSUB automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk (void)
| Indicate whether the AON_MUCSUB automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_xqspi_hclk (void)
| Enable XQSPI automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_xqspi_hclk (void)
| Disable XQSPI automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_xqspi_hclk (void)
| Indicate whether the XQSPI automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_sram_hclk (void)
| Enable SRAM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_sram_hclk (void)
| Disable SRAM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_sram_hclk (void)
| Indicate whether the SRAM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_secu_div4_hclk (void)
| Enable security blocks automatic turn off div4 clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_secu_div4_hclk (void)
| Disable security blocks automatic turn off div4 clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_secu_div4_hclk (void)
| Indicate whether the security blocks automatic turn off div4 clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_xqspi_div4_hclk (void)
| Enable XQSPI automatic turn off div4 clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_xqspi_div4_hclk (void)
| Disable XQSPI automatic turn off div4 clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk (void)
| Indicate whether the XQSPI automatic turn off div4 clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_secu_hclk (void)
| Enabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC). More...
__STATIC_INLINE void | ll_cgc_disable_force_off_secu_hclk (void)
| Disabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC). More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_secu_hclk (void)
| Indicate whether the clock for security blocks(including AES, PKC, Present, HMAC) is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_htb_hclk (void)
| Enabling force to turn off the clock for Hopping Table. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_htb_hclk (void)
| Disabling force to turn off the clock for Hopping Table. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_htb_hclk (void)
| Indicate whether the clock for Hopping Table is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_rom_hclk (void)
| Enabling force to turn off the clock for ROM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_rom_hclk (void)
| Disabling force to turn off the clock for ROM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_rom_hclk (void)
| Indicate whether the clock for ROM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_snsadc_hclk (void)
| Enabling force to turn off the clock for SNSADC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_snsadc_hclk (void)
| Disabling force to turn off the clock for SNSADC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_snsadc_hclk (void)
| Indicate whether the clock for SNSADC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_gpio_hclk (void)
| Enabling force to turn off the clock for GPIO. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_gpio_hclk (void)
| Disabling force to turn off the clock for GPIO. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_gpio_hclk (void)
| Indicate whether the clock for GPIO is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_ble_brg_hclk (void)
| Enabling force to turn off the clock for BLE Bridge. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_ble_brg_hclk (void)
| Disabling force to turn off the clock for BLE Bridge. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_ble_brg_hclk (void)
| Indicate whether the clock for BLE Bridge is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_apb_sub_hclk (void)
| Enabling force to turn off the clock for APB Subsystem. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_apb_sub_hclk (void)
| Disabling force to turn off the clock for APB Subsystem. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_apb_sub_hclk (void)
| Indicate whether the clock for APB Subsystem is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_serial_hclk (void)
| Enabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI). More...
__STATIC_INLINE void | ll_cgc_disable_force_off_serial_hclk (void)
| Disabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI). More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_serial_hclk (void)
| Indicate whether the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI) is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_aon_mcusub_hclk (void)
| Enabling force to turn off the clock for AON_MUCSUB. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_aon_mcusub_hclk (void)
| Disabling force to turn off the clock for AON_MUCSUB. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_aon_mcusub_hclk (void)
| Indicate whether the clock for AON_MUCSUB is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xqspi_hclk (void)
| Enabling force to turn off the clock for XQSPI. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xqspi_hclk (void)
| Disabling force to turn off the clock for XQSPI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xqspi_hclk (void)
| Indicate whether the clock for XQSPI is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_sram_hclk (void)
| Enabling force to turn off the clock for SRAM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_sram_hclk (void)
| Disabling force to turn off the clock for SRAM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_sram_hclk (void)
| Indicate whether the clock for SRAM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart0_hclk (void)
| Enabling force to turn off the clock for UART0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart0_hclk (void)
| Disabling force to turn off the clock for UART0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart0_hclk (void)
| Indicate whether the clock for UART0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart1_hclk (void)
| Enabling force to turn off the clock for UART1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart1_hclk (void)
| Disabling force to turn off the clock for UART1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart1_hclk (void)
| Indicate whether the clock for UART1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart2_hclk (void)
| Enabling force to turn off the clock for UART2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart2_hclk (void)
| Disabling force to turn off the clock for UART2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart2_hclk (void)
| Indicate whether the clock for UART2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart3_hclk (void)
| Enabling force to turn off the clock for UART3. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart3_hclk (void)
| Disabling force to turn off the clock for UART3. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart3_hclk (void)
| Indicate whether the clock for UART3 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart4_hclk (void)
| Enabling force to turn off the clock for UART4. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart4_hclk (void)
| Disabling force to turn off the clock for UART4. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart4_hclk (void)
| Indicate whether the clock for UART4 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart5_hclk (void)
| Enabling force to turn off the clock for UART5. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart5_hclk (void)
| Disabling force to turn off the clock for UART5. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart5_hclk (void)
| Indicate whether the clock for UART5 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c0_hclk (void)
| Enabling force to turn off the clock for I2C0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c0_hclk (void)
| Disabling force to turn off the clock for I2C0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c0_hclk (void)
| Indicate whether the clock for I2C0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c1_hclk (void)
| Enabling force to turn off the clock for I2C1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c1_hclk (void)
| Disabling force to turn off the clock for I2C1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c1_hclk (void)
| Indicate whether the clock for I2C1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c2_hclk (void)
| Enabling force to turn off the clock for I2C2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c2_hclk (void)
| Disabling force to turn off the clock for I2C2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c2_hclk (void)
| Indicate whether the clock for I2C2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c3_hclk (void)
| Enabling force to turn off the clock for I2C3. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c3_hclk (void)
| Disabling force to turn off the clock for I2C3. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c3_hclk (void)
| Indicate whether the clock for I2C3 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c4_hclk (void)
| Enabling force to turn off the clock for I2C4. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c4_hclk (void)
| Disabling force to turn off the clock for I2C4. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c4_hclk (void)
| Indicate whether the clock for I2C4 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c5_hclk (void)
| Enabling force to turn off the clock for I2C5. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c5_hclk (void)
| Disabling force to turn off the clock for I2C5. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c5_hclk (void)
| Indicate whether the clock for I2C5 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_spim_hclk (void)
| Enabling force to turn off the clock for SPIM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_spim_hclk (void)
| Disabling force to turn off the clock for SPIM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_spim_hclk (void)
| Indicate whether the clock for SPIM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_spis_hclk (void)
| Enabling force to turn off the clock for SPIS. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_spis_hclk (void)
| Disabling force to turn off the clock for SPIS. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_spis_hclk (void)
| Indicate whether the clock for SPIS is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi0_hclk (void)
| Enabling force to turn off the clock for QSPI0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi0_hclk (void)
| Disabling force to turn off the clock for QSPI0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi0_hclk (void)
| Indicate whether the clock for QSPI0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi1_hclk (void)
| Enabling force to turn off the clock for QSPI1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi1_hclk (void)
| Disabling force to turn off the clock for QSPI1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi1_hclk (void)
| Indicate whether the clock for QSPI1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi2_hclk (void)
| Enabling force to turn off the clock for QSPI2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi2_hclk (void)
| Disabling force to turn off the clock for QSPI2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi2_hclk (void)
| Indicate whether the clock for QSPI2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2s_m_hclk (void)
| Enabling force to turn off the clock for I2S master. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2s_m_hclk (void)
| Disabling force to turn off the clock for I2S master. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2s_m_hclk (void)
| Indicate whether the clock for I2S master is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2s_s_p_hclk (void)
| Enabling force to turn off the clock for I2S slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2s_s_p_hclk (void)
| Disabling force to turn off the clock for I2S slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2s_s_p_hclk (void)
| Indicate whether the clock for I2S slave is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dspi_hclk (void)
| Enabling force to turn off the clock for DSPI slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dspi_hclk (void)
| Disabling force to turn off the clock for DSPI slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dspi_hclk (void)
| Indicate whether the clock for DSPI is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pdm_hclk (void)
| Enabling force to turn off the clock for PDM slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pdm_hclk (void)
| Disabling force to turn off the clock for PDM slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pdm_hclk (void)
| Indicate whether the clock for PDM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_secu_div4_pclk (void)
| Enabling force to turn off the div4 clock for security blocks. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_secu_div4_pclk (void)
| Disabling force to turn off the div4 clock for security blocks. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_secu_div4_pclk (void)
| Indicate whether the div4 clock for security blocks is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xf_xqspi_div4_pclk (void)
| Enabling force to turn off the div4 clock for xf qspi blocks. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xf_xqspi_div4_pclk (void)
| Disabling force to turn off the div4 clock for xf qspi blocks. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xf_xqspi_div4_pclk (void)
| Indicate whether the div4 clock for xf qspi blocks is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pwm0_hclk (void)
| Enabling force to turn off the clock for PWM0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pwm0_hclk (void)
| Disabling force to turn off the clock for PWM0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pwm0_hclk (void)
| Indicate whether the clock for PWM0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pwm1_hclk (void)
| Enabling force to turn off the clock for PWM1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pwm1_hclk (void)
| Disabling force to turn off the clock for PWM1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pwm1_hclk (void)
| Indicate whether the clock for PWM1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_vttbl_hclk (void)
| Enabling force to turn off the clock for VTTBL. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_vttbl_hclk (void)
| Disabling force to turn off the clock for VTTBL. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_vttbl_hclk (void)
| Indicate whether the clock for VTTBL is forced to close. More...
__STATIC_INLINE void | ll_cgc_set_mcu_periph_low_power (uint32_t clk_mask)
| Some peripherals has low power feature. (Include: UART/I2S/SPIM/SPIS/I2C/AHB BUS) More...
__STATIC_INLINE uint32_t | ll_cgc_get_mcu_periph_low_power (void)
| Return to clock blocks that has low power feature. (Include: UART/I2S/SPIM/SPIS/I2C/AHB BUS) More...
__STATIC_INLINE void | ll_cgc_enable_uart_sclk_low_power (void)
| Enable uart sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_uart_sclk_low_power (void)
| Disable uart sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart_sclk_low_power (void)
| Indicate whether the uart sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart_pclk_low_power (void)
| Enable uart pclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_uart_pclk_low_power (void)
| Disable uart pclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart_pclk_low_power (void)
| Indicate whether the uart pclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_low_power (void)
| Enable i2s low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_low_power (void)
| Disable i2s low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_low_power (void)
| Indicate whether the i2s low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spim_sclk_low_power (void)
| Enable spim sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_spim_sclk_low_power (void)
| Disable spim sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spim_sclk_low_power (void)
| Indicate whether the spim sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spis_sclk_low_power (void)
| Enable spis sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_spis_sclk_low_power (void)
| Disable spis sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spis_sclk_low_power (void)
| Indicate whether the spis sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c_sclk_low_power (void)
| Enable i2c sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_i2c_sclk_low_power (void)
| Disable i2c sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c_sclk_low_power (void)
| Indicate whether the i2c sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb_bus_low_power (void)
| Enable ahb bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb_bus_low_power (void)
| Disable ahb bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb_bus_low_power (void)
| Indicate whether the ahb bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim_low_power (void)
| Enable QSPIM low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_qspim_low_power (void)
| Disable QSPIM low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim_low_power (void)
| Indicate whether the QSPIM low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb2apb_sync_bus_low_power (void)
| Enable AHB2APB bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb2apb_sync_bus_low_power (void)
| Disable AHB2APB bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb2apb_sync_bus_low_power (void)
| Indicate whether the AHB2APB bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb2apb_async_bus_low_power (void)
| Enable ahb bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb2apb_async_bus_low_power (void)
| Disable ahb bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb2apb_async_bus_low_power (void)
| Indicate whether the ahb bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart0_slp_wfi (void)
| Enable turn UART0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart0_slp_wfi (void)
| Disable turn UART0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart0_slp_wfi (void)
| Indicate whether turn UART0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart1_slp_wfi (void)
| Enable turn UART1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart1_slp_wfi (void)
| Disable turn UART1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart1_slp_wfi (void)
| Indicate whether turn UART1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart2_slp_wfi (void)
| Enable turn UART2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart2_slp_wfi (void)
| Disable turn UART2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart2_slp_wfi (void)
| Indicate whether turn UART2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart3_slp_wfi (void)
| Enable turn UART3 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart3_slp_wfi (void)
| Disable turn UART3 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart3_slp_wfi (void)
| Indicate whether turn UART3 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart4_slp_wfi (void)
| Enable turn UART4 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart4_slp_wfi (void)
| Disable turn UART4 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart4_slp_wfi (void)
| Indicate whether turn UART4 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart5_slp_wfi (void)
| Enable turn UART5 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart5_slp_wfi (void)
| Disable turn UART5 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart5_slp_wfi (void)
| Indicate whether turn UART5 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c0_slp_wfi (void)
| Enable turn I2C0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c0_slp_wfi (void)
| Disable turn I2C0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c0_slp_wfi (void)
| Indicate whether turn I2C0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c1_slp_wfi (void)
| Enable turn I2C1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c1_slp_wfi (void)
| Disable turn I2C1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c1_slp_wfi (void)
| Indicate whether turn I2C1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c2_slp_wfi (void)
| Enable turn I2C2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c2_slp_wfi (void)
| Disable turn I2C2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c2_slp_wfi (void)
| Indicate whether turn I2C2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c3_slp_wfi (void)
| Enable turn I2C3 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c3_slp_wfi (void)
| Disable turn I2C3 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c3_slp_wfi (void)
| Indicate whether turn I2C3 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c4_slp_wfi (void)
| Enable turn I2C4 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c4_slp_wfi (void)
| Disable turn I2C4 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c4_slp_wfi (void)
| Indicate whether turn I2C4 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c5_slp_wfi (void)
| Enable turn I2C5 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c5_slp_wfi (void)
| Disable turn I2C5 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c5_slp_wfi (void)
| Indicate whether turn I2C5 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_m_slp_wfi (void)
| Enable turn I2S_M off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_m_slp_wfi (void)
| Disable turn I2S_M off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_m_slp_wfi (void)
| Indicate whether turn I2S_M off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_s_slp_wfi (void)
| Enable turn I2S_S off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_s_slp_wfi (void)
| Disable turn I2S_S off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_s_slp_wfi (void)
| Indicate whether turn I2S_S off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spi_m_slp_wfi (void)
| Enable turn SPI_M off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_spi_m_slp_wfi (void)
| Disable turn SPI_M off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spi_m_slp_wfi (void)
| Indicate whether turn SPI_M off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spi_s_slp_wfi (void)
| Enable turn SPI_S off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_spi_s_slp_wfi (void)
| Disable turn SPI_S off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spi_s_slp_wfi (void)
| Indicate whether turn SPI_S off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pwm0_slp_wfi (void)
| Enable turn pwm0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pwm0_slp_wfi (void)
| Disable turn pwm0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pwm0_slp_wfi (void)
| Indicate whether turn pwm0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pwm1_slp_wfi (void)
| Enable turn pwm1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pwm1_slp_wfi (void)
| Disable turn pwm1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pwm1_slp_wfi (void)
| Indicate whether turn pwm1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim0_slp_wfi (void)
| Enable turn QSPIM0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim0_slp_wfi (void)
| Disable turn QSPIM0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim0_slp_wfi (void)
| Indicate whether turn QSPIM0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim1_slp_wfi (void)
| Enable turn QSPIM1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim1_slp_wfi (void)
| Disable turn QSPIM1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim1_slp_wfi (void)
| Indicate whether turn QSPIM1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim2_slp_wfi (void)
| Enable turn QSPIM2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim2_slp_wfi (void)
| Disable turn QSPIM2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim2_slp_wfi (void)
| Indicate whether turn QSPIM2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_dspi_slp_wfi (void)
| Enable turn DSPI off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_dspi_slp_wfi (void)
| Disable turn DSPI off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_dspi_slp_wfi (void)
| Indicate whether turn DSPI off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pdm_slp_wfi (void)
| Enable turn PDM off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pdm_slp_wfi (void)
| Disable turn PDM off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pdm_slp_wfi (void)
| Indicate whether turn PDM off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_secu (uint32_t clk_mask)
| Individual block's clock control inside security system which was forced to turn off (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_secu (void)
| Return to clock blocks that was forcibly closed inside security system.(Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE void | ll_cgc_set_slp_off_hclk_secu (uint32_t clk_mask)
| Some security blocks automatic turn off clock during WFI/WFE. (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE uint32_t | ll_cgc_get_slp_off_secu (void)
| Return to security clock blocks that is turned off during WFI/WFE.(Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE void | ll_cgc_enable_force_off_aes_hclk (void)
| Enabling force to turn off the clock for AES. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_aes_hclk (void)
| Disabling force to turn off the clock for AES. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_aes_hclk (void)
| Indicate whether the clock for AES is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_hmac_hclk (void)
| Enabling force to turn off the clock for HMAC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_hmac_hclk (void)
| Disabling force to turn off the clock for HMAC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_hmac_hclk (void)
| Indicate whether the clock for HMAC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pkc_hclk (void)
| Enabling force to turn off the clock for PKC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pkc_hclk (void)
| Disabling force to turn off the clock for PKC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pkc_hclk (void)
| Indicate whether the clock for PKC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_present_hclk (void)
| Enabling force to turn off the clock for PRESENT. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_present_hclk (void)
| Disabling force to turn off the clock for PRESENT. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_present_hclk (void)
| Indicate whether the clock for PRESENT is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_ramkey_hclk (void)
| Enabling force to turn off the clock for RAMKEY. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_ramkey_hclk (void)
| Disabling force to turn off the clock for RAMKEY. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_ramkey_hclk (void)
| Indicate whether the clock for RAMKEY is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_rng_hclk (void)
| Enabling force to turn off the clock for RNG. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_rng_hclk (void)
| Disabling force to turn off the clock for RNG. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_rng_hclk (void)
| Indicate whether the clock for RNG is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_efuse_hclk (void)
| Enabling force to turn off the clock for EFUSE. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_efuse_hclk (void)
| Disabling force to turn off the clock for EFUSE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_efuse_hclk (void)
| Indicate whether the clock for EFUSE is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_aes_hclk (void)
| Enable AES automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_aes_hclk (void)
| Disable AES automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_aes_hclk (void)
| Indicate whether the AES automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_hmac_hclk (void)
| Enable HMAC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_hmac_hclk (void)
| Disable HMAC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_hmac_hclk (void)
| Indicate whether the HMAC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_pkc_hclk (void)
| Enable PKC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_pkc_hclk (void)
| Disable PKC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_pkc_hclk (void)
| Indicate whether the PKC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_present_hclk (void)
| Enable PRESENT automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_present_hclk (void)
| Disable PRESENT automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_present_hclk (void)
| Indicate whether the PRESENT automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_ramkey_hclk (void)
| Enable RAMKEY automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_ramkey_hclk (void)
| Disable RAMKEY automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_ramkey_hclk (void)
| Indicate whether the RAMKEY automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_rng_hclk (void)
| Enable RNG automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_rng_hclk (void)
| Disable RNG automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_rng_hclk (void)
| Indicate whether the RNG automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_efuse_hclk (void)
| Enable EFUSE automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_efuse_hclk (void)
| Disable EFUSE automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_efuse_hclk (void)
| Indicate whether the EFUSE automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_set_misc_clk (uint32_t clk_mask)
| Some MISC_CLK blocks turn off clock. (Include: GPADC/XQSPI/DMA0) More...
__STATIC_INLINE uint32_t | ll_cgc_get_misc_clk (void)
| Return to MISC_CLK clock blocks that is turned off.(Include: GPADC/XQSPI/DMA0) More...
__STATIC_INLINE void | ll_cgc_enable_force_off_gpadc_hclk (void)
| Enabling force to turn off the clock for GPADC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_gpadc_hclk (void)
| Disabling force to turn off the clock for GPADC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_gpadc_hclk (void)
| Indicate whether the clock for GPADC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_gpadc_hclk (void)
| Enable GPADC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_gpadc_hclk (void)
| Disable GPADC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_gpadc_hclk (void)
| Indicate whether the GPADC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xqspi_sck (void)
| Enable XQSPI SCK CLK turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xqspi_sck (void)
| Disable XQSPI SCK CLK turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xqspi_sck (void)
| Indicate whether the XQSPI SCK CLK automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dma0_hclk (void)
| Enable DMA0 turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dma0_hclk (void)
| Disable DMA0 turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dma0_hclk (void)
| Indicate whether the DMA0 automatic turn off clock is enabled. More...

## Detailed Description

Header file containing functions prototypes of CGC LL library.

Author
  BLE Driver Team

Attention
  #####Copyright (c) 2019 GOODIX All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file ll_cgc.h.