Macros
IT Defines
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants

Interrupt definitions which can be used with LL_UART_ReadReg and LL_UART_WriteReg functions. More...

## Macros
#define | LL_UART_IER_MS UART_IER_EDSSI
#define | LL_UART_IER_RLS UART_IER_ERLS
#define | LL_UART_IER_THRE (UART_IER_ETBEI | UART_IER_PTIME)
#define | LL_UART_IER_RDA UART_IER_ERBFI

## Detailed Description

Interrupt definitions which can be used with LL_UART_ReadReg and LL_UART_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_UART_IER_MS

#define LL_UART_IER_MS UART_IER_EDSSI

Enable Modem Status Interrupt

Definition at line 146 of file ll_uart.h.

## ◆ LL_UART_IER_RDA

#define LL_UART_IER_RDA UART_IER_ERBFI

Enable Received Data Available Interrupt and Character Timeout Interrupt

Definition at line 149 of file ll_uart.h.

## ◆ LL_UART_IER_RLS

#define LL_UART_IER_RLS UART_IER_ERLS

Enable Receiver Line Status Interrupt

Definition at line 147 of file ll_uart.h.

## ◆ LL_UART_IER_THRE

#define LL_UART_IER_THRE (UART_IER_ETBEI | UART_IER_PTIME)

Enable Transmit Holding Register Empty Interrupt

Definition at line 148 of file ll_uart.h.