Macros
ADC CLOCK
Peripheral Driver » LL Driver » ADC » Defines » ADC Exported Constants

## Macros
#define | LL_ADC_CLK_16M (4UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_8M (5UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_4M (6UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_1M (7UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_16K (1UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_8K (2UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_4K (3UL << MCU_SUB_SNSADC_CLK_WR_Pos)
#define | LL_ADC_CLK_NONE (0UL << MCU_SUB_SNSADC_CLK_WR_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ADC_CLK_16K

#define LL_ADC_CLK_16K (1UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 16KHz

Definition at line 131 of file ll_adc.h.

## ◆ LL_ADC_CLK_16M

#define LL_ADC_CLK_16M (4UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 16 MHz

Definition at line 127 of file ll_adc.h.

## ◆ LL_ADC_CLK_1M

#define LL_ADC_CLK_1M (7UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 1 MHz

Definition at line 130 of file ll_adc.h.

## ◆ LL_ADC_CLK_4K

#define LL_ADC_CLK_4K (3UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 4KHz

Definition at line 133 of file ll_adc.h.

## ◆ LL_ADC_CLK_4M

#define LL_ADC_CLK_4M (6UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 4 MHz

Definition at line 129 of file ll_adc.h.

## ◆ LL_ADC_CLK_8K

#define LL_ADC_CLK_8K (2UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 8KHz

Definition at line 132 of file ll_adc.h.

## ◆ LL_ADC_CLK_8M

#define LL_ADC_CLK_8M (5UL << MCU_SUB_SNSADC_CLK_WR_Pos)

ADC Clock = 8 MHz

Definition at line 128 of file ll_adc.h.

## ◆ LL_ADC_CLK_NONE

#define LL_ADC_CLK_NONE (0UL << MCU_SUB_SNSADC_CLK_WR_Pos)

No ADC Clock

Definition at line 134 of file ll_adc.h.