Macros
SPI Direction
Peripheral Driver » HAL Driver » SPI » CS Signal Description » Defines » SPI Exported Constants

## Macros
#define | SPI_DIRECTION_FULL_DUPLEX LL_SPI_FULL_DUPLEX
#define | SPI_DIRECTION_SIMPLEX_TX LL_SPI_SIMPLEX_TX
#define | SPI_DIRECTION_SIMPLEX_RX LL_SPI_SIMPLEX_RX
#define | SPI_DIRECTION_READ_EEPROM LL_SPI_READ_EEPROM

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_DIRECTION_FULL_DUPLEX

#define SPI_DIRECTION_FULL_DUPLEX LL_SPI_FULL_DUPLEX

Full Duplex: Transmit & Receive

Definition at line 276 of file hal_spi.h.

## ◆ SPI_DIRECTION_READ_EEPROM

#define SPI_DIRECTION_READ_EEPROM LL_SPI_READ_EEPROM

Read EEPROM

Definition at line 279 of file hal_spi.h.

## ◆ SPI_DIRECTION_SIMPLEX_RX

#define SPI_DIRECTION_SIMPLEX_RX LL_SPI_SIMPLEX_RX

Simplex Rx: Receive only

Definition at line 278 of file hal_spi.h.

## ◆ SPI_DIRECTION_SIMPLEX_TX

#define SPI_DIRECTION_SIMPLEX_TX LL_SPI_SIMPLEX_TX

Simplex Tx: Transmit only

Definition at line 277 of file hal_spi.h.