Macros
XIP read command
Peripheral Driver » LL Driver » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_XIP_CMD_READ 0x03
#define | LL_XQSPI_XIP_CMD_FAST_READ 0x0B
#define | LL_XQSPI_XIP_CMD_DUAL_OUT_READ 0x3B
#define | LL_XQSPI_XIP_CMD_DUAL_IO_READ 0xBB
#define | LL_XQSPI_XIP_CMD_QUAD_OUT_READ 0x6B
#define | LL_XQSPI_XIP_CMD_QUAD_IO_READ 0xEB

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_XIP_CMD_DUAL_IO_READ

#define LL_XQSPI_XIP_CMD_DUAL_IO_READ 0xBB

Dual-IO Fast Read mode

Definition at line 176 of file ll_xqspi.h.

## ◆ LL_XQSPI_XIP_CMD_DUAL_OUT_READ

#define LL_XQSPI_XIP_CMD_DUAL_OUT_READ 0x3B

Dual-Out Fast Read mode

Definition at line 175 of file ll_xqspi.h.

## ◆ LL_XQSPI_XIP_CMD_FAST_READ

#define LL_XQSPI_XIP_CMD_FAST_READ 0x0B

Fast Read mode

Definition at line 174 of file ll_xqspi.h.

## ◆ LL_XQSPI_XIP_CMD_QUAD_IO_READ

#define LL_XQSPI_XIP_CMD_QUAD_IO_READ 0xEB

Quad-IO Fast Read mode

Definition at line 178 of file ll_xqspi.h.

## ◆ LL_XQSPI_XIP_CMD_QUAD_OUT_READ

#define LL_XQSPI_XIP_CMD_QUAD_OUT_READ 0x6B

Quad-Out Fast Read mode

Definition at line 177 of file ll_xqspi.h.

## ◆ LL_XQSPI_XIP_CMD_READ

#define LL_XQSPI_XIP_CMD_READ 0x03

Read mode

Definition at line 173 of file ll_xqspi.h.