Macros
Defines
Peripheral Driver » APP DRIVER » GPIO » Defines

## Macros
#define | APP_IO_PIN_0 ((uint32_t)0x00000001U)
| APP_GPIO_DEFINE IO pins. More...
#define | APP_IO_PIN_1 ((uint32_t)0x00000002U)
#define | APP_IO_PIN_2 ((uint32_t)0x00000004U)
#define | APP_IO_PIN_3 ((uint32_t)0x00000008U)
#define | APP_IO_PIN_4 ((uint32_t)0x00000010U)
#define | APP_IO_PIN_5 ((uint32_t)0x00000020U)
#define | APP_IO_PIN_6 ((uint32_t)0x00000040U)
#define | APP_IO_PIN_7 ((uint32_t)0x00000080U)
#define | APP_IO_PIN_8 ((uint32_t)0x00000100U)
#define | APP_IO_PIN_9 ((uint32_t)0x00000200U)
#define | APP_IO_PIN_10 ((uint32_t)0x00000400U)
#define | APP_IO_PIN_11 ((uint32_t)0x00000800U)
#define | APP_IO_PIN_12 ((uint32_t)0x00001000U)
#define | APP_IO_PIN_13 ((uint32_t)0x00002000U)
#define | APP_IO_PIN_14 ((uint32_t)0x00004000U)
#define | APP_IO_PIN_15 ((uint32_t)0x00008000U)
#define | APP_IO_PINS_0_7 ((uint32_t)0x000000FFU)
#define | APP_IO_PINS_0_15 ((uint32_t)0x0000FFFFU)
#define | APP_IO_PINS_16_31 ((uint32_t)0xFFFF0000U)
#define | APP_AON_IO_PIN_ALL ((uint32_t)0x000000FFU)
#define | APP_IO_PIN_ALL ((uint32_t)0x0000FFFFU)
#define | APP_MSIO_IO_PIN_ALL ((uint32_t)0x000000FFU)
#define | APP_IO_PIN_MASK ((uint32_t)0xFFFFFFFFU)
#define | APP_IO_DEFAULT_CONFIG
| GR5xxx_APP_GPIO_default_config initStruct default config of APP_GPIOn. More...

## Detailed Description

## Macro Definition Documentation

## ◆ APP_AON_IO_PIN_ALL

#define APP_AON_IO_PIN_ALL ((uint32_t)0x000000FFU)

All AON pins selected

Definition at line 107 of file app_io.h.

## ◆ APP_IO_DEFAULT_CONFIG

#define APP_IO_DEFAULT_CONFIG

Value:
{ \
.pin = APP_IO_PIN_ALL, \
.mode = APP_IO_MODE_INPUT, \
.pull = APP_IO_PULLDOWN, \
}

GR5xxx_APP_GPIO_default_config initStruct default config of APP_GPIOn.

Definition at line 115 of file app_io.h.

## ◆ APP_IO_PIN_0

#define APP_IO_PIN_0 ((uint32_t)0x00000001U)

APP_GPIO_DEFINE IO pins.

Pin 0 selected

Definition at line 69 of file app_io.h.

## ◆ APP_IO_PIN_1

#define APP_IO_PIN_1 ((uint32_t)0x00000002U)

Pin 1 selected

Definition at line 70 of file app_io.h.

## ◆ APP_IO_PIN_10

#define APP_IO_PIN_10 ((uint32_t)0x00000400U)

Pin 10 selected

Definition at line 79 of file app_io.h.

## ◆ APP_IO_PIN_11

#define APP_IO_PIN_11 ((uint32_t)0x00000800U)

Pin 11 selected

Definition at line 80 of file app_io.h.

## ◆ APP_IO_PIN_12

#define APP_IO_PIN_12 ((uint32_t)0x00001000U)

Pin 12 selected

Definition at line 81 of file app_io.h.

## ◆ APP_IO_PIN_13

#define APP_IO_PIN_13 ((uint32_t)0x00002000U)

Pin 13 selected

Definition at line 82 of file app_io.h.

## ◆ APP_IO_PIN_14

#define APP_IO_PIN_14 ((uint32_t)0x00004000U)

Pin 14 selected

Definition at line 83 of file app_io.h.

## ◆ APP_IO_PIN_15

#define APP_IO_PIN_15 ((uint32_t)0x00008000U)

Pin 15 selected

Definition at line 84 of file app_io.h.

## ◆ APP_IO_PIN_2

#define APP_IO_PIN_2 ((uint32_t)0x00000004U)

Pin 2 selected

Definition at line 71 of file app_io.h.

## ◆ APP_IO_PIN_3

#define APP_IO_PIN_3 ((uint32_t)0x00000008U)

Pin 3 selected

Definition at line 72 of file app_io.h.

## ◆ APP_IO_PIN_4

#define APP_IO_PIN_4 ((uint32_t)0x00000010U)

Pin 4 selected

Definition at line 73 of file app_io.h.

## ◆ APP_IO_PIN_5

#define APP_IO_PIN_5 ((uint32_t)0x00000020U)

Pin 5 selected

Definition at line 74 of file app_io.h.

## ◆ APP_IO_PIN_6

#define APP_IO_PIN_6 ((uint32_t)0x00000040U)

Pin 6 selected

Definition at line 75 of file app_io.h.

## ◆ APP_IO_PIN_7

#define APP_IO_PIN_7 ((uint32_t)0x00000080U)

Pin 7 selected

Definition at line 76 of file app_io.h.

## ◆ APP_IO_PIN_8

#define APP_IO_PIN_8 ((uint32_t)0x00000100U)

Pin 8 selected

Definition at line 77 of file app_io.h.

## ◆ APP_IO_PIN_9

#define APP_IO_PIN_9 ((uint32_t)0x00000200U)

Pin 9 selected

Definition at line 78 of file app_io.h.

## ◆ APP_IO_PIN_ALL

#define APP_IO_PIN_ALL ((uint32_t)0x0000FFFFU)

All pins selected

Definition at line 108 of file app_io.h.

## ◆ APP_IO_PIN_MASK

#define APP_IO_PIN_MASK ((uint32_t)0xFFFFFFFFU)

PIN mask for assert test

Definition at line 110 of file app_io.h.

## ◆ APP_IO_PINS_0_15

#define APP_IO_PINS_0_15 ((uint32_t)0x0000FFFFU)

0~15 pins selected

Definition at line 105 of file app_io.h.

## ◆ APP_IO_PINS_0_7

#define APP_IO_PINS_0_7 ((uint32_t)0x000000FFU)

0~7 pins selected

Definition at line 104 of file app_io.h.

## ◆ APP_IO_PINS_16_31

#define APP_IO_PINS_16_31 ((uint32_t)0xFFFF0000U)

16~31 pins selected

Definition at line 106 of file app_io.h.

## ◆ APP_MSIO_IO_PIN_ALL

#define APP_MSIO_IO_PIN_ALL ((uint32_t)0x000000FFU)

All MISO pins selected

Definition at line 109 of file app_io.h.

APP_IO_MODE_INPUT
@ APP_IO_MODE_INPUT
Definition: app_io.h:158
APP_IO_PULLDOWN
@ APP_IO_PULLDOWN
Definition: app_io.h:179
APP_IO_PIN_ALL
#define APP_IO_PIN_ALL
Definition: app_io.h:108