Enumerations
Enums
BLE » BLE_ID

## Enumerations
enum | hci_opcode { HCI_NO_OPERATION_CMD_OPCODE = 0x0000, HCI_INQ_CMD_OPCODE = 0x0401, HCI_INQ_CANCEL_CMD_OPCODE = 0x0402, HCI_PER_INQ_MODE_CMD_OPCODE = 0x0403, HCI_EXIT_PER_INQ_MODE_CMD_OPCODE = 0x0404, HCI_CREATE_CON_CMD_OPCODE = 0x0405, HCI_DISCONNECT_CMD_OPCODE = 0x0406, HCI_CREATE_CON_CANCEL_CMD_OPCODE = 0x0408, HCI_ACCEPT_CON_REQ_CMD_OPCODE = 0x0409, HCI_REJECT_CON_REQ_CMD_OPCODE = 0x040A, HCI_LK_REQ_REPLY_CMD_OPCODE = 0x040B, HCI_LK_REQ_NEG_REPLY_CMD_OPCODE = 0x040C, HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE = 0x040D, HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE = 0x040E, HCI_CHG_CON_PKT_TYPE_CMD_OPCODE = 0x040F, HCI_AUTH_REQ_CMD_OPCODE = 0x0411, HCI_SET_CON_ENC_CMD_OPCODE = 0x0413, HCI_CHG_CON_LK_CMD_OPCODE = 0x0415, HCI_MASTER_LK_CMD_OPCODE = 0x0417, HCI_REM_NAME_REQ_CMD_OPCODE = 0x0419, HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE = 0x041A, HCI_RD_REM_SUPP_FEATS_CMD_OPCODE = 0x041B, HCI_RD_REM_EXT_FEATS_CMD_OPCODE = 0x041C, HCI_RD_REM_VER_INFO_CMD_OPCODE = 0x041D, HCI_RD_CLK_OFF_CMD_OPCODE = 0x041F, HCI_RD_LMP_HDL_CMD_OPCODE = 0x0420, HCI_SETUP_SYNC_CON_CMD_OPCODE = 0x0428, HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE = 0x0429, HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE = 0x042A, HCI_IO_CAP_REQ_REPLY_CMD_OPCODE = 0x042B, HCI_USER_CFM_REQ_REPLY_CMD_OPCODE = 0x042C, HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE = 0x042D, HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE = 0x042E, HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE = 0x042F, HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE = 0x0430, HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE = 0x0433, HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE = 0x0434, HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE = 0x043D, HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE = 0x043E, HCI_TRUNC_PAGE_CMD_OPCODE = 0x043F, HCI_TRUNC_PAGE_CAN_CMD_OPCODE = 0x0440, HCI_SET_CON_SLV_BCST_CMD_OPCODE = 0x0441, HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE = 0x0442, HCI_START_SYNC_TRAIN_CMD_OPCODE = 0x0443, HCI_REC_SYNC_TRAIN_CMD_OPCODE = 0x0444, HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE = 0x0445, HCI_HOLD_MODE_CMD_OPCODE = 0x0801, HCI_SNIFF_MODE_CMD_OPCODE = 0x0803, HCI_EXIT_SNIFF_MODE_CMD_OPCODE = 0x0804, HCI_PARK_STATE_CMD_OPCODE = 0x0805, HCI_EXIT_PARK_STATE_CMD_OPCODE = 0x0806, HCI_QOS_SETUP_CMD_OPCODE = 0x0807, HCI_ROLE_DISCOVERY_CMD_OPCODE = 0x0809, HCI_SWITCH_ROLE_CMD_OPCODE = 0x080B, HCI_RD_LINK_POL_STG_CMD_OPCODE = 0x080C, HCI_WR_LINK_POL_STG_CMD_OPCODE = 0x080D, HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE = 0x080E, HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE = 0x080F, HCI_FLOW_SPEC_CMD_OPCODE = 0x0810, HCI_SNIFF_SUB_CMD_OPCODE = 0x0811, HCI_SET_EVT_MASK_CMD_OPCODE = 0x0C01, HCI_RESET_CMD_OPCODE = 0x0C03, HCI_SET_EVT_FILTER_CMD_OPCODE = 0x0C05, HCI_FLUSH_CMD_OPCODE = 0x0C08, HCI_RD_PIN_TYPE_CMD_OPCODE = 0x0C09, HCI_WR_PIN_TYPE_CMD_OPCODE = 0x0C0A, HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE = 0x0C0B, HCI_RD_STORED_LK_CMD_OPCODE = 0x0C0D, HCI_WR_STORED_LK_CMD_OPCODE = 0x0C11, HCI_DEL_STORED_LK_CMD_OPCODE = 0x0C12, HCI_WR_LOCAL_NAME_CMD_OPCODE = 0x0C13, HCI_RD_LOCAL_NAME_CMD_OPCODE = 0x0C14, HCI_RD_CON_ACCEPT_TO_CMD_OPCODE = 0x0C15, HCI_WR_CON_ACCEPT_TO_CMD_OPCODE = 0x0C16, HCI_RD_PAGE_TO_CMD_OPCODE = 0x0C17, HCI_WR_PAGE_TO_CMD_OPCODE = 0x0C18, HCI_RD_SCAN_EN_CMD_OPCODE = 0x0C19, HCI_WR_SCAN_EN_CMD_OPCODE = 0x0C1A, HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE = 0x0C1B, HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE = 0x0C1C, HCI_RD_INQ_SCAN_ACT_CMD_OPCODE = 0x0C1D, HCI_WR_INQ_SCAN_ACT_CMD_OPCODE = 0x0C1E, HCI_RD_AUTH_EN_CMD_OPCODE = 0x0C1F, HCI_WR_AUTH_EN_CMD_OPCODE = 0x0C20, HCI_RD_CLASS_OF_DEV_CMD_OPCODE = 0x0C23, HCI_WR_CLASS_OF_DEV_CMD_OPCODE = 0x0C24, HCI_RD_VOICE_STG_CMD_OPCODE = 0x0C25, HCI_WR_VOICE_STG_CMD_OPCODE = 0x0C26, HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE = 0x0C27, HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE = 0x0C28, HCI_RD_NB_BDCST_RETX_CMD_OPCODE = 0x0C29, HCI_WR_NB_BDCST_RETX_CMD_OPCODE = 0x0C2A, HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE = 0x0C2B, HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE = 0x0C2C, HCI_RD_TX_PWR_LVL_CMD_OPCODE = 0x0C2D, HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE = 0x0C2E, HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE = 0x0C2F, HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE = 0x0C31, HCI_HOST_BUF_SIZE_CMD_OPCODE = 0x0C33, HCI_HOST_NB_CMP_PKTS_CMD_OPCODE = 0x0C35, HCI_RD_LINK_SUPV_TO_CMD_OPCODE = 0x0C36, HCI_WR_LINK_SUPV_TO_CMD_OPCODE = 0x0C37, HCI_RD_NB_SUPP_IAC_CMD_OPCODE = 0x0C38, HCI_RD_CURR_IAC_LAP_CMD_OPCODE = 0x0C39, HCI_WR_CURR_IAC_LAP_CMD_OPCODE = 0x0C3A, HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE = 0x0C3F, HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE = 0x0C42, HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE = 0x0C43, HCI_RD_INQ_MODE_CMD_OPCODE = 0x0C44, HCI_WR_INQ_MODE_CMD_OPCODE = 0x0C45, HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE = 0x0C46, HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE = 0x0C47, HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE = 0x0C48, HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE = 0x0C49, HCI_RD_EXT_INQ_RSP_CMD_OPCODE = 0x0C51, HCI_WR_EXT_INQ_RSP_CMD_OPCODE = 0x0C52, HCI_REFRESH_ENC_KEY_CMD_OPCODE = 0x0C53, HCI_RD_SP_MODE_CMD_OPCODE = 0x0C55, HCI_WR_SP_MODE_CMD_OPCODE = 0x0C56, HCI_RD_LOC_OOB_DATA_CMD_OPCODE = 0x0C57, HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE = 0x0C58, HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE = 0x0C59, HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE = 0x0C5A, HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE = 0x0C5B, HCI_ENH_FLUSH_CMD_OPCODE = 0x0C5F, HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE = 0x0C60, HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE = 0x0C63, HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE = 0x0C66, HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE = 0x0C67, HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE = 0x0C68, HCI_RD_LE_HOST_SUPP_CMD_OPCODE = 0x0C6C, HCI_WR_LE_HOST_SUPP_CMD_OPCODE = 0x0C6D, HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE = 0x0C6E, HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE = 0x0C6F, HCI_SET_MWS_SIGNALING_CMD_OPCODE = 0x0C70, HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE = 0x0C71, HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE = 0x0C72, HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE = 0x0C73, HCI_SET_RES_LT_ADDR_CMD_OPCODE = 0x0C74, HCI_DEL_RES_LT_ADDR_CMD_OPCODE = 0x0C75, HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE = 0x0C76, HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE = 0x0C77, HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE = 0x0C78, HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE = 0x0C79, HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE = 0x0C7A, HCI_RD_AUTH_PAYL_TO_CMD_OPCODE = 0x0C7B, HCI_WR_AUTH_PAYL_TO_CMD_OPCODE = 0x0C7C, HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE = 0x0C7D, HCI_RD_EXT_PAGE_TO_CMD_OPCODE = 0x0C7E, HCI_WR_EXT_PAGE_TO_CMD_OPCODE = 0x0C7F, HCI_RD_EXT_INQ_LEN_CMD_OPCODE = 0x0C80, HCI_WR_EXT_INQ_LEN_CMD_OPCODE = 0x0C81, HCI_SET_ECO_BASE_INTV_CMD_OPCODE = 0x0C82, HCI_CONFIG_DATA_PATH_CMD_OPCODE = 0x0C83, HCI_RD_LOCAL_VER_INFO_CMD_OPCODE = 0x1001, HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE = 0x1002, HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE = 0x1003, HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE = 0x1004, HCI_RD_BUF_SIZE_CMD_OPCODE = 0x1005, HCI_RD_BD_ADDR_CMD_OPCODE = 0x1009, HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE = 0x100A, HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE = 0x100B, HCI_RD_LOCAL_SP_OPT_CMD_OPCODE = 0x100C, HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE = 0x100D, HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE = 0x100E, HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE = 0x100F, HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE = 0x1401, HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE = 0x1402, HCI_RD_LINK_QUAL_CMD_OPCODE = 0x1403, HCI_RD_RSSI_CMD_OPCODE = 0x1405, HCI_RD_AFH_CH_MAP_CMD_OPCODE = 0x1406, HCI_RD_CLK_CMD_OPCODE = 0x1407, HCI_RD_ENC_KEY_SIZE_CMD_OPCODE = 0x1408, HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE = 0x140C, HCI_RD_LOOPBACK_MODE_CMD_OPCODE = 0x1801, HCI_WR_LOOPBACK_MODE_CMD_OPCODE = 0x1802, HCI_EN_DUT_MODE_CMD_OPCODE = 0x1803, HCI_WR_SP_DBG_MODE_CMD_OPCODE = 0x1804, HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE = 0x180A, HCI_LE_SET_EVT_MASK_CMD_OPCODE = 0x2001, HCI_LE_RD_BUF_SIZE_CMD_OPCODE = 0x2002, HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE = 0x2003, HCI_LE_SET_RAND_ADDR_CMD_OPCODE = 0x2005, HCI_LE_SET_ADV_PARAM_CMD_OPCODE = 0x2006, HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE = 0x2007, HCI_LE_SET_ADV_DATA_CMD_OPCODE = 0x2008, HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE = 0x2009, HCI_LE_SET_ADV_EN_CMD_OPCODE = 0x200A, HCI_LE_SET_SCAN_PARAM_CMD_OPCODE = 0x200B, HCI_LE_SET_SCAN_EN_CMD_OPCODE = 0x200C, HCI_LE_CREATE_CON_CMD_OPCODE = 0x200D, HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE = 0x200E, HCI_LE_RD_WLST_SIZE_CMD_OPCODE = 0x200F, HCI_LE_CLEAR_WLST_CMD_OPCODE = 0x2010, HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE = 0x2011, HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE = 0x2012, HCI_LE_CON_UPDATE_CMD_OPCODE = 0x2013, HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE = 0x2014, HCI_LE_RD_CHNL_MAP_CMD_OPCODE = 0x2015, HCI_LE_RD_REM_FEATS_CMD_OPCODE = 0x2016, HCI_LE_ENC_CMD_OPCODE = 0x2017, HCI_LE_RAND_CMD_OPCODE = 0x2018, HCI_LE_EN_ENC_CMD_OPCODE = 0x2019, HCI_LE_LTK_REQ_REPLY_CMD_OPCODE = 0x201A, HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE = 0x201B, HCI_LE_RD_SUPP_STATES_CMD_OPCODE = 0x201C, HCI_LE_RX_TEST_V1_CMD_OPCODE = 0x201D, HCI_LE_TX_TEST_V1_CMD_OPCODE = 0x201E, HCI_LE_TEST_END_CMD_OPCODE = 0x201F, HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE = 0x2020, HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE = 0x2021, HCI_LE_SET_DATA_LEN_CMD_OPCODE = 0x2022, HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE = 0x2023, HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE = 0x2024, HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE = 0x2025, HCI_LE_GEN_DHKEY_V1_CMD_OPCODE = 0x2026, HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE = 0x2027, HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE = 0x2028, HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE = 0x2029, HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE = 0x202A, HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE = 0x202B, HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE = 0x202C, HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE = 0x202D, HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE = 0x202E, HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE = 0x202F, HCI_LE_RD_PHY_CMD_OPCODE = 0x2030, HCI_LE_SET_DFT_PHY_CMD_OPCODE = 0x2031, HCI_LE_SET_PHY_CMD_OPCODE = 0x2032, HCI_LE_RX_TEST_V2_CMD_OPCODE = 0x2033, HCI_LE_TX_TEST_V2_CMD_OPCODE = 0x2034, HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE = 0x2035, HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE = 0x2036, HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE = 0x2037, HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE = 0x2038, HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE = 0x2039, HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE = 0x203A, HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE = 0x203B, HCI_LE_RMV_ADV_SET_CMD_OPCODE = 0x203C, HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE = 0x203D, HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE = 0x203E, HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE = 0x203F, HCI_LE_SET_PER_ADV_EN_CMD_OPCODE = 0x2040, HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE = 0x2041, HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE = 0x2042, HCI_LE_EXT_CREATE_CON_CMD_OPCODE = 0x2043, HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE = 0x2044, HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE = 0x2045, HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE = 0x2046, HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE = 0x2047, HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE = 0x2048, HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE = 0x2049, HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE = 0x204A, HCI_LE_RD_TX_PWR_CMD_OPCODE = 0x204B, HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE = 0x204C, HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE = 0x204D, HCI_LE_SET_PRIV_MODE_CMD_OPCODE = 0x204E, HCI_LE_RX_TEST_V3_CMD_OPCODE = 0x204F, HCI_LE_TX_TEST_V3_CMD_OPCODE = 0x2050, HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE = 0x2051, HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE = 0x2052, HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE = 0x2053, HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE = 0x2054, HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE = 0x2055, HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE = 0x2056, HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE = 0x2057, HCI_LE_RD_ANTENNA_INF_CMD_OPCODE = 0x2058, HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE = 0x2059, HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE = 0x205A, HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE = 0x205B, HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE = 0x205C, HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE = 0x205D, HCI_LE_GEN_DHKEY_V2_CMD_OPCODE = 0x205E, HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE = 0x205F, HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE = 0x2060, HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE = 0x2061, HCI_LE_SET_CIG_PARAMS_CMD_OPCODE = 0x2062, HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE = 0x2063, HCI_LE_CREATE_CIS_CMD_OPCODE = 0x2064, HCI_LE_REMOVE_CIG_CMD_OPCODE = 0x2065, HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE = 0x2066, HCI_LE_REJECT_CIS_REQ_CMD_OPCODE = 0x2067, HCI_LE_CREATE_BIG_CMD_OPCODE = 0x2068, HCI_LE_CREATE_BIG_TEST_CMD_OPCODE = 0x2069, HCI_LE_TERMINATE_BIG_CMD_OPCODE = 0x206A, HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE = 0x206B, HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE = 0x206C, HCI_LE_REQ_PEER_SCA_CMD_OPCODE = 0x206D, HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE = 0x206E, HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE = 0x206F, HCI_LE_ISO_TX_TEST_CMD_OPCODE = 0x2070, HCI_LE_ISO_RX_TEST_CMD_OPCODE = 0x2071, HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE = 0x2072, HCI_LE_ISO_TEST_END_CMD_OPCODE = 0x2073, HCI_LE_SET_HOST_FEATURE_CMD_OPCODE = 0x2074, HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE = 0x2075, HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE = 0x2076, HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE = 0x2077, HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE = 0x2078, HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE = 0x2079, HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE = 0x207A, HCI_LE_TX_TEST_V4_CMD_OPCODE = 0x207B, HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE = 0x20F9, HCI_LE_START_RANGING_CMD_OPCODE = 0x20FA, HCI_PUBLIC_ADDR_SET_CMD_OPCODE = 0x20FB, HCI_LE_TIME_SYNC_EN_CMD_OPCODE = 0x20FC, HCI_DBG_RD_MEM_CMD_OPCODE = 0xFC01, HCI_DBG_WR_MEM_CMD_OPCODE = 0xFC02, HCI_DBG_DEL_PAR_CMD_OPCODE = 0xFC03, HCI_DBG_ID_FLASH_CMD_OPCODE = 0xFC05, HCI_DBG_ER_FLASH_CMD_OPCODE = 0xFC06, HCI_DBG_WR_FLASH_CMD_OPCODE = 0xFC07, HCI_DBG_RD_FLASH_CMD_OPCODE = 0xFC08, HCI_DBG_RD_PAR_CMD_OPCODE = 0xFC09, HCI_DBG_WR_PAR_CMD_OPCODE = 0xFC0A, HCI_DBG_WLAN_COEX_CMD_OPCODE = 0xFC0B, HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE = 0xFC0D, HCI_DBG_BT_SEND_LMP_CMD_OPCODE = 0xFC0E, HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE = 0xFC0F, HCI_DBG_RD_KE_STATS_CMD_OPCODE = 0xFC10, HCI_DBG_PLF_RESET_CMD_OPCODE = 0xFC11, HCI_DBG_RD_MEM_INFO_CMD_OPCODE = 0xFC12, HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE = 0xFC13, HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE = 0xFC14, HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE = 0xFC15, HCI_DBG_BLE_REG_RD_CMD_OPCODE = 0xFC30, HCI_DBG_BLE_REG_WR_CMD_OPCODE = 0xFC31, HCI_DBG_SEND_LLCP_CMD_OPCODE = 0xFC35, HCI_DBG_LLCP_DISCARD_CMD_OPCODE = 0xFC36, HCI_DBG_RF_REG_RD_CMD_OPCODE = 0xFC39, HCI_DBG_RF_REG_WR_CMD_OPCODE = 0xFC3A, HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE = 0xFC3C, HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE = 0xFC3D, HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE = 0xFC3E, HCI_DBG_RF_CNTL_TX_CMD_OPCODE = 0xFC3F }
enum | hci_evt_code { HCI_INQ_CMP_EVT_CODE = 0x01, HCI_INQ_RES_EVT_CODE = 0x02, HCI_CON_CMP_EVT_CODE = 0x03, HCI_CON_REQ_EVT_CODE = 0x04, HCI_DISC_CMP_EVT_CODE = 0x05, HCI_AUTH_CMP_EVT_CODE = 0x06, HCI_REM_NAME_REQ_CMP_EVT_CODE = 0x07, HCI_ENC_CHG_EVT_CODE = 0x08, HCI_CHG_CON_LK_CMP_EVT_CODE = 0x09, HCI_MASTER_LK_CMP_EVT_CODE = 0x0A, HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE = 0x0B, HCI_RD_REM_VER_INFO_CMP_EVT_CODE = 0x0C, HCI_QOS_SETUP_CMP_EVT_CODE = 0x0D, HCI_CMD_CMP_EVT_CODE = 0x0E, HCI_CMD_STATUS_EVT_CODE = 0x0F, HCI_HW_ERR_EVT_CODE = 0x10, HCI_FLUSH_OCCURRED_EVT_CODE = 0x11, HCI_ROLE_CHG_EVT_CODE = 0x12, HCI_NB_CMP_PKTS_EVT_CODE = 0x13, HCI_MODE_CHG_EVT_CODE = 0x14, HCI_RETURN_LINK_KEYS_EVT_CODE = 0x15, HCI_PIN_CODE_REQ_EVT_CODE = 0x16, HCI_LK_REQ_EVT_CODE = 0x17, HCI_LK_NOTIF_EVT_CODE = 0x18, HCI_DATA_BUF_OVFLW_EVT_CODE = 0x1A, HCI_MAX_SLOT_CHG_EVT_CODE = 0x1B, HCI_RD_CLK_OFF_CMP_EVT_CODE = 0x1C, HCI_CON_PKT_TYPE_CHG_EVT_CODE = 0x1D, HCI_QOS_VIOL_EVT_CODE = 0x1E, HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE = 0x20, HCI_FLOW_SPEC_CMP_EVT_CODE = 0x21, HCI_INQ_RES_WITH_RSSI_EVT_CODE = 0x22, HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE = 0x23, HCI_SYNC_CON_CMP_EVT_CODE = 0x2C, HCI_SYNC_CON_CHG_EVT_CODE = 0x2D, HCI_SNIFF_SUB_EVT_CODE = 0x2E, HCI_EXT_INQ_RES_EVT_CODE = 0x2F, HCI_ENC_KEY_REFRESH_CMP_EVT_CODE = 0x30, HCI_IO_CAP_REQ_EVT_CODE = 0x31, HCI_IO_CAP_RSP_EVT_CODE = 0x32, HCI_USER_CFM_REQ_EVT_CODE = 0x33, HCI_USER_PASSKEY_REQ_EVT_CODE = 0x34, HCI_REM_OOB_DATA_REQ_EVT_CODE = 0x35, HCI_SP_CMP_EVT_CODE = 0x36, HCI_LINK_SUPV_TO_CHG_EVT_CODE = 0x38, HCI_ENH_FLUSH_CMP_EVT_CODE = 0x39, HCI_USER_PASSKEY_NOTIF_EVT_CODE = 0x3B, HCI_KEYPRESS_NOTIF_EVT_CODE = 0x3C, HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE = 0x3D, HCI_LE_META_EVT_CODE = 0x3E, HCI_MAX_EVT_MSK_PAGE_1_CODE = 0x40, HCI_SYNC_TRAIN_CMP_EVT_CODE = 0x4F, HCI_SYNC_TRAIN_REC_EVT_CODE = 0x50, HCI_CON_SLV_BCST_REC_EVT_CODE = 0x51, HCI_CON_SLV_BCST_TO_EVT_CODE = 0x52, HCI_TRUNC_PAGE_CMP_EVT_CODE = 0x53, HCI_SLV_PAGE_RSP_TO_EVT_CODE = 0x54, HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE = 0x55, HCI_AUTH_PAYL_TO_EXP_EVT_CODE = 0x57, HCI_SAM_STATUS_CHANGE_EVT_CODE = 0x58, HCI_MAX_EVT_MSK_PAGE_2_CODE = 0x59, HCI_DBG_META_EVT_CODE = 0xFF }
enum | hci_le_evt_subcode { HCI_LE_CON_CMP_EVT_SUBCODE = 0x01, HCI_LE_ADV_REPORT_EVT_SUBCODE = 0x02, HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE = 0x03, HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE = 0x04, HCI_LE_LTK_REQUEST_EVT_SUBCODE = 0x05, HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE = 0x06, HCI_LE_DATA_LEN_CHG_EVT_SUBCODE = 0x07, HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE = 0x08, HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE = 0x09, HCI_LE_ENH_CON_CMP_EVT_SUBCODE = 0x0A, HCI_LE_DIR_ADV_REP_EVT_SUBCODE = 0x0B, HCI_LE_PHY_UPD_CMP_EVT_SUBCODE = 0x0C, HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE = 0x0D, HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE = 0x0E, HCI_LE_PER_ADV_REPORT_EVT_SUBCODE = 0x0F, HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE = 0x10, HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE = 0x11, HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE = 0x12, HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE = 0x13, HCI_LE_CH_SEL_ALGO_EVT_SUBCODE = 0x14, HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE = 0x15, HCI_LE_CON_IQ_REPORT_EVT_SUBCODE = 0x16, HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE = 0x17, HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE = 0x18, HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE = 0x19, HCI_LE_CIS_REQUEST_EVT_SUBCODE = 0x1A, HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE = 0x1B, HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE = 0x1C, HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE = 0x1D, HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE = 0x1E, HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE = 0x1F, HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE = 0x20, HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE = 0x21, HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE = 0x22, HCI_LE_RANGING_IND_EVT_SUBCODE = 0x31, HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE = 0x32, HCI_LE_RANGING_CMP_EVT_SUBCODE = 0x33 }
enum | hci_vs_opcode { HCI_VS_LE_SET_DK_DEVICE_INFO_CMD_OPCODE = 0xFC70, HCI_VS_LE_GET_LINK_INFO_CMD_OPCODE = 0xFC73, HCI_VS_LE_CREATE_SNIFFER_CMD_OPCODE = 0xFC74, HCI_VS_LE_DISCONNECT_SNIFFER_CMD_OPCODE = 0xFC75, HCI_VS_LE_UPDATE_SNIFFER_CON_PARAM_CMD_OPCODE = 0xFC76, HCI_VS_LE_UPDATE_SNIFFER_CH_MAP_PARAM_CMD_OPCODE = 0xFC77, HCI_VS_LE_UPDATE_SNIFFER_PHY_PARAM_CMD_OPCODE = 0xFC78, HCI_VS_LE_RSSI_ENABLE_RANGING_CMD_OPCODE = 0xFC79, HCI_VS_LE_RSSI_UPDATE_RANGING_TYPE_CMD_OPCODE = 0xFC7A, HCI_VS_LE_EVENT_NOTIFICATION_EN_CMD_OPCODE = 0xFC7D }
enum | hci_vs_dbg_evt_subcode { HCI_VS_LE_GET_LINK_INFO_CMP_EVT_SUBCODE = 0x10, HCI_VS_LE_SNIFFER_DISC_CMP_EVT_SUBCODE = 0x11, HCI_VS_LE_REQ_BLE_CLOCK_SYNC_EVT_SUBCODE = 0x12, HCI_VS_LE_CON_PARAM_NOTIF_EVT_SUBCODE = 0x13, HCI_VS_LE_CH_MAP_PARAM_NOTIF_EVT_SUBCODE = 0x14, HCI_VS_LE_PHY_PARAM_NOTIF_EVT_SUBCODE = 0x15, HCI_VS_LE_RSSI_REPORT_INFO_EVT_SUBCODE = 0x16, HCI_VS_LE_RSSI_RANGING_TYPE_NOTIF_EVT_SUBCODE = 0x17, HCI_VS_LE_EVENT_NOTIFICATION_REPORT_INFO_EVT_SUBCODE = 0x18 }
enum | TASK_API_ID { TASK_ID_LLM = 0, TASK_ID_LLC = 1, TASK_ID_LLD = 2, TASK_ID_LLI = 3, TASK_ID_DBG = 4, TASK_ID_LM = 5, TASK_ID_LC = 6, TASK_ID_LB = 7, TASK_ID_LD = 8, TASK_ID_SDK = 9, TASK_ID_L2CC = 10, TASK_ID_GATTM = 11, TASK_ID_GATTC = 12, TASK_ID_GAPM = 13, TASK_ID_GAPC = 14, TASK_ID_APP = 15, TASK_ID_AHI = 16, TASK_ID_HCI = 17, TASK_ID_DISPLAY = 19, TASK_ID_MESH = 200, TASK_ID_RTLS = 250, TASK_ID_INVALID = 0xFF }
enum | hci_msg_id { HCI_MSG_ID_FIRST = TASK_FIRST_MSG(TASK_ID_HCI), HCI_CMD_CMP_EVENT, HCI_CMD_STAT_EVENT, HCI_EVENT, HCI_LE_EVENT, HCI_COMMAND, HCI_ACL_DATA, HCI_VS_EVENT, HCI_MSG_ID_LAST }
| HCI task Message ID. More...
enum | sdk_msg_id { SDK_COMMON_TIMEOUT_TIMER_0 = TASK_FIRST_MSG(TASK_ID_SDK), SDK_COMMON_TIMEOUT_TIMER_1, SDK_COMMON_TIMEOUT_TIMER_2, SDK_COMMON_TIMEOUT_TIMER_3, SDK_COMMON_TIMEOUT_TIMER_4, SDK_COMMON_TIMEOUT_TIMER_5, SDK_COMMON_TIMEOUT_TIMER_6, SDK_COMMON_TIMEOUT_TIMER_7, SDK_COMMON_TIMEOUT_TIMER_8, SDK_COMMON_TIMEOUT_TIMER_9, SDK_RANGING_INTER_NODE_COMM_RX_DATA, SDK_RANGING_INTER_NODE_COMM_TX_DATA_CMP, SDK_RANGING_INTER_NODE_COMM_ABORT_TX_CMP, SDK_RANGING_INTER_NODE_COMM_ERR_OCCUR, SDK_RANGING_SLEEP_RANGING, SDK_RANGING_WAKEUP_RANGING, SDK_RANGING_START_RANGING, SDK_RANGING_STOP_RANGING, SDK_RANGING_ANCHOR_START_RANGING, SDK_RANGING_ANCHOR_STOP_RANGING, SDK_RANGING_UPDATE_CI, SDK_RANGING_TIMEOUT_DISPATCH, SDK_APP_SET_SCAN_ADDR }
| SDK_TASK Message ID. More...
enum | gapc_msg_id { GAPC_CMP_EVT = MSG_ID(GAPC, 0x00), GAPC_CONNECTION_REQ_IND = MSG_ID(GAPC, 0x01), GAPC_CONNECTION_CFM = MSG_ID(GAPC, 0x02), GAPC_DISCONNECT_IND = MSG_ID(GAPC, 0x03), GAPC_DISCONNECT_CMD = MSG_ID(GAPC, 0x04), GAPC_GET_INFO_CMD = MSG_ID(GAPC, 0x05), GAPC_PEER_ATT_INFO_IND = MSG_ID(GAPC, 0x06), GAPC_PEER_VERSION_IND = MSG_ID(GAPC, 0x07), GAPC_PEER_FEATURES_IND = MSG_ID(GAPC, 0x08), GAPC_CON_RSSI_IND = MSG_ID(GAPC, 0x09), GAPC_GET_DEV_INFO_REQ_IND = MSG_ID(GAPC, 0x0A), GAPC_GET_DEV_INFO_CFM = MSG_ID(GAPC, 0x0B), GAPC_SET_DEV_INFO_REQ_IND = MSG_ID(GAPC, 0x0C), GAPC_SET_DEV_INFO_CFM = MSG_ID(GAPC, 0x0D), GAPC_PARAM_UPDATE_CMD = MSG_ID(GAPC, 0x0E), GAPC_PARAM_UPDATE_REQ_IND = MSG_ID(GAPC, 0x0F), GAPC_PARAM_UPDATE_CFM = MSG_ID(GAPC, 0x10), GAPC_PARAM_UPDATED_IND = MSG_ID(GAPC, 0x11), GAPC_BOND_CMD = MSG_ID(GAPC, 0x12), GAPC_BOND_REQ_IND = MSG_ID(GAPC, 0x13), GAPC_BOND_CFM = MSG_ID(GAPC, 0x14), GAPC_BOND_IND = MSG_ID(GAPC, 0x15), GAPC_ENCRYPT_CMD = MSG_ID(GAPC, 0x16), GAPC_ENCRYPT_REQ_IND = MSG_ID(GAPC, 0x17), GAPC_ENCRYPT_CFM = MSG_ID(GAPC, 0x18), GAPC_ENCRYPT_IND = MSG_ID(GAPC, 0x19), GAPC_SECURITY_CMD = MSG_ID(GAPC, 0x1A), GAPC_SECURITY_IND = MSG_ID(GAPC, 0x1B), GAPC_SIGN_COUNTER_IND = MSG_ID(GAPC, 0x1C), GAPC_CON_CHANNEL_MAP_IND = MSG_ID(GAPC, 0x1D), GAPC_SEC_REQ_TIMEOUT_IND = MSG_ID(GAPC, 0x1E), GAPC_SET_LE_PING_TO_CMD = MSG_ID(GAPC, 0x28), GAPC_LE_PING_TO_VAL_IND = MSG_ID(GAPC, 0x29), GAPC_LE_PING_TO_IND = MSG_ID(GAPC, 0x2A), GAPC_SET_LE_PKT_SIZE_CMD = MSG_ID(GAPC, 0x2B), GAPC_LE_PKT_SIZE_IND = MSG_ID(GAPC, 0x2C), GAPC_KEY_PRESS_NOTIFICATION_CMD = MSG_ID(GAPC, 0x2D), GAPC_KEY_PRESS_NOTIFICATION_IND = MSG_ID(GAPC, 0x2E), GAPC_SET_PHY_CMD = MSG_ID(GAPC, 0x2F), GAPC_LE_PHY_IND = MSG_ID(GAPC, 0x30), GAPC_CHAN_SEL_ALGO_IND = MSG_ID(GAPC, 0x31), GAPC_SET_PREF_SLAVE_LATENCY_CMD = MSG_ID(GAPC, 0x32), GAPC_SET_PREF_SLAVE_EVT_DUR_CMD = MSG_ID(GAPC, 0x33), GAPC_UNKNOWN_MSG_IND = MSG_ID(GAPC, 0x34), GAPC_PER_ADV_SYNC_TRANS_CMD = MSG_ID(GAPC, 0x35), GAPC_CTE_TX_CFG_CMD = MSG_ID(GAPC, 0x38), GAPC_CTE_RX_CFG_CMD = MSG_ID(GAPC, 0x39), GAPC_CTE_REQ_CTRL_CMD = MSG_ID(GAPC, 0x3A), GAPC_CTE_RSP_CTRL_CMD = MSG_ID(GAPC, 0x3B), GAPC_CTE_IQ_REPORT_IND = MSG_ID(GAPC, 0x3C), GAPC_READ_LOCAL_TX_PWR_CMD = MSG_ID(GAPC, 0x3D), GAPC_READ_REMOTE_TX_PWR_CMD = MSG_ID(GAPC, 0x3E), GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD = MSG_ID(GAPC, 0x3F), GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD = MSG_ID(GAPC, 0x40), GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD = MSG_ID(GAPC, 0x41), GAPC_READ_LOCAL_TX_PWR_IND = MSG_ID(GAPC, 0x42), GAPC_READ_REMOTE_TX_PWR_IND = MSG_ID(GAPC, 0x43), GAPC_TX_PWR_CHANGE_REPORT_IND = MSG_ID(GAPC, 0x44), GAPC_PATH_LOSS_THRESHOLD_REPORT_IND = MSG_ID(GAPC, 0x45), GAPC_RANGING_START_CMD = MSG_ID(GAPC, 0x46), GAPC_RANGING_IND = MSG_ID(GAPC, 0x47), GAPC_RANGING_SAMPLE_REPORT_IND = MSG_ID(GAPC, 0x48), GAPC_RANGING_CMP_IND = MSG_ID(GAPC, 0x49), GAPC_SIGN_CMD = MSG_ID(GAPC, 0xF0), GAPC_SIGN_IND = MSG_ID(GAPC, 0xF1), GAPC_PARAM_UPDATE_TO_IND = MSG_ID(GAPC, 0xF2), GAPC_SMP_TIMEOUT_TIMER_IND = MSG_ID(GAPC, 0xF3), GAPC_SMP_REP_ATTEMPTS_TIMER_IND = MSG_ID(GAPC, 0xF4) }
| GAPC_TASK Message ID. More...
enum | gapm_msg_id { GAPM_CMP_EVT = MSG_ID(GAPM, 0x00), GAPM_RESET_CMD = MSG_ID(GAPM, 0x02), GAPM_SET_DEV_CONFIG_CMD = MSG_ID(GAPM, 0x04), GAPM_SET_CHANNEL_MAP_CMD = MSG_ID(GAPM, 0x05), GAPM_GET_DEV_INFO_CMD = MSG_ID(GAPM, 0x06), GAPM_DEV_VERSION_IND = MSG_ID(GAPM, 0x07), GAPM_DEV_BDADDR_IND = MSG_ID(GAPM, 0x08), GAPM_DEV_ADV_TX_POWER_IND = MSG_ID(GAPM, 0x09), GAPM_DBG_MEM_INFO_IND = MSG_ID(GAPM, 0x0A), GAPM_ANTENNA_INF_IND = MSG_ID(GAPM, 0x0B), GAPM_RESOLV_ADDR_CMD = MSG_ID(GAPM, 0x14), GAPM_ADDR_SOLVED_IND = MSG_ID(GAPM, 0x15), GAPM_GEN_RAND_ADDR_CMD = MSG_ID(GAPM, 0x16), GAPM_USE_ENC_BLOCK_CMD = MSG_ID(GAPM, 0x17), GAPM_USE_ENC_BLOCK_IND = MSG_ID(GAPM, 0x18), GAPM_GEN_RAND_NB_CMD = MSG_ID(GAPM, 0x19), GAPM_GEN_RAND_NB_IND = MSG_ID(GAPM, 0x1A), GAPM_PROFILE_TASK_ADD_CMD = MSG_ID(GAPM, 0x1B), GAPM_PROFILE_ADDED_IND = MSG_ID(GAPM, 0x1C), GAPM_UNKNOWN_TASK_IND = MSG_ID(GAPM, 0x1D), GAPM_SUGG_DFLT_DATA_LEN_IND = MSG_ID(GAPM, 0x1E), GAPM_MAX_DATA_LEN_IND = MSG_ID(GAPM, 0x1F), GAPM_RAL_ADDR_IND = MSG_ID(GAPM, 0x22), GAPM_SET_IRK_CMD = MSG_ID(GAPM, 0x23), GAPM_LEPSM_REGISTER_CMD = MSG_ID(GAPM, 0x24), GAPM_LEPSM_UNREGISTER_CMD = MSG_ID(GAPM, 0x25), GAPM_LE_TEST_MODE_CTRL_CMD = MSG_ID(GAPM, 0x26), GAPM_LE_TEST_END_IND = MSG_ID(GAPM, 0x27), GAPM_LE_TEST_IQ_REPORT_IND = MSG_ID(GAPM, 0x2D), GAPM_ISO_STAT_IND = MSG_ID(GAPM, 0x28), GAPM_GEN_DH_KEY_CMD = MSG_ID(GAPM, 0x29), GAPM_GEN_DH_KEY_IND = MSG_ID(GAPM, 0x2A), GAPM_GET_PUB_KEY_CMD = MSG_ID(GAPM, 0x2B), GAPM_PUB_KEY_IND = MSG_ID(GAPM, 0x2C), GAPM_GET_RAL_ADDR_CMD = MSG_ID(GAPM, 0x90), GAPM_LIST_SET_CMD = MSG_ID(GAPM, 0x91), GAPM_LIST_SIZE_IND = MSG_ID(GAPM, 0x92), GAPM_ACTIVITY_CREATE_CMD = MSG_ID(GAPM, 0xA0), GAPM_ACTIVITY_START_CMD = MSG_ID(GAPM, 0xA1), GAPM_ACTIVITY_STOP_CMD = MSG_ID(GAPM, 0xA2), GAPM_ACTIVITY_DELETE_CMD = MSG_ID(GAPM, 0xA3), GAPM_ACTIVITY_CREATED_IND = MSG_ID(GAPM, 0xA4), GAPM_ACTIVITY_STOPPED_IND = MSG_ID(GAPM, 0xA5), GAPM_SET_ADV_DATA_CMD = MSG_ID(GAPM, 0xA6), GAPM_EXT_ADV_REPORT_IND = MSG_ID(GAPM, 0xA7), GAPM_SCAN_REQUEST_IND = MSG_ID(GAPM, 0xA8), GAPM_SYNC_ESTABLISHED_IND = MSG_ID(GAPM, 0xA9), GAPM_MAX_ADV_DATA_LEN_IND = MSG_ID(GAPM, 0xAA), GAPM_NB_ADV_SETS_IND = MSG_ID(GAPM, 0xAB), GAPM_DEV_TX_PWR_IND = MSG_ID(GAPM, 0xAC), GAPM_DEV_RF_PATH_COMP_IND = MSG_ID(GAPM, 0xAD), GAPM_UNKNOWN_MSG_IND = MSG_ID(GAPM, 0xAE), GAPM_PER_ADV_REPORT_CTRL_CMD = MSG_ID(GAPM, 0xAF), GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD = MSG_ID(GAPM, 0xB0), GAPM_PER_ADV_IQ_REPORT_IND = MSG_ID(GAPM, 0xB1), GAPM_PER_ADV_CTE_TX_CTL_CMD = MSG_ID(GAPM, 0xB2), GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD = MSG_ID(GAPM, 0xB3), GAPM_DBG_IQGEN_CFG_CMD = MSG_ID(GAPM, 0x50), GAPM_UNKNOWN_TASK_MSG = MSG_ID(GAPM, 0xF0), GAPM_ADDR_RENEW_TO_IND = MSG_ID(GAPM, 0xF1), GAPM_AUTO_CONN_TO_IND = MSG_ID(GAPM, 0xF2), GAPM_ADDR_RENEW_CMD = MSG_ID(GAPM, 0xF3), GAPM_PUBLIC_ADDR_SET_CMD = MSG_ID(GAPM, 0xF4), GAPM_SET_GDX_RANGING_PARAM_CMD = MSG_ID(GAPM, 0xF5), GAPM_ADV_SCAN_MONITOR_EVT_REPORT_IND = MSG_ID(GAPM, 0xF6) }
| GAPM_TASK Message ID. More...
enum | gattc_msg_id { GATTC_CMP_EVT = TASK_FIRST_MSG(TASK_ID_GATTC), GATTC_EXC_MTU_CMD, GATTC_MTU_CHANGED_IND, GATTC_DISC_CMD, GATTC_DISC_SVC_IND, GATTC_DISC_SVC_INCL_IND, GATTC_DISC_CHAR_IND, GATTC_DISC_CHAR_DESC_IND, GATTC_READ_CMD, GATTC_READ_IND, GATTC_WRITE_CMD, GATTC_EXECUTE_WRITE_CMD, GATTC_EVENT_IND, GATTC_EVENT_REQ_IND, GATTC_EVENT_CFM, GATTC_REG_TO_PEER_EVT_CMD, GATTC_SEND_EVT_CMD, GATTC_SEND_SVC_CHANGED_CMD, GATTC_SVC_CHANGED_CFG_IND, GATTC_READ_REQ_IND, GATTC_READ_CFM, GATTC_WRITE_REQ_IND, GATTC_WRITE_CFM, GATTC_ATT_INFO_REQ_IND, GATTC_ATT_INFO_CFM, GATTC_SDP_SVC_DISC_CMD, GATTC_SDP_SVC_IND, GATTC_TRANSACTION_TO_ERROR_IND, GATTC_UNKNOWN_MSG_IND, GATTC_CLIENT_RTX_IND, GATTC_SERVER_RTX_IND }
| GATTC_TASK Message ID. More...
enum | l2cc_msg_id { L2CC_CMP_EVT = TASK_FIRST_MSG(TASK_ID_L2CC) + L2CC_NB_DEPRECATED_MSG, L2CC_LECB_CONNECT_CMD, L2CC_LECB_CONNECT_REQ_IND, L2CC_LECB_CONNECT_CFM, L2CC_LECB_CONNECT_IND, L2CC_LECB_DISCONNECT_CMD, L2CC_LECB_DISCONNECT_IND, L2CC_LECB_ADD_CMD, L2CC_LECB_ADD_IND, L2CC_LECB_SDU_SEND_CMD, L2CC_LECB_SDU_RECV_IND, L2CC_UNKNOWN_MSG_IND, L2CC_DBG_PDU_SEND_CMD, L2CC_DBG_PDU_RECV_IND, L2CC_PDU_SEND_CMD, L2CC_PDU_RECV_IND, L2CC_SIGNALING_TRANS_TO_IND }
| GATTC_TASK Message ID. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ gapc_msg_id

enum gapc_msg_id

GAPC_TASK Message ID.

Enumerator
GAPC_CMP_EVT |
GAPC_CONNECTION_REQ_IND |
GAPC_CONNECTION_CFM |
GAPC_DISCONNECT_IND |
GAPC_DISCONNECT_CMD |
GAPC_GET_INFO_CMD |
GAPC_PEER_ATT_INFO_IND |
GAPC_PEER_VERSION_IND |
GAPC_PEER_FEATURES_IND |
GAPC_CON_RSSI_IND |
GAPC_GET_DEV_INFO_REQ_IND |
GAPC_GET_DEV_INFO_CFM |
GAPC_SET_DEV_INFO_REQ_IND |
GAPC_SET_DEV_INFO_CFM |
GAPC_PARAM_UPDATE_CMD |
GAPC_PARAM_UPDATE_REQ_IND |
GAPC_PARAM_UPDATE_CFM |
GAPC_PARAM_UPDATED_IND |
GAPC_BOND_CMD |
GAPC_BOND_REQ_IND |
GAPC_BOND_CFM |
GAPC_BOND_IND |
GAPC_ENCRYPT_CMD |
GAPC_ENCRYPT_REQ_IND |
GAPC_ENCRYPT_CFM |
GAPC_ENCRYPT_IND |
GAPC_SECURITY_CMD |
GAPC_SECURITY_IND |
GAPC_SIGN_COUNTER_IND |
GAPC_CON_CHANNEL_MAP_IND |
GAPC_SEC_REQ_TIMEOUT_IND |
GAPC_SET_LE_PING_TO_CMD |
GAPC_LE_PING_TO_VAL_IND |
GAPC_LE_PING_TO_IND |
GAPC_SET_LE_PKT_SIZE_CMD |
GAPC_LE_PKT_SIZE_IND |
GAPC_KEY_PRESS_NOTIFICATION_CMD |
GAPC_KEY_PRESS_NOTIFICATION_IND |
GAPC_SET_PHY_CMD |
GAPC_LE_PHY_IND |
GAPC_CHAN_SEL_ALGO_IND |
GAPC_SET_PREF_SLAVE_LATENCY_CMD |
GAPC_SET_PREF_SLAVE_EVT_DUR_CMD |
GAPC_UNKNOWN_MSG_IND |
GAPC_PER_ADV_SYNC_TRANS_CMD |
GAPC_CTE_TX_CFG_CMD |
GAPC_CTE_RX_CFG_CMD |
GAPC_CTE_REQ_CTRL_CMD |
GAPC_CTE_RSP_CTRL_CMD |
GAPC_CTE_IQ_REPORT_IND |
GAPC_READ_LOCAL_TX_PWR_CMD |
GAPC_READ_REMOTE_TX_PWR_CMD |
GAPC_SET_PATH_LOSS_REPORTING_PARAM_CMD |
GAPC_SET_PATH_LOSS_REPORTING_ENABLE_CMD |
GAPC_SET_TX_PWR_REPORTING_ENABLE_CMD |
GAPC_READ_LOCAL_TX_PWR_IND |
GAPC_READ_REMOTE_TX_PWR_IND |
GAPC_TX_PWR_CHANGE_REPORT_IND |
GAPC_PATH_LOSS_THRESHOLD_REPORT_IND |
GAPC_RANGING_START_CMD |
GAPC_RANGING_IND |
GAPC_RANGING_SAMPLE_REPORT_IND |
GAPC_RANGING_CMP_IND |
GAPC_SIGN_CMD |
GAPC_SIGN_IND |
GAPC_PARAM_UPDATE_TO_IND |
GAPC_SMP_TIMEOUT_TIMER_IND |
GAPC_SMP_REP_ATTEMPTS_TIMER_IND |

Definition at line 664 of file ble_id.h.

## ◆ gapm_msg_id

enum gapm_msg_id

GAPM_TASK Message ID.

Enumerator
GAPM_CMP_EVT |
GAPM_RESET_CMD |
GAPM_SET_DEV_CONFIG_CMD |
GAPM_SET_CHANNEL_MAP_CMD |
GAPM_GET_DEV_INFO_CMD |
GAPM_DEV_VERSION_IND |
GAPM_DEV_BDADDR_IND |
GAPM_DEV_ADV_TX_POWER_IND |
GAPM_DBG_MEM_INFO_IND |
GAPM_ANTENNA_INF_IND |
GAPM_RESOLV_ADDR_CMD |
GAPM_ADDR_SOLVED_IND |
GAPM_GEN_RAND_ADDR_CMD |
GAPM_USE_ENC_BLOCK_CMD |
GAPM_USE_ENC_BLOCK_IND |
GAPM_GEN_RAND_NB_CMD |
GAPM_GEN_RAND_NB_IND |
GAPM_PROFILE_TASK_ADD_CMD |
GAPM_PROFILE_ADDED_IND |
GAPM_UNKNOWN_TASK_IND |
GAPM_SUGG_DFLT_DATA_LEN_IND |
GAPM_MAX_DATA_LEN_IND |
GAPM_RAL_ADDR_IND |
GAPM_SET_IRK_CMD |
GAPM_LEPSM_REGISTER_CMD |
GAPM_LEPSM_UNREGISTER_CMD |
GAPM_LE_TEST_MODE_CTRL_CMD |
GAPM_LE_TEST_END_IND |
GAPM_LE_TEST_IQ_REPORT_IND |
GAPM_ISO_STAT_IND |
GAPM_GEN_DH_KEY_CMD |
GAPM_GEN_DH_KEY_IND |
GAPM_GET_PUB_KEY_CMD |
GAPM_PUB_KEY_IND |
GAPM_GET_RAL_ADDR_CMD |
GAPM_LIST_SET_CMD |
GAPM_LIST_SIZE_IND |
GAPM_ACTIVITY_CREATE_CMD |
GAPM_ACTIVITY_START_CMD |
GAPM_ACTIVITY_STOP_CMD |
GAPM_ACTIVITY_DELETE_CMD |
GAPM_ACTIVITY_CREATED_IND |
GAPM_ACTIVITY_STOPPED_IND |
GAPM_SET_ADV_DATA_CMD |
GAPM_EXT_ADV_REPORT_IND |
GAPM_SCAN_REQUEST_IND |
GAPM_SYNC_ESTABLISHED_IND |
GAPM_MAX_ADV_DATA_LEN_IND |
GAPM_NB_ADV_SETS_IND |
GAPM_DEV_TX_PWR_IND |
GAPM_DEV_RF_PATH_COMP_IND |
GAPM_UNKNOWN_MSG_IND |
GAPM_PER_ADV_REPORT_CTRL_CMD |
GAPM_PER_SYNC_IQ_SAMPLING_CTRL_CMD |
GAPM_PER_ADV_IQ_REPORT_IND |
GAPM_PER_ADV_CTE_TX_CTL_CMD |
GAPM_PER_ADV_CTE_TX_PARAM_SET_CMD |
GAPM_DBG_IQGEN_CFG_CMD |
GAPM_UNKNOWN_TASK_MSG |
GAPM_ADDR_RENEW_TO_IND |
GAPM_AUTO_CONN_TO_IND |
GAPM_ADDR_RENEW_CMD |
GAPM_PUBLIC_ADDR_SET_CMD |
GAPM_SET_GDX_RANGING_PARAM_CMD |
GAPM_ADV_SCAN_MONITOR_EVT_REPORT_IND |

Definition at line 739 of file ble_id.h.

## ◆ gattc_msg_id

enum gattc_msg_id

GATTC_TASK Message ID.

Enumerator
GATTC_CMP_EVT |
GATTC_EXC_MTU_CMD |
GATTC_MTU_CHANGED_IND |
GATTC_DISC_CMD |
GATTC_DISC_SVC_IND |
GATTC_DISC_SVC_INCL_IND |
GATTC_DISC_CHAR_IND |
GATTC_DISC_CHAR_DESC_IND |
GATTC_READ_CMD |
GATTC_READ_IND |
GATTC_WRITE_CMD |
GATTC_EXECUTE_WRITE_CMD |
GATTC_EVENT_IND |
GATTC_EVENT_REQ_IND |
GATTC_EVENT_CFM |
GATTC_REG_TO_PEER_EVT_CMD |
GATTC_SEND_EVT_CMD |
GATTC_SEND_SVC_CHANGED_CMD |
GATTC_SVC_CHANGED_CFG_IND |
GATTC_READ_REQ_IND |
GATTC_READ_CFM |
GATTC_WRITE_REQ_IND |
GATTC_WRITE_CFM |
GATTC_ATT_INFO_REQ_IND |
GATTC_ATT_INFO_CFM |
GATTC_SDP_SVC_DISC_CMD |
GATTC_SDP_SVC_IND |
GATTC_TRANSACTION_TO_ERROR_IND |
GATTC_UNKNOWN_MSG_IND |
GATTC_CLIENT_RTX_IND |
GATTC_SERVER_RTX_IND |

Definition at line 811 of file ble_id.h.

## ◆ hci_evt_code

enum hci_evt_code

Enumerator
HCI_INQ_CMP_EVT_CODE |
HCI_INQ_RES_EVT_CODE |
HCI_CON_CMP_EVT_CODE |
HCI_CON_REQ_EVT_CODE |
HCI_DISC_CMP_EVT_CODE |
HCI_AUTH_CMP_EVT_CODE |
HCI_REM_NAME_REQ_CMP_EVT_CODE |
HCI_ENC_CHG_EVT_CODE |
HCI_CHG_CON_LK_CMP_EVT_CODE |
HCI_MASTER_LK_CMP_EVT_CODE |
HCI_RD_REM_SUPP_FEATS_CMP_EVT_CODE |
HCI_RD_REM_VER_INFO_CMP_EVT_CODE |
HCI_QOS_SETUP_CMP_EVT_CODE |
HCI_CMD_CMP_EVT_CODE |
HCI_CMD_STATUS_EVT_CODE |
HCI_HW_ERR_EVT_CODE |
HCI_FLUSH_OCCURRED_EVT_CODE |
HCI_ROLE_CHG_EVT_CODE |
HCI_NB_CMP_PKTS_EVT_CODE |
HCI_MODE_CHG_EVT_CODE |
HCI_RETURN_LINK_KEYS_EVT_CODE |
HCI_PIN_CODE_REQ_EVT_CODE |
HCI_LK_REQ_EVT_CODE |
HCI_LK_NOTIF_EVT_CODE |
HCI_DATA_BUF_OVFLW_EVT_CODE |
HCI_MAX_SLOT_CHG_EVT_CODE |
HCI_RD_CLK_OFF_CMP_EVT_CODE |
HCI_CON_PKT_TYPE_CHG_EVT_CODE |
HCI_QOS_VIOL_EVT_CODE |
HCI_PAGE_SCAN_REPET_MODE_CHG_EVT_CODE |
HCI_FLOW_SPEC_CMP_EVT_CODE |
HCI_INQ_RES_WITH_RSSI_EVT_CODE |
HCI_RD_REM_EXT_FEATS_CMP_EVT_CODE |
HCI_SYNC_CON_CMP_EVT_CODE |
HCI_SYNC_CON_CHG_EVT_CODE |
HCI_SNIFF_SUB_EVT_CODE |
HCI_EXT_INQ_RES_EVT_CODE |
HCI_ENC_KEY_REFRESH_CMP_EVT_CODE |
HCI_IO_CAP_REQ_EVT_CODE |
HCI_IO_CAP_RSP_EVT_CODE |
HCI_USER_CFM_REQ_EVT_CODE |
HCI_USER_PASSKEY_REQ_EVT_CODE |
HCI_REM_OOB_DATA_REQ_EVT_CODE |
HCI_SP_CMP_EVT_CODE |
HCI_LINK_SUPV_TO_CHG_EVT_CODE |
HCI_ENH_FLUSH_CMP_EVT_CODE |
HCI_USER_PASSKEY_NOTIF_EVT_CODE |
HCI_KEYPRESS_NOTIF_EVT_CODE |
HCI_REM_HOST_SUPP_FEATS_NOTIF_EVT_CODE |
HCI_LE_META_EVT_CODE |
HCI_MAX_EVT_MSK_PAGE_1_CODE |
HCI_SYNC_TRAIN_CMP_EVT_CODE |
HCI_SYNC_TRAIN_REC_EVT_CODE |
HCI_CON_SLV_BCST_REC_EVT_CODE |
HCI_CON_SLV_BCST_TO_EVT_CODE |
HCI_TRUNC_PAGE_CMP_EVT_CODE |
HCI_SLV_PAGE_RSP_TO_EVT_CODE |
HCI_CON_SLV_BCST_CH_MAP_CHG_EVT_CODE |
HCI_AUTH_PAYL_TO_EXP_EVT_CODE |
HCI_SAM_STATUS_CHANGE_EVT_CODE |
HCI_MAX_EVT_MSK_PAGE_2_CODE |
HCI_DBG_META_EVT_CODE |

Definition at line 429 of file ble_id.h.

## ◆ hci_le_evt_subcode

enum hci_le_evt_subcode

Enumerator
HCI_LE_CON_CMP_EVT_SUBCODE |
HCI_LE_ADV_REPORT_EVT_SUBCODE |
HCI_LE_CON_UPDATE_CMP_EVT_SUBCODE |
HCI_LE_RD_REM_FEATS_CMP_EVT_SUBCODE |
HCI_LE_LTK_REQUEST_EVT_SUBCODE |
HCI_LE_REM_CON_PARAM_REQ_EVT_SUBCODE |
HCI_LE_DATA_LEN_CHG_EVT_SUBCODE |
HCI_LE_RD_LOC_P256_PUB_KEY_CMP_EVT_SUBCODE |
HCI_LE_GEN_DHKEY_CMP_EVT_SUBCODE |
HCI_LE_ENH_CON_CMP_EVT_SUBCODE |
HCI_LE_DIR_ADV_REP_EVT_SUBCODE |
HCI_LE_PHY_UPD_CMP_EVT_SUBCODE |
HCI_LE_EXT_ADV_REPORT_EVT_SUBCODE |
HCI_LE_PER_ADV_SYNC_EST_EVT_SUBCODE |
HCI_LE_PER_ADV_REPORT_EVT_SUBCODE |
HCI_LE_PER_ADV_SYNC_LOST_EVT_SUBCODE |
HCI_LE_SCAN_TIMEOUT_EVT_SUBCODE |
HCI_LE_ADV_SET_TERMINATED_EVT_SUBCODE |
HCI_LE_SCAN_REQ_RCVD_EVT_SUBCODE |
HCI_LE_CH_SEL_ALGO_EVT_SUBCODE |
HCI_LE_CONLESS_IQ_REPORT_EVT_SUBCODE |
HCI_LE_CON_IQ_REPORT_EVT_SUBCODE |
HCI_LE_CTE_REQ_FAILED_EVT_SUBCODE |
HCI_LE_PER_ADV_SYNC_TRANSF_REC_EVT_SUBCODE |
HCI_LE_CIS_ESTABLISHED_EVT_SUBCODE |
HCI_LE_CIS_REQUEST_EVT_SUBCODE |
HCI_LE_CREATE_BIG_CMP_EVT_SUBCODE |
HCI_LE_TERMINATE_BIG_CMP_EVT_SUBCODE |
HCI_LE_BIG_SYNC_ESTABLISHED_EVT_SUBCODE |
HCI_LE_BIG_SYNC_LOST_EVT_SUBCODE |
HCI_LE_REQ_PEER_SCA_CMP_EVT_SUBCODE |
HCI_LE_PATH_LOSS_THRESHOLD_EVT_SUBCODE |
HCI_LE_TX_POWER_REPORTING_EVT_SUBCODE |
HCI_LE_BIG_INFO_ADV_REPORT_EVT_SUBCODE |
HCI_LE_RANGING_IND_EVT_SUBCODE |
HCI_LE_RANGING_SAMPLE_REPORT_EVT_SUBCODE |
HCI_LE_RANGING_CMP_EVT_SUBCODE |

Definition at line 495 of file ble_id.h.

## ◆ hci_msg_id

enum hci_msg_id

HCI task Message ID.

Enumerator
HCI_MSG_ID_FIRST |
HCI_CMD_CMP_EVENT |
HCI_CMD_STAT_EVENT |
HCI_EVENT |
HCI_LE_EVENT |
HCI_COMMAND |
HCI_ACL_DATA |
HCI_VS_EVENT |
HCI_MSG_ID_LAST |

Definition at line 611 of file ble_id.h.

## ◆ hci_opcode

enum hci_opcode

Enumerator
HCI_NO_OPERATION_CMD_OPCODE |
HCI_INQ_CMD_OPCODE |
HCI_INQ_CANCEL_CMD_OPCODE |
HCI_PER_INQ_MODE_CMD_OPCODE |
HCI_EXIT_PER_INQ_MODE_CMD_OPCODE |
HCI_CREATE_CON_CMD_OPCODE |
HCI_DISCONNECT_CMD_OPCODE |
HCI_CREATE_CON_CANCEL_CMD_OPCODE |
HCI_ACCEPT_CON_REQ_CMD_OPCODE |
HCI_REJECT_CON_REQ_CMD_OPCODE |
HCI_LK_REQ_REPLY_CMD_OPCODE |
HCI_LK_REQ_NEG_REPLY_CMD_OPCODE |
HCI_PIN_CODE_REQ_REPLY_CMD_OPCODE |
HCI_PIN_CODE_REQ_NEG_REPLY_CMD_OPCODE |
HCI_CHG_CON_PKT_TYPE_CMD_OPCODE |
HCI_AUTH_REQ_CMD_OPCODE |
HCI_SET_CON_ENC_CMD_OPCODE |
HCI_CHG_CON_LK_CMD_OPCODE |
HCI_MASTER_LK_CMD_OPCODE |
HCI_REM_NAME_REQ_CMD_OPCODE |
HCI_REM_NAME_REQ_CANCEL_CMD_OPCODE |
HCI_RD_REM_SUPP_FEATS_CMD_OPCODE |
HCI_RD_REM_EXT_FEATS_CMD_OPCODE |
HCI_RD_REM_VER_INFO_CMD_OPCODE |
HCI_RD_CLK_OFF_CMD_OPCODE |
HCI_RD_LMP_HDL_CMD_OPCODE |
HCI_SETUP_SYNC_CON_CMD_OPCODE |
HCI_ACCEPT_SYNC_CON_REQ_CMD_OPCODE |
HCI_REJECT_SYNC_CON_REQ_CMD_OPCODE |
HCI_IO_CAP_REQ_REPLY_CMD_OPCODE |
HCI_USER_CFM_REQ_REPLY_CMD_OPCODE |
HCI_USER_CFM_REQ_NEG_REPLY_CMD_OPCODE |
HCI_USER_PASSKEY_REQ_REPLY_CMD_OPCODE |
HCI_USER_PASSKEY_REQ_NEG_REPLY_CMD_OPCODE |
HCI_REM_OOB_DATA_REQ_REPLY_CMD_OPCODE |
HCI_REM_OOB_DATA_REQ_NEG_REPLY_CMD_OPCODE |
HCI_IO_CAP_REQ_NEG_REPLY_CMD_OPCODE |
HCI_ENH_SETUP_SYNC_CON_CMD_OPCODE |
HCI_ENH_ACCEPT_SYNC_CON_CMD_OPCODE |
HCI_TRUNC_PAGE_CMD_OPCODE |
HCI_TRUNC_PAGE_CAN_CMD_OPCODE |
HCI_SET_CON_SLV_BCST_CMD_OPCODE |
HCI_SET_CON_SLV_BCST_REC_CMD_OPCODE |
HCI_START_SYNC_TRAIN_CMD_OPCODE |
HCI_REC_SYNC_TRAIN_CMD_OPCODE |
HCI_REM_OOB_EXT_DATA_REQ_REPLY_CMD_OPCODE |
HCI_HOLD_MODE_CMD_OPCODE |
HCI_SNIFF_MODE_CMD_OPCODE |
HCI_EXIT_SNIFF_MODE_CMD_OPCODE |
HCI_PARK_STATE_CMD_OPCODE |
HCI_EXIT_PARK_STATE_CMD_OPCODE |
HCI_QOS_SETUP_CMD_OPCODE |
HCI_ROLE_DISCOVERY_CMD_OPCODE |
HCI_SWITCH_ROLE_CMD_OPCODE |
HCI_RD_LINK_POL_STG_CMD_OPCODE |
HCI_WR_LINK_POL_STG_CMD_OPCODE |
HCI_RD_DFT_LINK_POL_STG_CMD_OPCODE |
HCI_WR_DFT_LINK_POL_STG_CMD_OPCODE |
HCI_FLOW_SPEC_CMD_OPCODE |
HCI_SNIFF_SUB_CMD_OPCODE |
HCI_SET_EVT_MASK_CMD_OPCODE |
HCI_RESET_CMD_OPCODE |
HCI_SET_EVT_FILTER_CMD_OPCODE |
HCI_FLUSH_CMD_OPCODE |
HCI_RD_PIN_TYPE_CMD_OPCODE |
HCI_WR_PIN_TYPE_CMD_OPCODE |
HCI_CREATE_NEW_UNIT_KEY_CMD_OPCODE |
HCI_RD_STORED_LK_CMD_OPCODE |
HCI_WR_STORED_LK_CMD_OPCODE |
HCI_DEL_STORED_LK_CMD_OPCODE |
HCI_WR_LOCAL_NAME_CMD_OPCODE |
HCI_RD_LOCAL_NAME_CMD_OPCODE |
HCI_RD_CON_ACCEPT_TO_CMD_OPCODE |
HCI_WR_CON_ACCEPT_TO_CMD_OPCODE |
HCI_RD_PAGE_TO_CMD_OPCODE |
HCI_WR_PAGE_TO_CMD_OPCODE |
HCI_RD_SCAN_EN_CMD_OPCODE |
HCI_WR_SCAN_EN_CMD_OPCODE |
HCI_RD_PAGE_SCAN_ACT_CMD_OPCODE |
HCI_WR_PAGE_SCAN_ACT_CMD_OPCODE |
HCI_RD_INQ_SCAN_ACT_CMD_OPCODE |
HCI_WR_INQ_SCAN_ACT_CMD_OPCODE |
HCI_RD_AUTH_EN_CMD_OPCODE |
HCI_WR_AUTH_EN_CMD_OPCODE |
HCI_RD_CLASS_OF_DEV_CMD_OPCODE |
HCI_WR_CLASS_OF_DEV_CMD_OPCODE |
HCI_RD_VOICE_STG_CMD_OPCODE |
HCI_WR_VOICE_STG_CMD_OPCODE |
HCI_RD_AUTO_FLUSH_TO_CMD_OPCODE |
HCI_WR_AUTO_FLUSH_TO_CMD_OPCODE |
HCI_RD_NB_BDCST_RETX_CMD_OPCODE |
HCI_WR_NB_BDCST_RETX_CMD_OPCODE |
HCI_RD_HOLD_MODE_ACTIVITY_CMD_OPCODE |
HCI_WR_HOLD_MODE_ACTIVITY_CMD_OPCODE |
HCI_RD_TX_PWR_LVL_CMD_OPCODE |
HCI_RD_SYNC_FLOW_CTRL_EN_CMD_OPCODE |
HCI_WR_SYNC_FLOW_CTRL_EN_CMD_OPCODE |
HCI_SET_CTRL_TO_HOST_FLOW_CTRL_CMD_OPCODE |
HCI_HOST_BUF_SIZE_CMD_OPCODE |
HCI_HOST_NB_CMP_PKTS_CMD_OPCODE |
HCI_RD_LINK_SUPV_TO_CMD_OPCODE |
HCI_WR_LINK_SUPV_TO_CMD_OPCODE |
HCI_RD_NB_SUPP_IAC_CMD_OPCODE |
HCI_RD_CURR_IAC_LAP_CMD_OPCODE |
HCI_WR_CURR_IAC_LAP_CMD_OPCODE |
HCI_SET_AFH_HOST_CH_CLASS_CMD_OPCODE |
HCI_RD_INQ_SCAN_TYPE_CMD_OPCODE |
HCI_WR_INQ_SCAN_TYPE_CMD_OPCODE |
HCI_RD_INQ_MODE_CMD_OPCODE |
HCI_WR_INQ_MODE_CMD_OPCODE |
HCI_RD_PAGE_SCAN_TYPE_CMD_OPCODE |
HCI_WR_PAGE_SCAN_TYPE_CMD_OPCODE |
HCI_RD_AFH_CH_ASSESS_MODE_CMD_OPCODE |
HCI_WR_AFH_CH_ASSESS_MODE_CMD_OPCODE |
HCI_RD_EXT_INQ_RSP_CMD_OPCODE |
HCI_WR_EXT_INQ_RSP_CMD_OPCODE |
HCI_REFRESH_ENC_KEY_CMD_OPCODE |
HCI_RD_SP_MODE_CMD_OPCODE |
HCI_WR_SP_MODE_CMD_OPCODE |
HCI_RD_LOC_OOB_DATA_CMD_OPCODE |
HCI_RD_INQ_RSP_TX_PWR_LVL_CMD_OPCODE |
HCI_WR_INQ_TX_PWR_LVL_CMD_OPCODE |
HCI_RD_DFT_ERR_DATA_REP_CMD_OPCODE |
HCI_WR_DFT_ERR_DATA_REP_CMD_OPCODE |
HCI_ENH_FLUSH_CMD_OPCODE |
HCI_SEND_KEYPRESS_NOTIF_CMD_OPCODE |
HCI_SET_EVT_MASK_PAGE_2_CMD_OPCODE |
HCI_RD_FLOW_CNTL_MODE_CMD_OPCODE |
HCI_WR_FLOW_CNTL_MODE_CMD_OPCODE |
HCI_RD_ENH_TX_PWR_LVL_CMD_OPCODE |
HCI_RD_LE_HOST_SUPP_CMD_OPCODE |
HCI_WR_LE_HOST_SUPP_CMD_OPCODE |
HCI_SET_MWS_CHANNEL_PARAMS_CMD_OPCODE |
HCI_SET_EXTERNAL_FRAME_CONFIG_CMD_OPCODE |
HCI_SET_MWS_SIGNALING_CMD_OPCODE |
HCI_SET_MWS_TRANSPORT_LAYER_CMD_OPCODE |
HCI_SET_MWS_SCAN_FREQ_TABLE_CMD_OPCODE |
HCI_SET_MWS_PATTERN_CONFIG_CMD_OPCODE |
HCI_SET_RES_LT_ADDR_CMD_OPCODE |
HCI_DEL_RES_LT_ADDR_CMD_OPCODE |
HCI_SET_CON_SLV_BCST_DATA_CMD_OPCODE |
HCI_RD_SYNC_TRAIN_PARAM_CMD_OPCODE |
HCI_WR_SYNC_TRAIN_PARAM_CMD_OPCODE |
HCI_RD_SEC_CON_HOST_SUPP_CMD_OPCODE |
HCI_WR_SEC_CON_HOST_SUPP_CMD_OPCODE |
HCI_RD_AUTH_PAYL_TO_CMD_OPCODE |
HCI_WR_AUTH_PAYL_TO_CMD_OPCODE |
HCI_RD_LOC_OOB_EXT_DATA_CMD_OPCODE |
HCI_RD_EXT_PAGE_TO_CMD_OPCODE |
HCI_WR_EXT_PAGE_TO_CMD_OPCODE |
HCI_RD_EXT_INQ_LEN_CMD_OPCODE |
HCI_WR_EXT_INQ_LEN_CMD_OPCODE |
HCI_SET_ECO_BASE_INTV_CMD_OPCODE |
HCI_CONFIG_DATA_PATH_CMD_OPCODE |
HCI_RD_LOCAL_VER_INFO_CMD_OPCODE |
HCI_RD_LOCAL_SUPP_CMDS_CMD_OPCODE |
HCI_RD_LOCAL_SUPP_FEATS_CMD_OPCODE |
HCI_RD_LOCAL_EXT_FEATS_CMD_OPCODE |
HCI_RD_BUF_SIZE_CMD_OPCODE |
HCI_RD_BD_ADDR_CMD_OPCODE |
HCI_RD_DATA_BLOCK_SIZE_CMD_OPCODE |
HCI_RD_LOCAL_SUPP_CODECS_CMD_OPCODE |
HCI_RD_LOCAL_SP_OPT_CMD_OPCODE |
HCI_RD_LOCAL_SUPP_CODECS_V2_CMD_OPCODE |
HCI_RD_LOCAL_SUPP_CODEC_CAP_CMD_OPCODE |
HCI_RD_LOCAL_SUPP_CTRL_DELAY_CMD_OPCODE |
HCI_RD_FAIL_CONTACT_CNT_CMD_OPCODE |
HCI_RST_FAIL_CONTACT_CNT_CMD_OPCODE |
HCI_RD_LINK_QUAL_CMD_OPCODE |
HCI_RD_RSSI_CMD_OPCODE |
HCI_RD_AFH_CH_MAP_CMD_OPCODE |
HCI_RD_CLK_CMD_OPCODE |
HCI_RD_ENC_KEY_SIZE_CMD_OPCODE |
HCI_GET_MWS_TRANSPORT_LAYER_CONFIG_CMD_OPCODE |
HCI_RD_LOOPBACK_MODE_CMD_OPCODE |
HCI_WR_LOOPBACK_MODE_CMD_OPCODE |
HCI_EN_DUT_MODE_CMD_OPCODE |
HCI_WR_SP_DBG_MODE_CMD_OPCODE |
HCI_WR_SEC_CON_TEST_MODE_CMD_OPCODE |
HCI_LE_SET_EVT_MASK_CMD_OPCODE | LE Commands Opcodes.
HCI_LE_RD_BUF_SIZE_CMD_OPCODE |
HCI_LE_RD_LOCAL_SUPP_FEATS_CMD_OPCODE |
HCI_LE_SET_RAND_ADDR_CMD_OPCODE |
HCI_LE_SET_ADV_PARAM_CMD_OPCODE |
HCI_LE_RD_ADV_CHNL_TX_PW_CMD_OPCODE |
HCI_LE_SET_ADV_DATA_CMD_OPCODE |
HCI_LE_SET_SCAN_RSP_DATA_CMD_OPCODE |
HCI_LE_SET_ADV_EN_CMD_OPCODE |
HCI_LE_SET_SCAN_PARAM_CMD_OPCODE |
HCI_LE_SET_SCAN_EN_CMD_OPCODE |
HCI_LE_CREATE_CON_CMD_OPCODE |
HCI_LE_CREATE_CON_CANCEL_CMD_OPCODE |
HCI_LE_RD_WLST_SIZE_CMD_OPCODE |
HCI_LE_CLEAR_WLST_CMD_OPCODE |
HCI_LE_ADD_DEV_TO_WLST_CMD_OPCODE |
HCI_LE_RMV_DEV_FROM_WLST_CMD_OPCODE |
HCI_LE_CON_UPDATE_CMD_OPCODE |
HCI_LE_SET_HOST_CH_CLASS_CMD_OPCODE |
HCI_LE_RD_CHNL_MAP_CMD_OPCODE |
HCI_LE_RD_REM_FEATS_CMD_OPCODE |
HCI_LE_ENC_CMD_OPCODE |
HCI_LE_RAND_CMD_OPCODE |
HCI_LE_EN_ENC_CMD_OPCODE |
HCI_LE_LTK_REQ_REPLY_CMD_OPCODE |
HCI_LE_LTK_REQ_NEG_REPLY_CMD_OPCODE |
HCI_LE_RD_SUPP_STATES_CMD_OPCODE |
HCI_LE_RX_TEST_V1_CMD_OPCODE |
HCI_LE_TX_TEST_V1_CMD_OPCODE |
HCI_LE_TEST_END_CMD_OPCODE |
HCI_LE_REM_CON_PARAM_REQ_REPLY_CMD_OPCODE |
HCI_LE_REM_CON_PARAM_REQ_NEG_REPLY_CMD_OPCODE |
HCI_LE_SET_DATA_LEN_CMD_OPCODE |
HCI_LE_RD_SUGGTED_DFT_DATA_LEN_CMD_OPCODE |
HCI_LE_WR_SUGGTED_DFT_DATA_LEN_CMD_OPCODE |
HCI_LE_RD_LOC_P256_PUB_KEY_CMD_OPCODE |
HCI_LE_GEN_DHKEY_V1_CMD_OPCODE |
HCI_LE_ADD_DEV_TO_RSLV_LIST_CMD_OPCODE |
HCI_LE_RMV_DEV_FROM_RSLV_LIST_CMD_OPCODE |
HCI_LE_CLEAR_RSLV_LIST_CMD_OPCODE |
HCI_LE_RD_RSLV_LIST_SIZE_CMD_OPCODE |
HCI_LE_RD_PEER_RSLV_ADDR_CMD_OPCODE |
HCI_LE_RD_LOC_RSLV_ADDR_CMD_OPCODE |
HCI_LE_SET_ADDR_RESOL_EN_CMD_OPCODE |
HCI_LE_SET_RSLV_PRIV_ADDR_TO_CMD_OPCODE |
HCI_LE_RD_MAX_DATA_LEN_CMD_OPCODE |
HCI_LE_RD_PHY_CMD_OPCODE |
HCI_LE_SET_DFT_PHY_CMD_OPCODE |
HCI_LE_SET_PHY_CMD_OPCODE |
HCI_LE_RX_TEST_V2_CMD_OPCODE |
HCI_LE_TX_TEST_V2_CMD_OPCODE |
HCI_LE_SET_ADV_SET_RAND_ADDR_CMD_OPCODE |
HCI_LE_SET_EXT_ADV_PARAM_CMD_OPCODE |
HCI_LE_SET_EXT_ADV_DATA_CMD_OPCODE |
HCI_LE_SET_EXT_SCAN_RSP_DATA_CMD_OPCODE |
HCI_LE_SET_EXT_ADV_EN_CMD_OPCODE |
HCI_LE_RD_MAX_ADV_DATA_LEN_CMD_OPCODE |
HCI_LE_RD_NB_SUPP_ADV_SETS_CMD_OPCODE |
HCI_LE_RMV_ADV_SET_CMD_OPCODE |
HCI_LE_CLEAR_ADV_SETS_CMD_OPCODE |
HCI_LE_SET_PER_ADV_PARAM_CMD_OPCODE |
HCI_LE_SET_PER_ADV_DATA_CMD_OPCODE |
HCI_LE_SET_PER_ADV_EN_CMD_OPCODE |
HCI_LE_SET_EXT_SCAN_PARAM_CMD_OPCODE |
HCI_LE_SET_EXT_SCAN_EN_CMD_OPCODE |
HCI_LE_EXT_CREATE_CON_CMD_OPCODE |
HCI_LE_PER_ADV_CREATE_SYNC_CMD_OPCODE |
HCI_LE_PER_ADV_CREATE_SYNC_CANCEL_CMD_OPCODE |
HCI_LE_PER_ADV_TERM_SYNC_CMD_OPCODE |
HCI_LE_ADD_DEV_TO_PER_ADV_LIST_CMD_OPCODE |
HCI_LE_RMV_DEV_FROM_PER_ADV_LIST_CMD_OPCODE |
HCI_LE_CLEAR_PER_ADV_LIST_CMD_OPCODE |
HCI_LE_RD_PER_ADV_LIST_SIZE_CMD_OPCODE |
HCI_LE_RD_TX_PWR_CMD_OPCODE |
HCI_LE_RD_RF_PATH_COMP_CMD_OPCODE |
HCI_LE_WR_RF_PATH_COMP_CMD_OPCODE |
HCI_LE_SET_PRIV_MODE_CMD_OPCODE |
HCI_LE_RX_TEST_V3_CMD_OPCODE |
HCI_LE_TX_TEST_V3_CMD_OPCODE |
HCI_LE_SET_CONLESS_CTE_TX_PARAM_CMD_OPCODE |
HCI_LE_SET_CONLESS_CTE_TX_EN_CMD_OPCODE |
HCI_LE_SET_CONLESS_IQ_SAMPL_EN_CMD_OPCODE |
HCI_LE_SET_CON_CTE_RX_PARAM_CMD_OPCODE |
HCI_LE_SET_CON_CTE_TX_PARAM_CMD_OPCODE |
HCI_LE_CON_CTE_REQ_EN_CMD_OPCODE |
HCI_LE_CON_CTE_RSP_EN_CMD_OPCODE |
HCI_LE_RD_ANTENNA_INF_CMD_OPCODE |
HCI_LE_SET_PER_ADV_REC_EN_CMD_OPCODE |
HCI_LE_PER_ADV_SYNC_TRANSF_CMD_OPCODE |
HCI_LE_PER_ADV_SET_INFO_TRANSF_CMD_OPCODE |
HCI_LE_SET_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE |
HCI_LE_SET_DFT_PER_ADV_SYNC_TRANSF_PARAM_CMD_OPCODE |
HCI_LE_GEN_DHKEY_V2_CMD_OPCODE |
HCI_LE_MOD_SLEEP_CLK_ACC_CMD_OPCODE |
HCI_LE_RD_BUF_SIZE_V2_CMD_OPCODE |
HCI_LE_RD_ISO_TX_SYNC_CMD_OPCODE |
HCI_LE_SET_CIG_PARAMS_CMD_OPCODE |
HCI_LE_SET_CIG_PARAMS_TEST_CMD_OPCODE |
HCI_LE_CREATE_CIS_CMD_OPCODE |
HCI_LE_REMOVE_CIG_CMD_OPCODE |
HCI_LE_ACCEPT_CIS_REQ_CMD_OPCODE |
HCI_LE_REJECT_CIS_REQ_CMD_OPCODE |
HCI_LE_CREATE_BIG_CMD_OPCODE |
HCI_LE_CREATE_BIG_TEST_CMD_OPCODE |
HCI_LE_TERMINATE_BIG_CMD_OPCODE |
HCI_LE_BIG_CREATE_SYNC_CMD_OPCODE |
HCI_LE_BIG_TERMINATE_SYNC_CMD_OPCODE |
HCI_LE_REQ_PEER_SCA_CMD_OPCODE |
HCI_LE_SETUP_ISO_DATA_PATH_CMD_OPCODE |
HCI_LE_REMOVE_ISO_DATA_PATH_CMD_OPCODE |
HCI_LE_ISO_TX_TEST_CMD_OPCODE |
HCI_LE_ISO_RX_TEST_CMD_OPCODE |
HCI_LE_ISO_READ_TEST_COUNTERS_CMD_OPCODE |
HCI_LE_ISO_TEST_END_CMD_OPCODE |
HCI_LE_SET_HOST_FEATURE_CMD_OPCODE |
HCI_LE_RD_ISO_LINK_QUALITY_CMD_OPCODE |
HCI_LE_ENH_RD_TX_PWR_LVL_CMD_OPCODE |
HCI_LE_RD_REMOTE_TX_PWR_LVL_CMD_OPCODE |
HCI_LE_SET_PATH_LOSS_REP_PARAM_CMD_OPCODE |
HCI_LE_SET_PATH_LOSS_REP_EN_CMD_OPCODE |
HCI_LE_SET_TX_POWER_REP_EN_CMD_OPCODE |
HCI_LE_TX_TEST_V4_CMD_OPCODE |
HCI_LE_SET_GDX_RANGING_PARAMS_CMD_OPCODE |
HCI_LE_START_RANGING_CMD_OPCODE |
HCI_PUBLIC_ADDR_SET_CMD_OPCODE |
HCI_LE_TIME_SYNC_EN_CMD_OPCODE |
HCI_DBG_RD_MEM_CMD_OPCODE | Debug commands - OGF = 0x3F (spec)
HCI_DBG_WR_MEM_CMD_OPCODE |
HCI_DBG_DEL_PAR_CMD_OPCODE |
HCI_DBG_ID_FLASH_CMD_OPCODE |
HCI_DBG_ER_FLASH_CMD_OPCODE |
HCI_DBG_WR_FLASH_CMD_OPCODE |
HCI_DBG_RD_FLASH_CMD_OPCODE |
HCI_DBG_RD_PAR_CMD_OPCODE |
HCI_DBG_WR_PAR_CMD_OPCODE |
HCI_DBG_WLAN_COEX_CMD_OPCODE |
HCI_DBG_WLAN_COEXTST_SCEN_CMD_OPCODE |
HCI_DBG_BT_SEND_LMP_CMD_OPCODE |
HCI_DBG_SET_LOCAL_CLOCK_CMD_OPCODE |
HCI_DBG_RD_KE_STATS_CMD_OPCODE |
HCI_DBG_PLF_RESET_CMD_OPCODE |
HCI_DBG_RD_MEM_INFO_CMD_OPCODE |
HCI_VS_SET_PREF_SLAVE_LATENCY_CMD_OPCODE |
HCI_VS_SET_PREF_SLAVE_EVT_DUR_CMD_OPCODE |
HCI_VS_SET_MAX_RX_SIZE_AND_TIME_CMD_OPCODE |
HCI_DBG_BLE_REG_RD_CMD_OPCODE |
HCI_DBG_BLE_REG_WR_CMD_OPCODE |
HCI_DBG_SEND_LLCP_CMD_OPCODE |
HCI_DBG_LLCP_DISCARD_CMD_OPCODE |
HCI_DBG_RF_REG_RD_CMD_OPCODE |
HCI_DBG_RF_REG_WR_CMD_OPCODE |
HCI_DBG_RF_SWITCH_CLK_CMD_OPCODE |
HCI_DBG_RF_WR_DATA_TX_CMD_OPCODE |
HCI_DBG_RF_RD_DATA_RX_CMD_OPCODE |
HCI_DBG_RF_CNTL_TX_CMD_OPCODE |

Definition at line 74 of file ble_id.h.

## ◆ hci_vs_dbg_evt_subcode

enum hci_vs_dbg_evt_subcode

Enumerator
HCI_VS_LE_GET_LINK_INFO_CMP_EVT_SUBCODE |
HCI_VS_LE_SNIFFER_DISC_CMP_EVT_SUBCODE |
HCI_VS_LE_REQ_BLE_CLOCK_SYNC_EVT_SUBCODE |
HCI_VS_LE_CON_PARAM_NOTIF_EVT_SUBCODE |
HCI_VS_LE_CH_MAP_PARAM_NOTIF_EVT_SUBCODE |
HCI_VS_LE_PHY_PARAM_NOTIF_EVT_SUBCODE |
HCI_VS_LE_RSSI_REPORT_INFO_EVT_SUBCODE |
HCI_VS_LE_RSSI_RANGING_TYPE_NOTIF_EVT_SUBCODE |
HCI_VS_LE_EVENT_NOTIFICATION_REPORT_INFO_EVT_SUBCODE |

Definition at line 555 of file ble_id.h.

## ◆ hci_vs_opcode

enum hci_vs_opcode

Enumerator
HCI_VS_LE_SET_DK_DEVICE_INFO_CMD_OPCODE |
HCI_VS_LE_GET_LINK_INFO_CMD_OPCODE |
HCI_VS_LE_CREATE_SNIFFER_CMD_OPCODE |
HCI_VS_LE_DISCONNECT_SNIFFER_CMD_OPCODE |
HCI_VS_LE_UPDATE_SNIFFER_CON_PARAM_CMD_OPCODE |
HCI_VS_LE_UPDATE_SNIFFER_CH_MAP_PARAM_CMD_OPCODE |
HCI_VS_LE_UPDATE_SNIFFER_PHY_PARAM_CMD_OPCODE |
HCI_VS_LE_RSSI_ENABLE_RANGING_CMD_OPCODE |
HCI_VS_LE_RSSI_UPDATE_RANGING_TYPE_CMD_OPCODE |
HCI_VS_LE_EVENT_NOTIFICATION_EN_CMD_OPCODE |

Definition at line 538 of file ble_id.h.

## ◆ l2cc_msg_id

enum l2cc_msg_id

GATTC_TASK Message ID.

Enumerator
L2CC_CMP_EVT |
L2CC_LECB_CONNECT_CMD |
L2CC_LECB_CONNECT_REQ_IND |
L2CC_LECB_CONNECT_CFM |
L2CC_LECB_CONNECT_IND |
L2CC_LECB_DISCONNECT_CMD |
L2CC_LECB_DISCONNECT_IND |
L2CC_LECB_ADD_CMD |
L2CC_LECB_ADD_IND |
L2CC_LECB_SDU_SEND_CMD |
L2CC_LECB_SDU_RECV_IND |
L2CC_UNKNOWN_MSG_IND |
L2CC_DBG_PDU_SEND_CMD |
L2CC_DBG_PDU_RECV_IND |
L2CC_PDU_SEND_CMD |
L2CC_PDU_RECV_IND |
L2CC_SIGNALING_TRANS_TO_IND |

Definition at line 849 of file ble_id.h.

## ◆ sdk_msg_id

enum sdk_msg_id

SDK_TASK Message ID.

Enumerator
SDK_COMMON_TIMEOUT_TIMER_0 | Timeout indication to sdk.
SDK_COMMON_TIMEOUT_TIMER_1 |
SDK_COMMON_TIMEOUT_TIMER_2 |
SDK_COMMON_TIMEOUT_TIMER_3 |
SDK_COMMON_TIMEOUT_TIMER_4 |
SDK_COMMON_TIMEOUT_TIMER_5 |
SDK_COMMON_TIMEOUT_TIMER_6 |
SDK_COMMON_TIMEOUT_TIMER_7 |
SDK_COMMON_TIMEOUT_TIMER_8 |
SDK_COMMON_TIMEOUT_TIMER_9 |
SDK_RANGING_INTER_NODE_COMM_RX_DATA |
SDK_RANGING_INTER_NODE_COMM_TX_DATA_CMP |
SDK_RANGING_INTER_NODE_COMM_ABORT_TX_CMP |
SDK_RANGING_INTER_NODE_COMM_ERR_OCCUR |
SDK_RANGING_SLEEP_RANGING |
SDK_RANGING_WAKEUP_RANGING |
SDK_RANGING_START_RANGING |
SDK_RANGING_STOP_RANGING |
SDK_RANGING_ANCHOR_START_RANGING |
SDK_RANGING_ANCHOR_STOP_RANGING |
SDK_RANGING_UPDATE_CI |
SDK_RANGING_TIMEOUT_DISPATCH |
SDK_APP_SET_SCAN_ADDR |

Definition at line 628 of file ble_id.h.

## ◆ TASK_API_ID

enum TASK_API_ID

Enumerator
TASK_ID_LLM |
TASK_ID_LLC |
TASK_ID_LLD |
TASK_ID_LLI |
TASK_ID_DBG |
TASK_ID_LM |
TASK_ID_LC |
TASK_ID_LB |
TASK_ID_LD |
TASK_ID_SDK |
TASK_ID_L2CC |
TASK_ID_GATTM |
TASK_ID_GATTC |
TASK_ID_GAPM |
TASK_ID_GAPC |
TASK_ID_APP |
TASK_ID_AHI |
TASK_ID_HCI |
TASK_ID_DISPLAY |
TASK_ID_MESH |
TASK_ID_RTLS |
TASK_ID_INVALID |

Definition at line 569 of file ble_id.h.