Macros
Measurement Flag Bits
BLE Services » Running Speed and Cadence Service Client (RSCS_C) » Defines

Running Speed and Cadence Measurement Flags. More...

## Macros
#define | RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT (0x01 << 0)
#define | RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT (0x01 << 1)
#define | RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT (0x01 << 2)

## Detailed Description

Running Speed and Cadence Measurement Flags.

## Macro Definition Documentation

## ◆ RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT

#define RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT (0x01 << 0)

Flag bit for Instantaneous Stride Length Measurement.

Definition at line 82 of file rscs_c.h.

## ◆ RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT

#define RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT (0x01 << 2)

Flag bit for Running or Walking.

Definition at line 84 of file rscs_c.h.

## ◆ RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT

#define RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT (0x01 << 1)

Flag bit for Total Distance Measurement.

Definition at line 83 of file rscs_c.h.