Functions
Functions
Peripheral Driver » APP DRIVER » DMA

## Functions
dma_id_t | app_dma_init (app_dma_params_t *p_params, app_dma_evt_handler_t evt_handler)
| Initialize the APP DMA DRIVER according to the specified parameters in the app_dma_params_t and app_dma_evt_handler_t. More...
uint16_t | app_dma_deinit (dma_id_t id)
| De-initialize the APP ADC DRIVER peripheral. More...
uint16_t | app_dma_start (dma_id_t id, uint32_t src_address, uint32_t dst_address, uint32_t data_length)
| Start the DMA Transfer. More...
dma_handle_t * | app_dma_get_handle (dma_id_t id)
| Return the DMA handle. More...

## Detailed Description

## Function Documentation

## ◆ app_dma_deinit()

uint16_t app_dma_deinit | ( | dma_id_t | id | ) |

De-initialize the APP ADC DRIVER peripheral.

Parameters

  [in] | id | Deinitialize DMA channel for a specific ID.

Returns
  Result of De-initialization.

## ◆ app_dma_get_handle()

dma_handle_t* app_dma_get_handle | ( | dma_id_t | id | ) |

Return the DMA handle.

Parameters

  [in] | id | DMA Channel ID.

Returns
  Pointer to the specified ID's DMA handle.

## ◆ app_dma_init()

dma_id_t app_dma_init | ( | app_dma_params_t * | p_params,
|  | app_dma_evt_handler_t | evt_handler
| ) |  |

Initialize the APP DMA DRIVER according to the specified parameters in the app_dma_params_t and app_dma_evt_handler_t.

Parameters

  [in] | p_params | Pointer to app_dma_params_t parameter which contains the configuration information for the specified DMA module.
  [in] | evt_handler | DMA user callback function.

Returns
  DMA ID

## ◆ app_dma_start()

uint16_t app_dma_start | ( | dma_id_t | id,
|  | uint32_t | src_address,
|  | uint32_t | dst_address,
|  | uint32_t | data_length
| ) |  |

Start the DMA Transfer.

Parameters

  [in] | id | DMA channel id.
  [in] | src_address | The source memory Buffer address
  [in] | dst_address | The destination memory Buffer address
  [in] | data_length | The length of data to be transferred from source to destination, ranging between 0 and 4095.