Macros
PWM period unit default configuretion
Peripheral Driver » LL Driver » PWM » Defines » PWM Exported Constants

## Macros
#define | LL_PWM_PRESCALER_UNIT (128)
#define | LL_PWM_BREATH_PRESCALER_UNIT (128)
#define | LL_PWM_HOLD_PRESCALER_UNIT (10)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PWM_BREATH_PRESCALER_UNIT

#define LL_PWM_BREATH_PRESCALER_UNIT (128)

The unit of breath prescaler is 128

Definition at line 278 of file ll_pwm.h.

## ◆ LL_PWM_HOLD_PRESCALER_UNIT

#define LL_PWM_HOLD_PRESCALER_UNIT (10)

The unit of hold prescaler is 10

Definition at line 279 of file ll_pwm.h.

## ◆ LL_PWM_PRESCALER_UNIT

#define LL_PWM_PRESCALER_UNIT (128)

The unit of prescaler is 128

Definition at line 277 of file ll_pwm.h.