Macros
DMA Peripheral type
Peripheral Driver » LL Driver » DMA » Defines » DMA Exported Constants
Collaboration diagram for DMA Peripheral type:

## Macros
#define | LL_DMA0_PERIPH_MEM ((uint32_t)0x0000000BU)
| DMA peripheral type is Memory. More...
#define | LL_DMA0_PERIPH_QSPI0_TX ((uint32_t)0x00000000U)
| DMA Peripheral type is QSPIM0 TX. More...
#define | LL_DMA0_PERIPH_QSPI0_RX ((uint32_t)0x00000001U)
| DMA Peripheral type is QSPIM0 RX. More...
#define | LL_DMA0_PERIPH_SPIM_TX ((uint32_t)0x00000002U)
| DMA Peripheral type is SPIM TX More...
#define | LL_DMA0_PERIPH_SPIM_RX ((uint32_t)0x00000003U)
| DMA Peripheral type is SPIM RX More...
#define | LL_DMA0_PERIPH_SPIS_TX ((uint32_t)0x00000004U)
| DMA Peripheral type is SPIS TX More...
#define | LL_DMA0_PERIPH_SPIS_RX ((uint32_t)0x00000005U)
| DMA Peripheral type is SPIS RX More...
#define | LL_DMA0_PERIPH_UART0_TX ((uint32_t)0x00000006U)
| DMA Peripheral type is UART0 TX More...
#define | LL_DMA0_PERIPH_UART0_RX ((uint32_t)0x00000007U)
| DMA Peripheral type is UART0 RX More...
#define | LL_DMA0_PERIPH_UART1_TX ((uint32_t)0x00000008U)
| DMA Peripheral type is UART1 TX More...
#define | LL_DMA0_PERIPH_UART1_RX ((uint32_t)0x00000009U)
| DMA Peripheral type is UART1 RX More...
#define | LL_DMA0_PERIPH_SNSADC ((uint32_t)0x0000000AU)
| DMA peripheral type is SNSADC More...
#define | LL_DMA0_PERIPH_OSPI_TX ((uint32_t)0x0000000CU)
| DMA Peripheral type is OSPIM TX More...
#define | LL_DMA0_PERIPH_OSPI_RX ((uint32_t)0x0000000DU)
| DMA Peripheral type is OSPIM RX More...
#define | LL_DMA0_PERIPH_UART2_TX ((uint32_t)0x0000000EU)
| DMA Peripheral type is UART2 TX More...
#define | LL_DMA0_PERIPH_UART2_RX ((uint32_t)0x0000000FU)
| DMA Peripheral type is UART2 RX More...
#define | LL_DMA0_PERIPH_I2C2_TX ((uint32_t)0x00000012U)
| DMA Peripheral type is I2C2 TX More...
#define | LL_DMA0_PERIPH_I2C2_RX ((uint32_t)0x00000013U)
| DMA Peripheral type is I2C2 RX More...
#define | LL_DMA0_PERIPH_UART3_TX ((uint32_t)0x00000014U)
| DMA Peripheral type is UART3 TX More...
#define | LL_DMA0_PERIPH_UART3_RX ((uint32_t)0x00000015U)
| DMA Peripheral type is UART3 RX More...
#define | LL_DMA0_PERIPH_I2C5_TX ((uint32_t)0x00000016U)
| DMA Peripheral type is I2C5 TX More...
#define | LL_DMA0_PERIPH_I2C5_RX ((uint32_t)0x00000017U)
| DMA Peripheral type is I2C5 RX More...
#define | LL_DMA0_PERIPH_I2C4_TX ((uint32_t)0x00000018U)
| DMA Peripheral type is I2C4 TX More...
#define | LL_DMA0_PERIPH_I2C4_RX ((uint32_t)0x00000019U)
| DMA Peripheral type is I2C5 RX More...
#define | LL_DMA0_PERIPH_UART4_TX ((uint32_t)0x0000001AU)
| DMA Peripheral type is UART4 TX More...
#define | LL_DMA0_PERIPH_UART4_RX ((uint32_t)0x0000001BU)
| DMA Peripheral type is UART4 RX More...
#define | LL_DMA0_PERIPH_QSPI1_TX ((uint32_t)0x0000001CU)
| DMA Peripheral type is QSPIM1 TX. More...
#define | LL_DMA0_PERIPH_QSPI1_RX ((uint32_t)0x0000001DU)
| DMA Peripheral type is QSPIM1 RX. More...
#define | LL_DMA0_PERIPH_I2C3_TX ((uint32_t)0x0000001EU)
| DMA Peripheral type is I2C3 TX More...
#define | LL_DMA0_PERIPH_I2C3_RX ((uint32_t)0x0000001FU)
| DMA Peripheral type is I2C3 RX More...
#define | LL_DMA1_PERIPH_MEM ((uint32_t)0x00000009U)
| DMA peripheral type is Memory. More...
#define | LL_DMA1_PERIPH_OSPI_TX ((uint32_t)0x00000000U)
| DMA Peripheral type is OSPIM TX More...
#define | LL_DMA1_PERIPH_OSPI_RX ((uint32_t)0x00000001U)
| DMA Peripheral type is OSPIM RX More...
#define | LL_DMA1_PERIPH_QSPI2_TX ((uint32_t)0x00000002U)
| DMA Peripheral type is QSPIM2 TX. More...
#define | LL_DMA1_PERIPH_QSPI2_RX ((uint32_t)0x00000003U)
| DMA Peripheral type is QSPIM2 RX. More...
#define | LL_DMA1_PERIPH_I2S_M_TX ((uint32_t)0x00000004U)
| DMA Peripheral type is IIS_M TX More...
#define | LL_DMA1_PERIPH_I2S_M_RX ((uint32_t)0x00000005U)
| DMA Peripheral type is IIS_M RX More...
#define | LL_DMA1_PERIPH_I2S_S_TX ((uint32_t)0x00000006U)
| DMA Peripheral type is IIS_S TX More...
#define | LL_DMA1_PERIPH_I2S_S_RX ((uint32_t)0x00000007U)
| DMA Peripheral type is IIS_S RX More...
#define | LL_DMA1_PERIPH_PDM_TX ((uint32_t)0x00000008U)
| DMA Peripheral type is PDM TX More...
#define | LL_DMA1_PERIPH_QSPI1_TX ((uint32_t)0x0000000AU)
| DMA Peripheral type is QSPIM1 TX. More...
#define | LL_DMA1_PERIPH_QSPI1_RX ((uint32_t)0x0000000BU)
| DMA Peripheral type is QSPIM1 RX. More...
#define | LL_DMA1_PERIPH_I2C0_TX ((uint32_t)0x0000000CU)
| DMA Peripheral type is I2C0 TX More...
#define | LL_DMA1_PERIPH_I2C0_RX ((uint32_t)0x0000000DU)
| DMA Peripheral type is I2C0 RX More...
#define | LL_DMA1_PERIPH_I2C1_TX ((uint32_t)0x0000000EU)
| DMA Peripheral type is I2C1 TX More...
#define | LL_DMA1_PERIPH_I2C1_RX ((uint32_t)0x0000000FU)
| DMA Peripheral type is I2C1 RX More...
#define | LL_DMA1_PERIPH_SPIM_TX ((uint32_t)0x00000010U)
| DMA Peripheral type is SPIM TX More...
#define | LL_DMA1_PERIPH_SPIM_RX ((uint32_t)0x00000011U)
| DMA Peripheral type is SPIM RX More...
#define | LL_DMA1_PERIPH_DSPIM_TX ((uint32_t)0x00000012U)
| DMA Peripheral type is DSPIM TX More...
#define | LL_DMA1_PERIPH_DSPIM_RX ((uint32_t)0x00000013U)
| DMA Peripheral type is DSPIM RX More...
#define | LL_DMA1_PERIPH_QSPI1_TX_2 ((uint32_t)0x00000014U)
| DMA Peripheral type is QSPI1 TX More...
#define | LL_DMA1_PERIPH_QSPI1_RX_2 ((uint32_t)0x00000015U)
| DMA Peripheral type is QSPI1 RX More...
#define | LL_DMA1_PERIPH_UART3_TX ((uint32_t)0x00000016U)
| DMA Peripheral type is UART3 TX More...
#define | LL_DMA1_PERIPH_UART3_RX ((uint32_t)0x00000017U)
| DMA Peripheral type is UART3 RX More...
#define | LL_DMA1_PERIPH_UART4_TX ((uint32_t)0x00000018U)
| DMA Peripheral type is UART4 TX More...
#define | LL_DMA1_PERIPH_UART4_RX ((uint32_t)0x00000019U)
| DMA Peripheral type is UART4 RX More...
#define | LL_DMA1_PERIPH_UART5_TX ((uint32_t)0x0000001AU)
| DMA Peripheral type is UART5 TX More...
#define | LL_DMA1_PERIPH_UART5_RX ((uint32_t)0x0000001BU)
| DMA Peripheral type is UART5 RX More...
#define | LL_DMA1_PERIPH_UART0_TX ((uint32_t)0x0000001EU)
| DMA Peripheral type is UART0 TX More...
#define | LL_DMA1_PERIPH_UART0_RX ((uint32_t)0x0000001FU)
| DMA Peripheral type is UART0 RX More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DMA0_PERIPH_I2C2_RX

#define LL_DMA0_PERIPH_I2C2_RX ((uint32_t)0x00000013U)

DMA Peripheral type is I2C2 RX

Definition at line 337 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C2_TX

#define LL_DMA0_PERIPH_I2C2_TX ((uint32_t)0x00000012U)

DMA Peripheral type is I2C2 TX

Definition at line 336 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C3_RX

#define LL_DMA0_PERIPH_I2C3_RX ((uint32_t)0x0000001FU)

DMA Peripheral type is I2C3 RX

Definition at line 349 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C3_TX

#define LL_DMA0_PERIPH_I2C3_TX ((uint32_t)0x0000001EU)

DMA Peripheral type is I2C3 TX

Definition at line 348 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C4_RX

#define LL_DMA0_PERIPH_I2C4_RX ((uint32_t)0x00000019U)

DMA Peripheral type is I2C5 RX

Definition at line 343 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C4_TX

#define LL_DMA0_PERIPH_I2C4_TX ((uint32_t)0x00000018U)

DMA Peripheral type is I2C4 TX

Definition at line 342 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C5_RX

#define LL_DMA0_PERIPH_I2C5_RX ((uint32_t)0x00000017U)

DMA Peripheral type is I2C5 RX

Definition at line 341 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_I2C5_TX

#define LL_DMA0_PERIPH_I2C5_TX ((uint32_t)0x00000016U)

DMA Peripheral type is I2C5 TX

Definition at line 340 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_MEM

#define LL_DMA0_PERIPH_MEM ((uint32_t)0x0000000BU)

DMA peripheral type is Memory.

Definition at line 316 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_OSPI_RX

#define LL_DMA0_PERIPH_OSPI_RX ((uint32_t)0x0000000DU)

DMA Peripheral type is OSPIM RX

Definition at line 331 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_OSPI_TX

#define LL_DMA0_PERIPH_OSPI_TX ((uint32_t)0x0000000CU)

DMA Peripheral type is OSPIM TX

Definition at line 330 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_QSPI0_RX

#define LL_DMA0_PERIPH_QSPI0_RX ((uint32_t)0x00000001U)

DMA Peripheral type is QSPIM0 RX.

Definition at line 320 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_QSPI0_TX

#define LL_DMA0_PERIPH_QSPI0_TX ((uint32_t)0x00000000U)

DMA Peripheral type is QSPIM0 TX.

Definition at line 319 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_QSPI1_RX

#define LL_DMA0_PERIPH_QSPI1_RX ((uint32_t)0x0000001DU)

DMA Peripheral type is QSPIM1 RX.

Definition at line 347 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_QSPI1_TX

#define LL_DMA0_PERIPH_QSPI1_TX ((uint32_t)0x0000001CU)

DMA Peripheral type is QSPIM1 TX.

Definition at line 346 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_SNSADC

#define LL_DMA0_PERIPH_SNSADC ((uint32_t)0x0000000AU)

DMA peripheral type is SNSADC

Definition at line 329 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIM_RX

#define LL_DMA0_PERIPH_SPIM_RX ((uint32_t)0x00000003U)

DMA Peripheral type is SPIM RX

Definition at line 322 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIM_TX

#define LL_DMA0_PERIPH_SPIM_TX ((uint32_t)0x00000002U)

DMA Peripheral type is SPIM TX

Definition at line 321 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIS_RX

#define LL_DMA0_PERIPH_SPIS_RX ((uint32_t)0x00000005U)

DMA Peripheral type is SPIS RX

Definition at line 324 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_SPIS_TX

#define LL_DMA0_PERIPH_SPIS_TX ((uint32_t)0x00000004U)

DMA Peripheral type is SPIS TX

Definition at line 323 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART0_RX

#define LL_DMA0_PERIPH_UART0_RX ((uint32_t)0x00000007U)

DMA Peripheral type is UART0 RX

Definition at line 326 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART0_TX

#define LL_DMA0_PERIPH_UART0_TX ((uint32_t)0x00000006U)

DMA Peripheral type is UART0 TX

Definition at line 325 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART1_RX

#define LL_DMA0_PERIPH_UART1_RX ((uint32_t)0x00000009U)

DMA Peripheral type is UART1 RX

Definition at line 328 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART1_TX

#define LL_DMA0_PERIPH_UART1_TX ((uint32_t)0x00000008U)

DMA Peripheral type is UART1 TX

Definition at line 327 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART2_RX

#define LL_DMA0_PERIPH_UART2_RX ((uint32_t)0x0000000FU)

DMA Peripheral type is UART2 RX

Definition at line 333 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART2_TX

#define LL_DMA0_PERIPH_UART2_TX ((uint32_t)0x0000000EU)

DMA Peripheral type is UART2 TX

Definition at line 332 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART3_RX

#define LL_DMA0_PERIPH_UART3_RX ((uint32_t)0x00000015U)

DMA Peripheral type is UART3 RX

Definition at line 339 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART3_TX

#define LL_DMA0_PERIPH_UART3_TX ((uint32_t)0x00000014U)

DMA Peripheral type is UART3 TX

Definition at line 338 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART4_RX

#define LL_DMA0_PERIPH_UART4_RX ((uint32_t)0x0000001BU)

DMA Peripheral type is UART4 RX

Definition at line 345 of file gr55xx_ll_dma.h.

## ◆ LL_DMA0_PERIPH_UART4_TX

#define LL_DMA0_PERIPH_UART4_TX ((uint32_t)0x0000001AU)

DMA Peripheral type is UART4 TX

Definition at line 344 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_DSPIM_RX

#define LL_DMA1_PERIPH_DSPIM_RX ((uint32_t)0x00000013U)

DMA Peripheral type is DSPIM RX

Definition at line 376 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_DSPIM_TX

#define LL_DMA1_PERIPH_DSPIM_TX ((uint32_t)0x00000012U)

DMA Peripheral type is DSPIM TX

Definition at line 375 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2C0_RX

#define LL_DMA1_PERIPH_I2C0_RX ((uint32_t)0x0000000DU)

DMA Peripheral type is I2C0 RX

Definition at line 368 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2C0_TX

#define LL_DMA1_PERIPH_I2C0_TX ((uint32_t)0x0000000CU)

DMA Peripheral type is I2C0 TX

Definition at line 367 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2C1_RX

#define LL_DMA1_PERIPH_I2C1_RX ((uint32_t)0x0000000FU)

DMA Peripheral type is I2C1 RX

Definition at line 370 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2C1_TX

#define LL_DMA1_PERIPH_I2C1_TX ((uint32_t)0x0000000EU)

DMA Peripheral type is I2C1 TX

Definition at line 369 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2S_M_RX

#define LL_DMA1_PERIPH_I2S_M_RX ((uint32_t)0x00000005U)

DMA Peripheral type is IIS_M RX

Definition at line 360 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2S_M_TX

#define LL_DMA1_PERIPH_I2S_M_TX ((uint32_t)0x00000004U)

DMA Peripheral type is IIS_M TX

Definition at line 359 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2S_S_RX

#define LL_DMA1_PERIPH_I2S_S_RX ((uint32_t)0x00000007U)

DMA Peripheral type is IIS_S RX

Definition at line 362 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_I2S_S_TX

#define LL_DMA1_PERIPH_I2S_S_TX ((uint32_t)0x00000006U)

DMA Peripheral type is IIS_S TX

Definition at line 361 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_MEM

#define LL_DMA1_PERIPH_MEM ((uint32_t)0x00000009U)

DMA peripheral type is Memory.

Definition at line 352 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_OSPI_RX

#define LL_DMA1_PERIPH_OSPI_RX ((uint32_t)0x00000001U)

DMA Peripheral type is OSPIM RX

Definition at line 356 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_OSPI_TX

#define LL_DMA1_PERIPH_OSPI_TX ((uint32_t)0x00000000U)

DMA Peripheral type is OSPIM TX

Definition at line 355 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_PDM_TX

#define LL_DMA1_PERIPH_PDM_TX ((uint32_t)0x00000008U)

DMA Peripheral type is PDM TX

Definition at line 363 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_QSPI1_RX

#define LL_DMA1_PERIPH_QSPI1_RX ((uint32_t)0x0000000BU)

DMA Peripheral type is QSPIM1 RX.

Definition at line 365 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_QSPI1_RX_2

#define LL_DMA1_PERIPH_QSPI1_RX_2 ((uint32_t)0x00000015U)

DMA Peripheral type is QSPI1 RX

Definition at line 378 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_QSPI1_TX

#define LL_DMA1_PERIPH_QSPI1_TX ((uint32_t)0x0000000AU)

DMA Peripheral type is QSPIM1 TX.

Definition at line 364 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_QSPI1_TX_2

#define LL_DMA1_PERIPH_QSPI1_TX_2 ((uint32_t)0x00000014U)

DMA Peripheral type is QSPI1 TX

Definition at line 377 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_QSPI2_RX

#define LL_DMA1_PERIPH_QSPI2_RX ((uint32_t)0x00000003U)

DMA Peripheral type is QSPIM2 RX.

Definition at line 358 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_QSPI2_TX

#define LL_DMA1_PERIPH_QSPI2_TX ((uint32_t)0x00000002U)

DMA Peripheral type is QSPIM2 TX.

Definition at line 357 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_SPIM_RX

#define LL_DMA1_PERIPH_SPIM_RX ((uint32_t)0x00000011U)

DMA Peripheral type is SPIM RX

Definition at line 374 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_SPIM_TX

#define LL_DMA1_PERIPH_SPIM_TX ((uint32_t)0x00000010U)

DMA Peripheral type is SPIM TX

Definition at line 373 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART0_RX

#define LL_DMA1_PERIPH_UART0_RX ((uint32_t)0x0000001FU)

DMA Peripheral type is UART0 RX

Definition at line 386 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART0_TX

#define LL_DMA1_PERIPH_UART0_TX ((uint32_t)0x0000001EU)

DMA Peripheral type is UART0 TX

Definition at line 385 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART3_RX

#define LL_DMA1_PERIPH_UART3_RX ((uint32_t)0x00000017U)

DMA Peripheral type is UART3 RX

Definition at line 380 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART3_TX

#define LL_DMA1_PERIPH_UART3_TX ((uint32_t)0x00000016U)

DMA Peripheral type is UART3 TX

Definition at line 379 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART4_RX

#define LL_DMA1_PERIPH_UART4_RX ((uint32_t)0x00000019U)

DMA Peripheral type is UART4 RX

Definition at line 382 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART4_TX

#define LL_DMA1_PERIPH_UART4_TX ((uint32_t)0x00000018U)

DMA Peripheral type is UART4 TX

Definition at line 381 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART5_RX

#define LL_DMA1_PERIPH_UART5_RX ((uint32_t)0x0000001BU)

DMA Peripheral type is UART5 RX

Definition at line 384 of file gr55xx_ll_dma.h.

## ◆ LL_DMA1_PERIPH_UART5_TX

#define LL_DMA1_PERIPH_UART5_TX ((uint32_t)0x0000001AU)

DMA Peripheral type is UART5 TX

Definition at line 383 of file gr55xx_ll_dma.h.