Public Attributes | List of all members
iso_sync_ann_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for sync announcement. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | sid
| public type. More...
uint8_t | peer_addr_type
| Peer address type, see iso_add_type_t. More...
uint8_t | peer_addr [ISO_ADDR_LEN]
| Peer address. More...
uint16_t | sync_timeout
| Synchronization timeout for the periodic advertising(in unit of 10ms between 100ms and 163.84s). More...

## Detailed Description

The parameter for sync announcement.

Definition at line 254 of file ble_iso.h.

## Member Data Documentation

## ◆ peer_addr

uint8_t iso_sync_ann_t::peer_addr[ISO_ADDR_LEN]

Peer address.

Definition at line 258 of file ble_iso.h.

## ◆ peer_addr_type

uint8_t iso_sync_ann_t::peer_addr_type

Peer address type, see iso_add_type_t.

Definition at line 257 of file ble_iso.h.

## ◆ sid

uint8_t iso_sync_ann_t::sid

public type.

Definition at line 256 of file ble_iso.h.

## ◆ sync_timeout

uint16_t iso_sync_ann_t::sync_timeout

Synchronization timeout for the periodic advertising(in unit of 10ms between 100ms and 163.84s).

Definition at line 259 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h