Macros
Individual Block's Clock Control
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

Individual block's clock control inside security system. More...

Collaboration diagram for Individual Block's Clock Control:

## Macros
#define | LL_CGC_MCU_FRC_AES_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_AES_HCLK_FORCE_OFF
| Force individual aes's clock control More...
#define | LL_CGC_MCU_SLP_AES_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_AES_HCLK_SLP_OFF
| Individual aes's clock control More...
#define | LL_CGC_MCU_FRC_HMAC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_HMAC_HCLK_FORCE_OFF
| Force individual hmac's clock control More...
#define | LL_CGC_MCU_SLP_HMAC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_HMAC_HCLK_SLP_OFF
| Individual hmac's clock control More...
#define | LL_CGC_MCU_FRC_PKC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PKC_HCLK_FORCE_OFF
| Force individual pkc's clock control More...
#define | LL_CGC_MCU_SLP_PKC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PKC_HCLK_SLP_OFF
| Individual pkc's clock control More...
#define | LL_CGC_MCU_FRC_PRESENT_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PRESENT_HCLK_FORCE_OFF
| Force individual present's clock control More...
#define | LL_CGC_MCU_SLP_PRESENT_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PRESENT_HCLK_SLP_OFF
| Individual present's clock control More...
#define | LL_CGC_MCU_FRC_RAMKEY_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RAMKEY_HCLK_FORCE_OFF
| Force individual ramkey's clock control More...
#define | LL_CGC_MCU_SLP_RAMKEY_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RAMKEY_HCLK_SLP_OFF
| Individual ramkey's clock control More...
#define | LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_FORCE_OFF
| Force individual rng's clock control More...
#define | LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_SLP_OFF
| Individual rng's clock control More...
#define | LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_FORCE_OFF
| Force individual efuse's clock control More...
#define | LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_SLP_OFF
| Individual efuse's clock control More...
#define | LL_CGC_MCU_SECU_FRC_OFF_HCLK ((uint32_t)0x00001555U)
| Hclk for security clock More...
#define | LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK ((uint32_t)0x00002AAAU)
| Hclk for security clock WFI/WFE More...
#define | LL_CGC_MCU_SECU_FRC_OFF_ALL
| Hclk for security clock More...
#define | LL_CGC_MCU_MISC_CLK_DEFAULT ((uint32_t)0x0000003BU)
| Hclk for msic default clock More...
#define | LL_CGC_MCU_MISC_CLK ((uint32_t)0x0000003FU)
| Hclk for msic all clock More...
#define | LL_CGC_MCU_MISC_DMA_CLK ((uint32_t)0x00000038U)
| Hclk for msic dma clock More...

## Detailed Description

Individual block's clock control inside security system.

## Macro Definition Documentation

## ◆ LL_CGC_MCU_FRC_AES_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_AES_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_AES_HCLK_FORCE_OFF

Force individual aes's clock control

Definition at line 222 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_FORCE_OFF

Force individual efuse's clock control

Definition at line 234 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_HMAC_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_HMAC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_HMAC_HCLK_FORCE_OFF

Force individual hmac's clock control

Definition at line 224 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_PKC_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_PKC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PKC_HCLK_FORCE_OFF

Force individual pkc's clock control

Definition at line 226 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_PRESENT_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_PRESENT_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PRESENT_HCLK_FORCE_OFF

Force individual present's clock control

Definition at line 228 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_RAMKEY_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_RAMKEY_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RAMKEY_HCLK_FORCE_OFF

Force individual ramkey's clock control

Definition at line 230 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN

#define LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_FORCE_OFF

Force individual rng's clock control

Definition at line 232 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_MISC_CLK

#define LL_CGC_MCU_MISC_CLK ((uint32_t)0x0000003FU)

Hclk for msic all clock

Definition at line 245 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_MISC_CLK_DEFAULT

#define LL_CGC_MCU_MISC_CLK_DEFAULT ((uint32_t)0x0000003BU)

Hclk for msic default clock

Definition at line 243 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_MISC_DMA_CLK

#define LL_CGC_MCU_MISC_DMA_CLK ((uint32_t)0x00000038U)

Hclk for msic dma clock

Definition at line 247 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SECU_FRC_OFF_ALL

#define LL_CGC_MCU_SECU_FRC_OFF_ALL

Value:
(LL_CGC_MCU_SECU_FRC_OFF_HCLK |\
LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK)

Hclk for security clock

Definition at line 241 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SECU_FRC_OFF_HCLK

#define LL_CGC_MCU_SECU_FRC_OFF_HCLK ((uint32_t)0x00001555U)

Hclk for security clock

Definition at line 237 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK

#define LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK ((uint32_t)0x00002AAAU)

Hclk for security clock WFI/WFE

Definition at line 238 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_AES_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_AES_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_AES_HCLK_SLP_OFF

Individual aes's clock control

Definition at line 223 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_EFUSE_HCLK_SLP_OFF

Individual efuse's clock control

Definition at line 235 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_HMAC_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_HMAC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_HMAC_HCLK_SLP_OFF

Individual hmac's clock control

Definition at line 225 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_PKC_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_PKC_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PKC_HCLK_SLP_OFF

Individual pkc's clock control

Definition at line 227 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_PRESENT_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_PRESENT_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_PRESENT_HCLK_SLP_OFF

Individual present's clock control

Definition at line 229 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_RAMKEY_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_RAMKEY_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RAMKEY_HCLK_SLP_OFF

Individual ramkey's clock control

Definition at line 231 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN

#define LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN MCU_SUB_SECU_CLK_CTRL_RNG_HCLK_SLP_OFF

Individual rng's clock control

Definition at line 233 of file gr55xx_ll_cgc.h.

LL_CGC_MCU_SECU_FRC_OFF_HCLK
#define LL_CGC_MCU_SECU_FRC_OFF_HCLK
Hclk for security clock
Definition: gr55xx_ll_cgc.h:237