Enumerations
Enumerations
BLE Services » Wechat (WECHAT)
Collaboration diagram for Enumerations:

## Enumerations
enum | wechat_evt_type_t { WECHAT_EVT_INVALID, WECHAT_EVT_AIRSYNC_IND_ENABLE, WECHAT_EVT_AIRSYNC_IND_DISABLE, WECHAT_EVT_PEDO_MEAS_NTF_ENABLE, WECHAT_EVT_PEDO_MEAS_NTF_DISABLE, WECHAT_EVT_PEDO_TARGET_IND_ENABLE, WECHAT_EVT_PEDO_TARGET_IND_DISABLE, WECHAT_EVT_PEDO_TARGET_UPDATE, WECHAT_EVT_AIRSYNC_DATA_RECIEVE }
| WeChat Service event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ wechat_evt_type_t

enum wechat_evt_type_t

WeChat Service event type.

Enumerator
WECHAT_EVT_INVALID | WeChat invalid event.
WECHAT_EVT_AIRSYNC_IND_ENABLE | WeChat Airsync indication has been enabled.
WECHAT_EVT_AIRSYNC_IND_DISABLE | WeChat Airsync indication has been disabled.
WECHAT_EVT_PEDO_MEAS_NTF_ENABLE | WeChat Pedometer measurement notification has been enabled.
WECHAT_EVT_PEDO_MEAS_NTF_DISABLE | WeChat Pedometer measurement notification has been disabled.
WECHAT_EVT_PEDO_TARGET_IND_ENABLE | WeChat Pedometer target indicaiton has been enabled.
WECHAT_EVT_PEDO_TARGET_IND_DISABLE | WeChat Pedometer target indicaiton has been disabled.
WECHAT_EVT_PEDO_TARGET_UPDATE | WeChat Pedometer target has been updated.
WECHAT_EVT_AIRSYNC_DATA_RECIEVE | Recieved Airsync data.

Definition at line 110 of file wechat.h.