Enumerations
Enumerations
SYSTEM » System SDK
Collaboration diagram for Enumerations:

## Enumerations
enum | sram_size_t { SYS_DEV_SRAM_288K = 0x01, SYS_DEV_SRAM_512K = 0x00 }
| Definition of Device SRAM Size Enumerations. More...
enum | package_type_t { PACKAGE_NONE = 0, PACKAGE_GR5526VGBIP = 0x0100, PACKAGE_GR5526VGBI = 0x0101, PACKAGE_GR5526_DEBUG = 0x0102, PACKAGE_GR5526RGNIP = 0x0200, PACKAGE_GR5526RGNI = 0x0201, PACKAGE_GR5526RJNIP = 0x0202 }
| package type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ package_type_t

enum package_type_t

package type.

Enumerator
PACKAGE_NONE | Package unused.
PACKAGE_GR5526VGBIP | BGA83 with 8Mb flash/GPU/PSRAM, with cap, no GND3 WB, add dummy Die.
PACKAGE_GR5526VGBI | BGA83 with 8Mb flash. no GPU/PSRAM.
PACKAGE_GR5526_DEBUG | BGA83 debug chip, test with XQSPI/OSPI pin-out.
PACKAGE_GR5526RGNIP | QFN68 with 8Mb flash/GPU/PSRAM, no GND3 WB, add dummy Die.
PACKAGE_GR5526RGNI | QFN68 with 8Mb flash. no GPU/PSRAM.
PACKAGE_GR5526RJNIP | QFN68 with 16Mb flash/GPU/PSRAM, no GND3 WB, add dummy Die.

Definition at line 120 of file gr55xx_sys_sdk.h.

## ◆ sram_size_t

enum sram_size_t

Definition of Device SRAM Size Enumerations.

Enumerator
SYS_DEV_SRAM_288K | Supported 288K SRAM.
SYS_DEV_SRAM_512K | Supported 512K SRAM.

Definition at line 113 of file gr55xx_sys_sdk.h.