Macros
Feature Bits
BLE Services » Cycling Speed and Cadence Service (CSCS) » Defines

Cycling Speed and Cadence Service feature bits. More...

Collaboration diagram for Feature Bits:

## Macros
#define | CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT (0x01 << 0)
| Bit for Wheel Revolution Data Supported. More...
#define | CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT (0x01 << 1)
| Bit for Crank Revolution Data Supported. More...
#define | CSCS_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 2)
| Bit for Multiple Sensor Locations Supported. More...
#define | CSCS_FEAR_FULL_BIT (0x07)
| Bit for all CSC features Supported. More...

## Detailed Description

Cycling Speed and Cadence Service feature bits.

## Macro Definition Documentation

## ◆ CSCS_FEAR_FULL_BIT

#define CSCS_FEAR_FULL_BIT (0x07)

Bit for all CSC features Supported.

Definition at line 108 of file cscs.h.

## ◆ CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT

#define CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT (0x01 << 1)

Bit for Crank Revolution Data Supported.

Definition at line 106 of file cscs.h.

## ◆ CSCS_FEAT_MULTIPLE_SENSORS_BIT

#define CSCS_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 2)

Bit for Multiple Sensor Locations Supported.

Definition at line 107 of file cscs.h.

## ◆ CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT

#define CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT (0x01 << 0)

Bit for Wheel Revolution Data Supported.

Definition at line 105 of file cscs.h.