Macros
DMA request definitions
Peripheral Driver » HAL Driver » DMA » Defines » DMA Exported Constants
Collaboration diagram for DMA request definitions:

## Macros
#define | DMA0_REQUEST_OSPI_TX LL_DMA0_PERIPH_OSPI_TX
| DMA OSPI transmit request. More...
#define | DMA0_REQUEST_OSPI_RX LL_DMA0_PERIPH_OSPI_RX
| DMA OSPI transmit request. More...
#define | DMA0_REQUEST_QSPI0_TX LL_DMA0_PERIPH_QSPI0_TX
| DMA QSPIM0 transmit request. More...
#define | DMA0_REQUEST_QSPI0_RX LL_DMA0_PERIPH_QSPI0_RX
| DMA QSPIM0 transmit request. More...
#define | DMA0_REQUEST_QSPI1_TX LL_DMA0_PERIPH_QSPI1_TX
| DMA QSPIM1 TX transmit request. More...
#define | DMA0_REQUEST_QSPI1_RX LL_DMA0_PERIPH_QSPI1_RX
| DMA QSPIM1 RX transmit request. More...
#define | DMA0_REQUEST_SPIM_TX LL_DMA0_PERIPH_SPIM_TX
| DMA SPIM transmit request. More...
#define | DMA0_REQUEST_SPIM_RX LL_DMA0_PERIPH_SPIM_RX
| DMA SPIM RX transmit request. More...
#define | DMA0_REQUEST_SPIS_TX LL_DMA0_PERIPH_SPIS_TX
| DMA SPIS TX transmit request. More...
#define | DMA0_REQUEST_SPIS_RX LL_DMA0_PERIPH_SPIS_RX
| DMA SPIS RX transmit request. More...
#define | DMA0_REQUEST_UART0_TX LL_DMA0_PERIPH_UART0_TX
| DMA UART0 TX transmit request. More...
#define | DMA0_REQUEST_UART0_RX LL_DMA0_PERIPH_UART0_RX
| DMA UART0 RX transmit request. More...
#define | DMA0_REQUEST_UART1_TX LL_DMA0_PERIPH_UART1_TX
| DMA UART1 TX transmit request. More...
#define | DMA0_REQUEST_UART1_RX LL_DMA0_PERIPH_UART1_RX
| DMA UART1 RX transmit request. More...
#define | DMA0_REQUEST_UART2_TX LL_DMA0_PERIPH_UART2_TX
| DMA UART2 TX transmit request. More...
#define | DMA0_REQUEST_UART2_RX LL_DMA0_PERIPH_UART2_RX
| DMA UART2 RX transmit request. More...
#define | DMA0_REQUEST_UART3_TX LL_DMA0_PERIPH_UART3_TX
| DMA UART3 TX transmit request. More...
#define | DMA0_REQUEST_UART3_RX LL_DMA0_PERIPH_UART3_RX
| DMA UART3 RX transmit request. More...
#define | DMA0_REQUEST_UART4_TX LL_DMA0_PERIPH_UART4_TX
| DMA UART4 TX transmit request. More...
#define | DMA0_REQUEST_UART4_RX LL_DMA0_PERIPH_UART4_RX
| DMA UART4 RX transmit request. More...
#define | DMA0_REQUEST_I2C2_TX LL_DMA0_PERIPH_I2C2_TX
| DMA I2C2 TX transmit request. More...
#define | DMA0_REQUEST_I2C2_RX LL_DMA0_PERIPH_I2C2_RX
| DMA I2C2 RX transmit request. More...
#define | DMA0_REQUEST_I2C3_TX LL_DMA0_PERIPH_I2C3_TX
| DMA I2C3 TX transmit request. More...
#define | DMA0_REQUEST_I2C3_RX LL_DMA0_PERIPH_I2C3_RX
| DMA I2C3 RX transmit request. More...
#define | DMA0_REQUEST_I2C4_TX LL_DMA0_PERIPH_I2C4_TX
| DMA I2C4 TX transmit request. More...
#define | DMA0_REQUEST_I2C4_RX LL_DMA0_PERIPH_I2C4_RX
| DMA I2C4 RX transmit request. More...
#define | DMA0_REQUEST_I2C5_TX LL_DMA0_PERIPH_I2C5_TX
| DMA I2C5 TX transmit request. More...
#define | DMA0_REQUEST_I2C5_RX LL_DMA0_PERIPH_I2C5_RX
| DMA I2C5 RX transmit request. More...
#define | DMA0_REQUEST_SNSADC LL_DMA0_PERIPH_SNSADC
| DMA SNSADC transmit request. More...
#define | DMA0_REQUEST_MEM LL_DMA0_PERIPH_MEM
| DMA is Memory transmit request. More...
#define | DMA1_REQUEST_OSPI_TX LL_DMA1_PERIPH_OSPI_TX
| DMA OSPI transmit request. More...
#define | DMA1_REQUEST_OSPI_RX LL_DMA1_PERIPH_OSPI_RX
| DMA OSPI transmit request. More...
#define | DMA1_REQUEST_QSPI1_TX LL_DMA1_PERIPH_QSPI1_TX
| DMA QSPIM1 TX transmit request. More...
#define | DMA1_REQUEST_QSPI1_RX LL_DMA1_PERIPH_QSPI1_RX
| DMA QSPIM1 RX transmit request. More...
#define | DMA1_REQUEST_QSPI2_TX LL_DMA1_PERIPH_QSPI2_TX
| DMA QSPIM2 TX transmit request. More...
#define | DMA1_REQUEST_QSPI2_RX LL_DMA1_PERIPH_QSPI2_RX
| DMA QSPIM2 RX transmit request. More...
#define | DMA1_REQUEST_SPIM_TX LL_DMA1_PERIPH_SPIM_TX
| DMA SPIM transmit request. More...
#define | DMA1_REQUEST_SPIM_RX LL_DMA1_PERIPH_SPIM_RX
| DMA SPIM RX transmit request. More...
#define | DMA1_REQUEST_DSPIM_TX LL_DMA1_PERIPH_DSPIM_TX
| DMA DSPIM TX transmit request. More...
#define | DMA1_REQUEST_DSPIM_RX LL_DMA1_PERIPH_DSPIM_RX
| DMA DSPIM RX transmit request. More...
#define | DMA1_REQUEST_I2S_M_TX LL_DMA1_PERIPH_I2S_M_TX
| DMA I2S_M TX transmit request. More...
#define | DMA1_REQUEST_I2S_M_RX LL_DMA1_PERIPH_I2S_M_RX
| DMA I2S_M RX transmit request. More...
#define | DMA1_REQUEST_I2S_S_TX LL_DMA1_PERIPH_I2S_S_TX
| DMA I2S_S TX transmit request. More...
#define | DMA1_REQUEST_I2S_S_RX LL_DMA1_PERIPH_I2S_S_RX
| DMA I2S_S RX transmit request. More...
#define | DMA1_REQUEST_PDM_TX LL_DMA1_PERIPH_PDM_TX
| DMA PDM TX transmit request. More...
#define | DMA1_REQUEST_I2C0_TX LL_DMA1_PERIPH_I2C0_TX
| DMA I2C0 TX transmit request. More...
#define | DMA1_REQUEST_I2C0_RX LL_DMA1_PERIPH_I2C0_RX
| DMA I2C0 RX transmit request. More...
#define | DMA1_REQUEST_I2C1_TX LL_DMA1_PERIPH_I2C1_TX
| DMA I2C1 TX transmit request. More...
#define | DMA1_REQUEST_I2C1_RX LL_DMA1_PERIPH_I2C1_RX
| DMA I2C1 RX transmit request. More...
#define | DMA1_REQUEST_UART0_TX LL_DMA1_PERIPH_UART0_TX
| DMA UART0 TX transmit request. More...
#define | DMA1_REQUEST_UART0_RX LL_DMA1_PERIPH_UART0_RX
| DMA UART0 RX transmit request. More...
#define | DMA1_REQUEST_UART3_TX LL_DMA1_PERIPH_UART3_TX
| DMA UART3 TX transmit request. More...
#define | DMA1_REQUEST_UART3_RX LL_DMA1_PERIPH_UART3_RX
| DMA UART3 RX transmit request. More...
#define | DMA1_REQUEST_UART4_TX LL_DMA1_PERIPH_UART4_TX
| DMA UART4 TX transmit request. More...
#define | DMA1_REQUEST_UART4_RX LL_DMA1_PERIPH_UART4_RX
| DMA UART4 RX transmit request. More...
#define | DMA1_REQUEST_UART5_TX LL_DMA1_PERIPH_UART5_TX
| DMA UART5 TX transmit request. More...
#define | DMA1_REQUEST_UART5_RX LL_DMA1_PERIPH_UART5_RX
| DMA UART5 RX transmit request. More...
#define | DMA1_REQUEST_MEM LL_DMA1_PERIPH_MEM
| DMA is Memory transmit request. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DMA0_REQUEST_I2C2_RX

#define DMA0_REQUEST_I2C2_RX LL_DMA0_PERIPH_I2C2_RX

DMA I2C2 RX transmit request.

Definition at line 353 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C2_TX

#define DMA0_REQUEST_I2C2_TX LL_DMA0_PERIPH_I2C2_TX

DMA I2C2 TX transmit request.

Definition at line 352 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C3_RX

#define DMA0_REQUEST_I2C3_RX LL_DMA0_PERIPH_I2C3_RX

DMA I2C3 RX transmit request.

Definition at line 355 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C3_TX

#define DMA0_REQUEST_I2C3_TX LL_DMA0_PERIPH_I2C3_TX

DMA I2C3 TX transmit request.

Definition at line 354 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C4_RX

#define DMA0_REQUEST_I2C4_RX LL_DMA0_PERIPH_I2C4_RX

DMA I2C4 RX transmit request.

Definition at line 357 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C4_TX

#define DMA0_REQUEST_I2C4_TX LL_DMA0_PERIPH_I2C4_TX

DMA I2C4 TX transmit request.

Definition at line 356 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C5_RX

#define DMA0_REQUEST_I2C5_RX LL_DMA0_PERIPH_I2C5_RX

DMA I2C5 RX transmit request.

Definition at line 359 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C5_TX

#define DMA0_REQUEST_I2C5_TX LL_DMA0_PERIPH_I2C5_TX

DMA I2C5 TX transmit request.

Definition at line 358 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_MEM

#define DMA0_REQUEST_MEM LL_DMA0_PERIPH_MEM

DMA is Memory transmit request.

Definition at line 361 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_OSPI_RX

#define DMA0_REQUEST_OSPI_RX LL_DMA0_PERIPH_OSPI_RX

DMA OSPI transmit request.

Definition at line 333 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_OSPI_TX

#define DMA0_REQUEST_OSPI_TX LL_DMA0_PERIPH_OSPI_TX

DMA OSPI transmit request.

Definition at line 332 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI0_RX

#define DMA0_REQUEST_QSPI0_RX LL_DMA0_PERIPH_QSPI0_RX

DMA QSPIM0 transmit request.

Definition at line 335 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI0_TX

#define DMA0_REQUEST_QSPI0_TX LL_DMA0_PERIPH_QSPI0_TX

DMA QSPIM0 transmit request.

Definition at line 334 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI1_RX

#define DMA0_REQUEST_QSPI1_RX LL_DMA0_PERIPH_QSPI1_RX

DMA QSPIM1 RX transmit request.

Definition at line 337 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI1_TX

#define DMA0_REQUEST_QSPI1_TX LL_DMA0_PERIPH_QSPI1_TX

DMA QSPIM1 TX transmit request.

Definition at line 336 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SNSADC

#define DMA0_REQUEST_SNSADC LL_DMA0_PERIPH_SNSADC

DMA SNSADC transmit request.

Definition at line 360 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIM_RX

#define DMA0_REQUEST_SPIM_RX LL_DMA0_PERIPH_SPIM_RX

DMA SPIM RX transmit request.

Definition at line 339 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIM_TX

#define DMA0_REQUEST_SPIM_TX LL_DMA0_PERIPH_SPIM_TX

DMA SPIM transmit request.

Definition at line 338 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIS_RX

#define DMA0_REQUEST_SPIS_RX LL_DMA0_PERIPH_SPIS_RX

DMA SPIS RX transmit request.

Definition at line 341 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIS_TX

#define DMA0_REQUEST_SPIS_TX LL_DMA0_PERIPH_SPIS_TX

DMA SPIS TX transmit request.

Definition at line 340 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART0_RX

#define DMA0_REQUEST_UART0_RX LL_DMA0_PERIPH_UART0_RX

DMA UART0 RX transmit request.

Definition at line 343 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART0_TX

#define DMA0_REQUEST_UART0_TX LL_DMA0_PERIPH_UART0_TX

DMA UART0 TX transmit request.

Definition at line 342 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART1_RX

#define DMA0_REQUEST_UART1_RX LL_DMA0_PERIPH_UART1_RX

DMA UART1 RX transmit request.

Definition at line 345 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART1_TX

#define DMA0_REQUEST_UART1_TX LL_DMA0_PERIPH_UART1_TX

DMA UART1 TX transmit request.

Definition at line 344 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART2_RX

#define DMA0_REQUEST_UART2_RX LL_DMA0_PERIPH_UART2_RX

DMA UART2 RX transmit request.

Definition at line 347 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART2_TX

#define DMA0_REQUEST_UART2_TX LL_DMA0_PERIPH_UART2_TX

DMA UART2 TX transmit request.

Definition at line 346 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART3_RX

#define DMA0_REQUEST_UART3_RX LL_DMA0_PERIPH_UART3_RX

DMA UART3 RX transmit request.

Definition at line 349 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART3_TX

#define DMA0_REQUEST_UART3_TX LL_DMA0_PERIPH_UART3_TX

DMA UART3 TX transmit request.

Definition at line 348 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART4_RX

#define DMA0_REQUEST_UART4_RX LL_DMA0_PERIPH_UART4_RX

DMA UART4 RX transmit request.

Definition at line 351 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART4_TX

#define DMA0_REQUEST_UART4_TX LL_DMA0_PERIPH_UART4_TX

DMA UART4 TX transmit request.

Definition at line 350 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_DSPIM_RX

#define DMA1_REQUEST_DSPIM_RX LL_DMA1_PERIPH_DSPIM_RX

DMA DSPIM RX transmit request.

Definition at line 373 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_DSPIM_TX

#define DMA1_REQUEST_DSPIM_TX LL_DMA1_PERIPH_DSPIM_TX

DMA DSPIM TX transmit request.

Definition at line 372 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2C0_RX

#define DMA1_REQUEST_I2C0_RX LL_DMA1_PERIPH_I2C0_RX

DMA I2C0 RX transmit request.

Definition at line 380 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2C0_TX

#define DMA1_REQUEST_I2C0_TX LL_DMA1_PERIPH_I2C0_TX

DMA I2C0 TX transmit request.

Definition at line 379 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2C1_RX

#define DMA1_REQUEST_I2C1_RX LL_DMA1_PERIPH_I2C1_RX

DMA I2C1 RX transmit request.

Definition at line 382 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2C1_TX

#define DMA1_REQUEST_I2C1_TX LL_DMA1_PERIPH_I2C1_TX

DMA I2C1 TX transmit request.

Definition at line 381 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2S_M_RX

#define DMA1_REQUEST_I2S_M_RX LL_DMA1_PERIPH_I2S_M_RX

DMA I2S_M RX transmit request.

Definition at line 375 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2S_M_TX

#define DMA1_REQUEST_I2S_M_TX LL_DMA1_PERIPH_I2S_M_TX

DMA I2S_M TX transmit request.

Definition at line 374 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2S_S_RX

#define DMA1_REQUEST_I2S_S_RX LL_DMA1_PERIPH_I2S_S_RX

DMA I2S_S RX transmit request.

Definition at line 377 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_I2S_S_TX

#define DMA1_REQUEST_I2S_S_TX LL_DMA1_PERIPH_I2S_S_TX

DMA I2S_S TX transmit request.

Definition at line 376 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_MEM

#define DMA1_REQUEST_MEM LL_DMA1_PERIPH_MEM

DMA is Memory transmit request.

Definition at line 391 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_OSPI_RX

#define DMA1_REQUEST_OSPI_RX LL_DMA1_PERIPH_OSPI_RX

DMA OSPI transmit request.

Definition at line 365 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_OSPI_TX

#define DMA1_REQUEST_OSPI_TX LL_DMA1_PERIPH_OSPI_TX

DMA OSPI transmit request.

Definition at line 364 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_PDM_TX

#define DMA1_REQUEST_PDM_TX LL_DMA1_PERIPH_PDM_TX

DMA PDM TX transmit request.

Definition at line 378 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_QSPI1_RX

#define DMA1_REQUEST_QSPI1_RX LL_DMA1_PERIPH_QSPI1_RX

DMA QSPIM1 RX transmit request.

Definition at line 367 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_QSPI1_TX

#define DMA1_REQUEST_QSPI1_TX LL_DMA1_PERIPH_QSPI1_TX

DMA QSPIM1 TX transmit request.

Definition at line 366 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_QSPI2_RX

#define DMA1_REQUEST_QSPI2_RX LL_DMA1_PERIPH_QSPI2_RX

DMA QSPIM2 RX transmit request.

Definition at line 369 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_QSPI2_TX

#define DMA1_REQUEST_QSPI2_TX LL_DMA1_PERIPH_QSPI2_TX

DMA QSPIM2 TX transmit request.

Definition at line 368 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_SPIM_RX

#define DMA1_REQUEST_SPIM_RX LL_DMA1_PERIPH_SPIM_RX

DMA SPIM RX transmit request.

Definition at line 371 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_SPIM_TX

#define DMA1_REQUEST_SPIM_TX LL_DMA1_PERIPH_SPIM_TX

DMA SPIM transmit request.

Definition at line 370 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART0_RX

#define DMA1_REQUEST_UART0_RX LL_DMA1_PERIPH_UART0_RX

DMA UART0 RX transmit request.

Definition at line 384 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART0_TX

#define DMA1_REQUEST_UART0_TX LL_DMA1_PERIPH_UART0_TX

DMA UART0 TX transmit request.

Definition at line 383 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART3_RX

#define DMA1_REQUEST_UART3_RX LL_DMA1_PERIPH_UART3_RX

DMA UART3 RX transmit request.

Definition at line 386 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART3_TX

#define DMA1_REQUEST_UART3_TX LL_DMA1_PERIPH_UART3_TX

DMA UART3 TX transmit request.

Definition at line 385 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART4_RX

#define DMA1_REQUEST_UART4_RX LL_DMA1_PERIPH_UART4_RX

DMA UART4 RX transmit request.

Definition at line 388 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART4_TX

#define DMA1_REQUEST_UART4_TX LL_DMA1_PERIPH_UART4_TX

DMA UART4 TX transmit request.

Definition at line 387 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART5_RX

#define DMA1_REQUEST_UART5_RX LL_DMA1_PERIPH_UART5_RX

DMA UART5 RX transmit request.

Definition at line 390 of file gr55xx_hal_dma.h.

## ◆ DMA1_REQUEST_UART5_TX

#define DMA1_REQUEST_UART5_TX LL_DMA1_PERIPH_UART5_TX

DMA UART5 TX transmit request.

Definition at line 389 of file gr55xx_hal_dma.h.