Macros | Typedefs | Enumerations | Functions
graphics_dc_lcd_drv.h File Reference

Header file containing functions prototypes of Graphics library. More...

`#include "grx_sys.h"`
`#include "app_graphics_dc.h"`
Include dependency graph for graphics_dc_lcd_drv.h:

Go to the source code of this file.

## Macros
#define | LCD_RES_390 0
| The resolution is 390X390. More...
#define | LCD_RES_454 1
| The resolution is 454X454. More...
#define | LCD_RES_360 2
| The resolution is 360X360. More...
#define | IS_SK_BOARD

## Typedefs
typedef uint32_t | lcd_res_e
| The LCD resolution type More...

## Enumerations
enum | lcd_pixel_mode_e { LCD_PIXEL_mode_16bit = 0, LCD_PIXEL_mode_24bit }
| Lcd pixel mode. More...

## Functions
void | graphics_dc_rm69330_qspi_lcd_init (lcd_res_e res, lcd_pixel_mode_e pixel_mode, graphics_dc_mipi_format_e mipi_format)
| DC rm69330 qspi lcd init. More...
void | graphics_dc_rm69330_qspi_lcd_test (lcd_res_e res, lcd_pixel_mode_e pixel_mode, app_graphics_dc_frame_timing_e frame_timing, graphics_dc_mipi_format_e mipi_format)
| DC rm69330 lcd test. More...
void | graphics_dc_rm69330_qspi_lcd_set_show_area (uint16_t x1, uint16_t x2, uint16_t y1, uint16_t y2)
| DC rm69330 lcd set show area for qspi output. More...
void | graphics_dc_rm69330_qspi_send_frame (app_graphics_dc_framelayer_t layer0, uint32_t lcd_w, uint32_t lcd_h)
| DC rm69330 lcd send one frame data. More...
void | graphics_dc_st7789_dspi_lcd_init (lcd_res_e res, lcd_pixel_mode_e pixel_mode, graphics_dc_mipi_format_e mipi_format)
| DC rm69330 dspi lcd init. More...
void | graphics_dc_st7789_dspi_lcd_set_show_area (uint16_t x1, uint16_t x2, uint16_t y1, uint16_t y2)
| DC rm69330 lcd set show area for dspi output. More...
void | graphics_dc_rm69330_spi_lcd_init (lcd_res_e res, lcd_pixel_mode_e pixel_mode, graphics_dc_mipi_format_e mipi_format)
| DC rm69330 spi lcd init. More...
void | graphics_dc_rm69330_spi_lcd_set_show_area (uint16_t x1, uint16_t x2, uint16_t y1, uint16_t y2)
| DC rm69330 lcd set show area for spi output. More...
void | graphics_dc_am139_qspi_lcd_init (lcd_res_e res, lcd_pixel_mode_e pixel_mode, graphics_dc_mipi_format_e mipi_format)
| DC fls-amo139 qspi lcd init. More...
void | graphics_dc_am139_qspi_lcd_set_show_area (uint16_t x1, uint16_t x2, uint16_t y1, uint16_t y2)
| DC fls-amo139 lcd set show area for qspi output. More...
void | graphics_dc_am139_qspi_send_frame (app_graphics_dc_framelayer_t layer0, uint32_t lcd_w, uint32_t lcd_h)
| DC fls-amo139 lcd send one frame data. More...

## Detailed Description

Header file containing functions prototypes of Graphics library.

Author
  BLE Driver Team

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file graphics_dc_lcd_drv.h.