Macros
DMA Priority Level
Peripheral Driver » HAL Driver » DMA » Defines » DMA Exported Constants
Collaboration diagram for DMA Priority Level:

## Macros
#define | DMA_PRIORITY_LOW LL_DMA_PRIORITY_0
| Priority level : Low More...
#define | DMA_PRIORITY_MEDIUM LL_DMA_PRIORITY_1
| Priority level : Medium More...
#define | DMA_PRIORITY_HIGH LL_DMA_PRIORITY_2
| Priority level : High More...
#define | DMA_PRIORITY_VERY_HIGH LL_DMA_PRIORITY_3
| Priority level : Very High. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DMA_PRIORITY_HIGH

#define DMA_PRIORITY_HIGH LL_DMA_PRIORITY_2

Priority level : High

Definition at line 448 of file gr55xx_hal_dma.h.

## ◆ DMA_PRIORITY_LOW

#define DMA_PRIORITY_LOW LL_DMA_PRIORITY_0

Priority level : Low

Definition at line 446 of file gr55xx_hal_dma.h.

## ◆ DMA_PRIORITY_MEDIUM

#define DMA_PRIORITY_MEDIUM LL_DMA_PRIORITY_1

Priority level : Medium

Definition at line 447 of file gr55xx_hal_dma.h.

## ◆ DMA_PRIORITY_VERY_HIGH

#define DMA_PRIORITY_VERY_HIGH LL_DMA_PRIORITY_3

Priority level : Very High.

Definition at line 449 of file gr55xx_hal_dma.h.