Macros
SPI Data Size
Peripheral Driver » HAL Driver » SPI » Defines » SPI Exported Constants
Collaboration diagram for SPI Data Size:

## Macros
#define | SPI_DATASIZE_4BIT LL_SPI_DATASIZE_4BIT
| 4-bit serial data transfer More...
#define | SPI_DATASIZE_5BIT LL_SPI_DATASIZE_5BIT
| 5-bit serial data transfer More...
#define | SPI_DATASIZE_6BIT LL_SPI_DATASIZE_6BIT
| 6-bit serial data transfer More...
#define | SPI_DATASIZE_7BIT LL_SPI_DATASIZE_7BIT
| 7-bit serial data transfer More...
#define | SPI_DATASIZE_8BIT LL_SPI_DATASIZE_8BIT
| 8-bit serial data transfer More...
#define | SPI_DATASIZE_9BIT LL_SPI_DATASIZE_9BIT
| 9-bit serial data transfer More...
#define | SPI_DATASIZE_10BIT LL_SPI_DATASIZE_10BIT
| 10-bit serial data transfer More...
#define | SPI_DATASIZE_11BIT LL_SPI_DATASIZE_11BIT
| 11-bit serial data transfer More...
#define | SPI_DATASIZE_12BIT LL_SPI_DATASIZE_12BIT
| 12-bit serial data transfer More...
#define | SPI_DATASIZE_13BIT LL_SPI_DATASIZE_13BIT
| 13-bit serial data transfer More...
#define | SPI_DATASIZE_14BIT LL_SPI_DATASIZE_14BIT
| 14-bit serial data transfer More...
#define | SPI_DATASIZE_15BIT LL_SPI_DATASIZE_15BIT
| 15-bit serial data transfer More...
#define | SPI_DATASIZE_16BIT LL_SPI_DATASIZE_16BIT
| 16-bit serial data transfer More...
#define | SPI_DATASIZE_17BIT LL_SPI_DATASIZE_17BIT
| 17-bit serial data transfer More...
#define | SPI_DATASIZE_18BIT LL_SPI_DATASIZE_18BIT
| 18-bit serial data transfer More...
#define | SPI_DATASIZE_19BIT LL_SPI_DATASIZE_19BIT
| 19-bit serial data transfer More...
#define | SPI_DATASIZE_20BIT LL_SPI_DATASIZE_20BIT
| 20-bit serial data transfer More...
#define | SPI_DATASIZE_21BIT LL_SPI_DATASIZE_21BIT
| 21-bit serial data transfer More...
#define | SPI_DATASIZE_22BIT LL_SPI_DATASIZE_22BIT
| 22-bit serial data transfer More...
#define | SPI_DATASIZE_23BIT LL_SPI_DATASIZE_23BIT
| 23-bit serial data transfer More...
#define | SPI_DATASIZE_24BIT LL_SPI_DATASIZE_24BIT
| 24-bit serial data transfer More...
#define | SPI_DATASIZE_25BIT LL_SPI_DATASIZE_25BIT
| 25-bit serial data transfer More...
#define | SPI_DATASIZE_26BIT LL_SPI_DATASIZE_26BIT
| 26-bit serial data transfer More...
#define | SPI_DATASIZE_27BIT LL_SPI_DATASIZE_27BIT
| 27-bit serial data transfer More...
#define | SPI_DATASIZE_28BIT LL_SPI_DATASIZE_28BIT
| 28-bit serial data transfer More...
#define | SPI_DATASIZE_29BIT LL_SPI_DATASIZE_29BIT
| 29-bit serial data transfer More...
#define | SPI_DATASIZE_30BIT LL_SPI_DATASIZE_30BIT
| 30-bit serial data transfer More...
#define | SPI_DATASIZE_31BIT LL_SPI_DATASIZE_31BIT
| 31-bit serial data transfer More...
#define | SPI_DATASIZE_32BIT LL_SPI_DATASIZE_32BIT
| 32-bit serial data transfer More...

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_DATASIZE_10BIT

#define SPI_DATASIZE_10BIT LL_SPI_DATASIZE_10BIT

10-bit serial data transfer

Definition at line 309 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_11BIT

#define SPI_DATASIZE_11BIT LL_SPI_DATASIZE_11BIT

11-bit serial data transfer

Definition at line 310 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_12BIT

#define SPI_DATASIZE_12BIT LL_SPI_DATASIZE_12BIT

12-bit serial data transfer

Definition at line 311 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_13BIT

#define SPI_DATASIZE_13BIT LL_SPI_DATASIZE_13BIT

13-bit serial data transfer

Definition at line 312 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_14BIT

#define SPI_DATASIZE_14BIT LL_SPI_DATASIZE_14BIT

14-bit serial data transfer

Definition at line 313 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_15BIT

#define SPI_DATASIZE_15BIT LL_SPI_DATASIZE_15BIT

15-bit serial data transfer

Definition at line 314 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_16BIT

#define SPI_DATASIZE_16BIT LL_SPI_DATASIZE_16BIT

16-bit serial data transfer

Definition at line 315 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_17BIT

#define SPI_DATASIZE_17BIT LL_SPI_DATASIZE_17BIT

17-bit serial data transfer

Definition at line 316 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_18BIT

#define SPI_DATASIZE_18BIT LL_SPI_DATASIZE_18BIT

18-bit serial data transfer

Definition at line 317 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_19BIT

#define SPI_DATASIZE_19BIT LL_SPI_DATASIZE_19BIT

19-bit serial data transfer

Definition at line 318 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_20BIT

#define SPI_DATASIZE_20BIT LL_SPI_DATASIZE_20BIT

20-bit serial data transfer

Definition at line 319 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_21BIT

#define SPI_DATASIZE_21BIT LL_SPI_DATASIZE_21BIT

21-bit serial data transfer

Definition at line 320 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_22BIT

#define SPI_DATASIZE_22BIT LL_SPI_DATASIZE_22BIT

22-bit serial data transfer

Definition at line 321 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_23BIT

#define SPI_DATASIZE_23BIT LL_SPI_DATASIZE_23BIT

23-bit serial data transfer

Definition at line 322 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_24BIT

#define SPI_DATASIZE_24BIT LL_SPI_DATASIZE_24BIT

24-bit serial data transfer

Definition at line 323 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_25BIT

#define SPI_DATASIZE_25BIT LL_SPI_DATASIZE_25BIT

25-bit serial data transfer

Definition at line 324 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_26BIT

#define SPI_DATASIZE_26BIT LL_SPI_DATASIZE_26BIT

26-bit serial data transfer

Definition at line 325 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_27BIT

#define SPI_DATASIZE_27BIT LL_SPI_DATASIZE_27BIT

27-bit serial data transfer

Definition at line 326 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_28BIT

#define SPI_DATASIZE_28BIT LL_SPI_DATASIZE_28BIT

28-bit serial data transfer

Definition at line 327 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_29BIT

#define SPI_DATASIZE_29BIT LL_SPI_DATASIZE_29BIT

29-bit serial data transfer

Definition at line 328 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_30BIT

#define SPI_DATASIZE_30BIT LL_SPI_DATASIZE_30BIT

30-bit serial data transfer

Definition at line 329 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_31BIT

#define SPI_DATASIZE_31BIT LL_SPI_DATASIZE_31BIT

31-bit serial data transfer

Definition at line 330 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_32BIT

#define SPI_DATASIZE_32BIT LL_SPI_DATASIZE_32BIT

32-bit serial data transfer

Definition at line 331 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_4BIT

#define SPI_DATASIZE_4BIT LL_SPI_DATASIZE_4BIT

4-bit serial data transfer

Definition at line 303 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_5BIT

#define SPI_DATASIZE_5BIT LL_SPI_DATASIZE_5BIT

5-bit serial data transfer

Definition at line 304 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_6BIT

#define SPI_DATASIZE_6BIT LL_SPI_DATASIZE_6BIT

6-bit serial data transfer

Definition at line 305 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_7BIT

#define SPI_DATASIZE_7BIT LL_SPI_DATASIZE_7BIT

7-bit serial data transfer

Definition at line 306 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_8BIT

#define SPI_DATASIZE_8BIT LL_SPI_DATASIZE_8BIT

8-bit serial data transfer

Definition at line 307 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_9BIT

#define SPI_DATASIZE_9BIT LL_SPI_DATASIZE_9BIT

9-bit serial data transfer

Definition at line 308 of file gr55xx_hal_spi.h.