Macros
COMP Input Channel Select
Peripheral Driver » HAL Driver » COMP » Defines » COMP Exported Constants
Collaboration diagram for COMP Input Channel Select:

## Macros
#define | COMP_INPUT_SRC_IO0 LL_COMP_INPUT_SRC_IO0
| Set MSIO_0 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO1 LL_COMP_INPUT_SRC_IO1
| Set MSIO_1 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO2 LL_COMP_INPUT_SRC_IO2
| Set MSIO_2 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO3 LL_COMP_INPUT_SRC_IO3
| Set MSIO_3 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO4 LL_COMP_INPUT_SRC_IO4
| Set MSIO_4 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO5 LL_COMP_INPUT_SRC_IO5
| Set MSIO_5 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO6 LL_COMP_INPUT_SRC_IO6
| Set MSIO_6 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_IO7 LL_COMP_INPUT_SRC_IO7
| Set MSIO_7 as inputs for the comparator. More...
#define | COMP_INPUT_SRC_VBAT LL_COMP_INPUT_SRC_VBAT
| Set VBATT as inputs for the comparator More...
#define | COMP_INPUT_SRC_VREF LL_COMP_INPUT_SRC_VREF
| Set VREF as inputs for the comparator More...

## Detailed Description

## Macro Definition Documentation

## ◆ COMP_INPUT_SRC_IO0

#define COMP_INPUT_SRC_IO0 LL_COMP_INPUT_SRC_IO0

Set MSIO_0 as inputs for the comparator.

Definition at line 171 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO1

#define COMP_INPUT_SRC_IO1 LL_COMP_INPUT_SRC_IO1

Set MSIO_1 as inputs for the comparator.

Definition at line 172 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO2

#define COMP_INPUT_SRC_IO2 LL_COMP_INPUT_SRC_IO2

Set MSIO_2 as inputs for the comparator.

Definition at line 173 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO3

#define COMP_INPUT_SRC_IO3 LL_COMP_INPUT_SRC_IO3

Set MSIO_3 as inputs for the comparator.

Definition at line 174 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO4

#define COMP_INPUT_SRC_IO4 LL_COMP_INPUT_SRC_IO4

Set MSIO_4 as inputs for the comparator.

Definition at line 175 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO5

#define COMP_INPUT_SRC_IO5 LL_COMP_INPUT_SRC_IO5

Set MSIO_5 as inputs for the comparator.

Definition at line 176 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO6

#define COMP_INPUT_SRC_IO6 LL_COMP_INPUT_SRC_IO6

Set MSIO_6 as inputs for the comparator.

Definition at line 177 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_IO7

#define COMP_INPUT_SRC_IO7 LL_COMP_INPUT_SRC_IO7

Set MSIO_7 as inputs for the comparator.

Definition at line 178 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_VBAT

#define COMP_INPUT_SRC_VBAT LL_COMP_INPUT_SRC_VBAT

Set VBATT as inputs for the comparator

Definition at line 179 of file gr55xx_hal_comp.h.

## ◆ COMP_INPUT_SRC_VREF

#define COMP_INPUT_SRC_VREF LL_COMP_INPUT_SRC_VREF

Set VREF as inputs for the comparator

Definition at line 180 of file gr55xx_hal_comp.h.