Macros
Watchdog Timer clock select defines
Peripheral Driver » LL Driver » AON_WDT » Defines » Exported Constants
Collaboration diagram for Watchdog Timer clock select defines:

## Macros
#define | LL_AON_WD_TIMER_CLK_SEL_RNG (0x0U << AON_WDT_CLK_SEL_Pos)
| Select RNG clcok source More...
#define | LL_AON_WD_TIMER_CLK_SEL_XO (0x1U << AON_WDT_CLK_SEL_Pos)
| Select XO clcok source More...
#define | LL_AON_WD_TIMER_CLK_SEL_RNG2 (0x2U << AON_WDT_CLK_SEL_Pos)
| Select RNG2 clcok source More...
#define | LL_AON_WD_TIMER_CLK_SEL_RTC (0x3U << AON_WDT_CLK_SEL_Pos)
| Select RTC clcok source More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_WD_TIMER_CLK_SEL_RNG

#define LL_AON_WD_TIMER_CLK_SEL_RNG (0x0U << AON_WDT_CLK_SEL_Pos)

Select RNG clcok source

Definition at line 71 of file gr55xx_ll_aon_wdt.h.

## ◆ LL_AON_WD_TIMER_CLK_SEL_RNG2

#define LL_AON_WD_TIMER_CLK_SEL_RNG2 (0x2U << AON_WDT_CLK_SEL_Pos)

Select RNG2 clcok source

Definition at line 73 of file gr55xx_ll_aon_wdt.h.

## ◆ LL_AON_WD_TIMER_CLK_SEL_RTC

#define LL_AON_WD_TIMER_CLK_SEL_RTC (0x3U << AON_WDT_CLK_SEL_Pos)

Select RTC clcok source

Definition at line 74 of file gr55xx_ll_aon_wdt.h.

## ◆ LL_AON_WD_TIMER_CLK_SEL_XO

#define LL_AON_WD_TIMER_CLK_SEL_XO (0x1U << AON_WDT_CLK_SEL_Pos)

Select XO clcok source

Definition at line 72 of file gr55xx_ll_aon_wdt.h.