Enumerations
Enumerations
SYSTEM » Platform SDK
Collaboration diagram for Enumerations:

## Enumerations
enum | table_idx_t { XIP_64M = 0, XIP_48M, XIP_XO16M, XIP_24M, XIP_16M, XIP_32M, MIRROR_64M, MIRROR_48M, MIRROR_XO16M, MIRROR_24M, MIRROR_16M, MIRROR_32M }
| system clock and run mode. More...
enum | sdk_clock_type_t { RNG_OSC_CLK = 0, RTC_OSC_CLK, RNG_OSC_CLK2 }
| sdk clock type. More...
enum | mem_power_t { MEM_POWER_FULL_MODE = 0, MEM_POWER_AUTO_MODE }
| memory power setting mode. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ mem_power_t

enum mem_power_t

memory power setting mode.

Enumerator
MEM_POWER_FULL_MODE | Full mode.
MEM_POWER_AUTO_MODE | Auto mode.

Definition at line 100 of file platform_sdk.h.

## ◆ sdk_clock_type_t

enum sdk_clock_type_t

sdk clock type.

Enumerator
RNG_OSC_CLK | RNG OSC CLOCK.
RTC_OSC_CLK | RTC OSC CLOCK.
RNG_OSC_CLK2 | RNG OSC CLOCK2.

Definition at line 91 of file platform_sdk.h.

## ◆ table_idx_t

enum table_idx_t

system clock and run mode.

Enumerator
XIP_64M | XIP 64M.
XIP_48M | XIP 48M.
XIP_XO16M | XIP XO 16M.
XIP_24M | XIP 24M.
XIP_16M | XIP 16M.
XIP_32M | XIP 32M.
MIRROR_64M | MIRROR 64M.
MIRROR_48M | MIRROR 48M.
MIRROR_XO16M | MIRROR X) 16M.
MIRROR_24M | MIRROR 24M.
MIRROR_16M | MIRROR 16M.
MIRROR_32M | MIRROR 32M.

Definition at line 74 of file platform_sdk.h.