Macros
UART Number of Data Bits
Peripheral Driver » HAL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for UART Number of Data Bits:

## Macros
#define | UART_DATABITS_5 LL_UART_DATABITS_5B
| UART frame with 5 data bits. More...
#define | UART_DATABITS_6 LL_UART_DATABITS_6B
| UART frame with 6 data bits. More...
#define | UART_DATABITS_7 LL_UART_DATABITS_7B
| UART frame with 7 data bits. More...
#define | UART_DATABITS_8 LL_UART_DATABITS_8B
| UART frame with 8 data bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ UART_DATABITS_5

#define UART_DATABITS_5 LL_UART_DATABITS_5B

UART frame with 5 data bits.

Definition at line 255 of file gr55xx_hal_uart.h.

## ◆ UART_DATABITS_6

#define UART_DATABITS_6 LL_UART_DATABITS_6B

UART frame with 6 data bits.

Definition at line 256 of file gr55xx_hal_uart.h.

## ◆ UART_DATABITS_7

#define UART_DATABITS_7 LL_UART_DATABITS_7B

UART frame with 7 data bits.

Definition at line 257 of file gr55xx_hal_uart.h.

## ◆ UART_DATABITS_8

#define UART_DATABITS_8 LL_UART_DATABITS_8B

UART frame with 8 data bits.

Definition at line 258 of file gr55xx_hal_uart.h.