Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants
Collaboration diagram for InitStrcut default configuartion:

## Macros
#define | LL_I2C_DEFAULT_CONFIG
| LL I2C InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_DEFAULT_CONFIG

#define LL_I2C_DEFAULT_CONFIG

Value:
{ \
.speed = LL_I2C_SPEED_400K, \
.own_address = 0x55U, \
.own_addr_size = LL_I2C_OWNADDRESS_7BIT, \
}

LL I2C InitStrcut default configuartion.

Definition at line 295 of file gr55xx_ll_i2c.h.

LL_I2C_OWNADDRESS_7BIT
#define LL_I2C_OWNADDRESS_7BIT
Own address 1 is a 7-bit address.
Definition: gr55xx_ll_i2c.h:179
LL_I2C_SPEED_400K
#define LL_I2C_SPEED_400K
Fast Speed.
Definition: gr55xx_ll_i2c.h:206