Functions
ble_enh_prf.h File Reference

BLE PRF ENHANCED API. More...

`#include "ble_error.h"`
`#include "ble_att.h"`
`#include "ble_gatts.h"`
`#include "ble_gattc.h"`
`#include "ble_gatt.h"`
`#include "ble_event.h"`
Include dependency graph for ble_enh_prf.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Functions
uint16_t | ble_gatts_enh_prf_add (ble_gatts_create_db_t *p_gatts_db, ble_evt_handler_t evt_handler)
| Add a server profile by providing its detailed information, including manager callback functions and GATT server callback functions. More...
uint16_t | ble_gatts_enh_read_cfm (uint8_t conn_idx, uint16_t cid, const ble_gatts_read_cfm_t *p_param)
| Respond to an attribute read request. More...
uint16_t | ble_gatts_enh_write_cfm (uint8_t conn_idx, uint16_t cid, const ble_gatts_write_cfm_t *p_param)
| Respond to an attribute write request. More...
uint16_t | ble_gatts_enh_prepare_write_cfm (uint8_t conn_idx, uint16_t cid, const ble_gatts_prep_write_cfm_t *p_param)
| Respond to an attribute prepare write request. More...
uint16_t | ble_gatts_enh_noti_ind (uint8_t conn_idx, uint16_t cid, const ble_gatts_noti_ind_t *p_param)
| Send out a notification or an indication. More...
uint16_t | ble_gatts_enh_mult_noti (uint8_t conn_idx, uint16_t cid, const ble_gatts_noti_multiple_t *p_param)
| Send out Multiple Variable Length Notifications. More...
uint16_t | ble_gattc_prf_enh_add (uint8_t *p_client_prf_id, ble_evt_handler_t evt_handler)
| Add a client profile by providing its detail information, including manager callback functions and GATT client callback functions. More...
uint16_t | ble_gattc_enh_prf_services_browse (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, const ble_uuid_t *p_srvc_uuid)
| Profile client Browse Specific Primary Service information on remote GATT server. More...
uint16_t | ble_gattc_enh_prf_primary_services_discover (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, const ble_uuid_t *p_srvc_uuid)
| Profile client Discover Primary Services on remote GATT server. More...
uint16_t | ble_gattc_enh_prf_included_services_discover (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, uint16_t start_hdl, uint16_t end_hdl)
| Profile client Discover Included Services on remote GATT server. More...
uint16_t | ble_gattc_enh_prf_char_discover (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, ble_gattc_disc_char_t *p_disc_char)
| Profile client Discover Characteristics on remote GATT server. More...
uint16_t | ble_gattc_enh_prf_char_desc_discover (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, uint16_t start_hdl, uint16_t end_hdl)
| Profile client Discover Characteristics Descriptors on remote GATT server. More...
uint16_t | ble_gattc_enh_prf_read (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, uint16_t handle, uint16_t offset)
| Profile client Read Attribute from remote GATT server. More...
uint16_t | ble_gattc_enh_prf_read_by_uuid (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, ble_gattc_read_by_uuid_t *p_read_by_uuid)
| Profile client Read Attribute by UUID. More...
uint16_t | ble_gattc_enh_prf_read_multiple (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, const ble_gattc_read_multiple_t *p_param)
| Profile client Initiate a Read Multiple Characteristic Values procedure. More...
uint16_t | ble_gattc_enh_prf_write (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, ble_gattc_write_attr_value_t *p_write_attr_value)
| Profile client Write (Long) Characteristic (Descriptor) Value. More...
uint16_t | ble_gattc_enh_prf_write_prepare (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, ble_gattc_write_attr_value_t *p_write_attr_value)
| Profile client Prepare Long/Reliable Write to remote GATT server. More...
uint16_t | ble_gattc_enh_prf_write_execute (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, bool execute)
| Profile client Execute Reliable/Long Write to remote GATT server. More...
uint16_t | ble_gattc_enh_prf_write_no_resp (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, ble_gattc_write_no_resp_t *p_write_no_resp)
| Profile client Write Attribute to remote GATT server (without response). More...
uint16_t | ble_gattc_enh_prf_indicate_cfm (uint8_t prf_id, uint8_t conn_idx, uint16_t cid, uint16_t handle)
| Profile client Confirm Reception of Indication. More...

## Detailed Description

BLE PRF ENHANCED API.

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file ble_enh_prf.h.