Public Attributes | List of all members
iso_rm_data_path_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for removing data path. More...

`#include <ble_iso.h>`

## Public Attributes
uint16_t | conn_hdl
| Connection handle of a CIS or BIS. More...
uint8_t | direction
| Specifies the input data transport path, see iso_data_path_direction_t. More...

## Detailed Description

The parameter for removing data path.

Definition at line 313 of file ble_iso.h.

## Member Data Documentation

## ◆ conn_hdl

uint16_t iso_rm_data_path_t::conn_hdl

Connection handle of a CIS or BIS.

Definition at line 315 of file ble_iso.h.

## ◆ direction

uint8_t iso_rm_data_path_t::direction

Specifies the input data transport path, see iso_data_path_direction_t.

Definition at line 316 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h