Public Attributes | List of all members
iso_cis_req_evt_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for cis request event. More...

`#include <ble_iso.h>`

## Public Attributes
uint16_t | conn_idx
| Connection index of the ACL. More...
uint16_t | cis_hdl
| Connection handle of CIS (Range 0x0000-0x0EFF). More...
uint8_t | cig_id
| Identifier of the CIG (Range 0x00-0xEF). More...
uint8_t | cis_id
| Identifier of the CIS (Range 0x00-0xEF). More...

## Detailed Description

The parameter for cis request event.

Definition at line 459 of file ble_iso.h.

## Member Data Documentation

## ◆ cig_id

uint8_t iso_cis_req_evt_t::cig_id

Identifier of the CIG (Range 0x00-0xEF).

Definition at line 463 of file ble_iso.h.

## ◆ cis_hdl

uint16_t iso_cis_req_evt_t::cis_hdl

Connection handle of CIS (Range 0x0000-0x0EFF).

Definition at line 462 of file ble_iso.h.

## ◆ cis_id

uint8_t iso_cis_req_evt_t::cis_id

Identifier of the CIS (Range 0x00-0xEF).

Definition at line 464 of file ble_iso.h.

## ◆ conn_idx

uint16_t iso_cis_req_evt_t::conn_idx

Connection index of the ACL.

Definition at line 461 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h