Macros
RTC Timer clock select defines
Peripheral Driver » LL Driver » RTC » Defines » RTC Exported Constants

## Macros
#define | LL_RTC_TIMER_CLK_SEL_RNG (0x0U << RTC_CLK_SEL_Pos)
#define | LL_RTC_TIMER_CLK_SEL_XO (0x1U << RTC_CLK_SEL_Pos)
#define | LL_RTC_TIMER_CLK_SEL_RNG2 (0x2U << RTC_CLK_SEL_Pos)
#define | LL_RTC_TIMER_CLK_SEL_RTC (0x3U << RTC_CLK_SEL_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_RTC_TIMER_CLK_SEL_RNG

#define LL_RTC_TIMER_CLK_SEL_RNG (0x0U << RTC_CLK_SEL_Pos)

Select RNG clcok source

Definition at line 86 of file gr55xx_ll_rtc.h.

## ◆ LL_RTC_TIMER_CLK_SEL_RNG2

#define LL_RTC_TIMER_CLK_SEL_RNG2 (0x2U << RTC_CLK_SEL_Pos)

Select RNG2 clcok source

Definition at line 88 of file gr55xx_ll_rtc.h.

## ◆ LL_RTC_TIMER_CLK_SEL_RTC

#define LL_RTC_TIMER_CLK_SEL_RTC (0x3U << RTC_CLK_SEL_Pos)

Select RTC clcok source

Definition at line 89 of file gr55xx_ll_rtc.h.

## ◆ LL_RTC_TIMER_CLK_SEL_XO

#define LL_RTC_TIMER_CLK_SEL_XO (0x1U << RTC_CLK_SEL_Pos)

Select XO clcok source

Definition at line 87 of file gr55xx_ll_rtc.h.