Modules | Macros
PDM Exported Constants
Peripheral Driver » HAL Driver » PDM » Defines

## Modules
| PDM Error Code

## Macros
#define | PDM_SAMPLE_RATE_15_625K LL_PDM_SAMPLE_RATE_15_625K
| PDM sample rate. More...
#define | PDM_SAMPLE_RATE_16K LL_PDM_SAMPLE_RATE_16K
#define | PDM_SAMPLE_RATE_8K LL_PDM_SAMPLE_RATE_8K
#define | PDM_MODE_LEFT LL_PDM_MODE_LEFT
| PDM operation mode. More...
#define | PDM_MODE_RIGHT LL_PDM_MODE_RIGHT
#define | PDM_MODE_STEREO LL_PDM_MODE_STEREO

## Detailed Description

## Macro Definition Documentation

## ◆ PDM_MODE_LEFT

#define PDM_MODE_LEFT LL_PDM_MODE_LEFT

PDM operation mode.

PDM left mono.

Definition at line 169 of file gr55xx_hal_pdm.h.

## ◆ PDM_MODE_RIGHT

#define PDM_MODE_RIGHT LL_PDM_MODE_RIGHT

PDM right mono.

Definition at line 170 of file gr55xx_hal_pdm.h.

## ◆ PDM_MODE_STEREO

#define PDM_MODE_STEREO LL_PDM_MODE_STEREO

PDM stereo mono.

Definition at line 171 of file gr55xx_hal_pdm.h.

## ◆ PDM_SAMPLE_RATE_15_625K

#define PDM_SAMPLE_RATE_15_625K LL_PDM_SAMPLE_RATE_15_625K

PDM sample rate.

PDM sample rate 15.625K.

Definition at line 162 of file gr55xx_hal_pdm.h.

## ◆ PDM_SAMPLE_RATE_16K

#define PDM_SAMPLE_RATE_16K LL_PDM_SAMPLE_RATE_16K

PDM sample rate 16K.

Definition at line 163 of file gr55xx_hal_pdm.h.

## ◆ PDM_SAMPLE_RATE_8K

#define PDM_SAMPLE_RATE_8K LL_PDM_SAMPLE_RATE_8K

PDM sample rate 8K.

Definition at line 164 of file gr55xx_hal_pdm.h.