Macros
Force Clock OFF
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_FRC_UART0_PCLK MCU_SUB_FORCE_UART0_PCLK
#define | LL_CGC_FRC_UART1_PCLK MCU_SUB_FORCE_UART1_PCLK
#define | LL_CGC_FRC_UART2_PCLK MCU_SUB_FORCE_UART2_PCLK
#define | LL_CGC_FRC_UART3_PCLK MCU_SUB_FORCE_UART3_PCLK
#define | LL_CGC_FRC_I2C0_PCLK MCU_SUB_FORCE_I2C0_PCLK
#define | LL_CGC_FRC_I2C1_PCLK MCU_SUB_FORCE_I2C1_PCLK
#define | LL_CGC_FRC_I2C2_PCLK MCU_SUB_FORCE_I2C2_PCLK
#define | LL_CGC_FRC_I2C3_PCLK MCU_SUB_FORCE_I2C3_PCLK
#define | LL_CGC_FRC_QSPI0_PCLK MCU_SUB_FORCE_QSPI0_PCLK
#define | LL_CGC_FRC_QSPI1_PCLK MCU_SUB_FORCE_QSPI1_PCLK
#define | LL_CGC_FRC_QSPI2_PCLK MCU_SUB_FORCE_QSPI2_PCLK
#define | LL_CGC_FRC_SPI_M_PCLK MCU_SUB_FORCE_SPI_M_PCLK
#define | LL_CGC_FRC_SPI_S_PCLK MCU_SUB_FORCE_SPI_S_PCLK
#define | LL_CGC_FRC_I2S_PCLK MCU_SUB_FORCE_I2S_PCLK
#define | LL_CGC_FRC_I2S_S_PCLK MCU_SUB_FORCE_I2S_S_PCLK
#define | LL_CGC_FRC_DSPI_PCLK MCU_SUB_FORCE_DSPI_PCLK
#define | LL_CGC_FRC_PDM_PCLK MCU_SUB_FORCE_PDM_PCLK
#define | LL_CGC_FRC_PWM_0_PCLK MCU_SUB_FORCE_PWM_0_PCLK
#define | LL_CGC_FRC_PWM_1_PCLK MCU_SUB_FORCE_PWM_1_PCLK
#define | LL_CGC_FRC_VTTBL_PCLK MCU_SUB_FORCE_VTTBL_PCLK
#define | LL_CGC_FRC_SECU_DIV4_PCLK MCU_SUB_FORCE_SECU_DIV4_PCLK
#define | LL_CGC_FRC_XQSPI_DIV4_PCLK MCU_SUB_FORCE_XQSPI_DIV4_PCLK
#define | LL_CGC_FRC_SERIALS_HCLK2 ((uint32_t)0x705E03CFUL)
#define | LL_CGC_FRC_ALL_HCLK2 ((uint32_t)0x7A7FC3CFUL)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_FRC_ALL_HCLK2

#define LL_CGC_FRC_ALL_HCLK2 ((uint32_t)0x7A7FC3CFUL)

All clock group 2

Definition at line 161 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_DSPI_PCLK

#define LL_CGC_FRC_DSPI_PCLK MCU_SUB_FORCE_DSPI_PCLK

Hclk for dspi

Definition at line 152 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_I2C0_PCLK

#define LL_CGC_FRC_I2C0_PCLK MCU_SUB_FORCE_I2C0_PCLK

Hclk for i2c0

Definition at line 141 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_I2C1_PCLK

#define LL_CGC_FRC_I2C1_PCLK MCU_SUB_FORCE_I2C1_PCLK

Hclk for i2c1

Definition at line 142 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_I2C2_PCLK

#define LL_CGC_FRC_I2C2_PCLK MCU_SUB_FORCE_I2C2_PCLK

Hclk for i2c2

Definition at line 143 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_I2C3_PCLK

#define LL_CGC_FRC_I2C3_PCLK MCU_SUB_FORCE_I2C3_PCLK

Hclk for i2c3

Definition at line 144 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_I2S_PCLK

#define LL_CGC_FRC_I2S_PCLK MCU_SUB_FORCE_I2S_PCLK

Hclk for i2s

Definition at line 150 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_I2S_S_PCLK

#define LL_CGC_FRC_I2S_S_PCLK MCU_SUB_FORCE_I2S_S_PCLK

Hclk for i2ss

Definition at line 151 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_PDM_PCLK

#define LL_CGC_FRC_PDM_PCLK MCU_SUB_FORCE_PDM_PCLK

Hclk for pdm

Definition at line 153 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_PWM_0_PCLK

#define LL_CGC_FRC_PWM_0_PCLK MCU_SUB_FORCE_PWM_0_PCLK

Pclk for PWM0

Definition at line 154 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_PWM_1_PCLK

#define LL_CGC_FRC_PWM_1_PCLK MCU_SUB_FORCE_PWM_1_PCLK

Pclk for PWM1

Definition at line 155 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_QSPI0_PCLK

#define LL_CGC_FRC_QSPI0_PCLK MCU_SUB_FORCE_QSPI0_PCLK

Hclk for qspi0

Definition at line 145 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_QSPI1_PCLK

#define LL_CGC_FRC_QSPI1_PCLK MCU_SUB_FORCE_QSPI1_PCLK

Hclk for qspi1

Definition at line 146 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_QSPI2_PCLK

#define LL_CGC_FRC_QSPI2_PCLK MCU_SUB_FORCE_QSPI2_PCLK

Hclk for qspi2

Definition at line 147 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_SECU_DIV4_PCLK

#define LL_CGC_FRC_SECU_DIV4_PCLK MCU_SUB_FORCE_SECU_DIV4_PCLK

Div4 clk for security blocksi

Definition at line 157 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_SERIALS_HCLK2

#define LL_CGC_FRC_SERIALS_HCLK2 ((uint32_t)0x705E03CFUL)

Hclk for serial blocks

Definition at line 160 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_SPI_M_PCLK

#define LL_CGC_FRC_SPI_M_PCLK MCU_SUB_FORCE_SPI_M_PCLK

Hclk for spim

Definition at line 148 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_SPI_S_PCLK

#define LL_CGC_FRC_SPI_S_PCLK MCU_SUB_FORCE_SPI_S_PCLK

Hclk for spis

Definition at line 149 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_UART0_PCLK

#define LL_CGC_FRC_UART0_PCLK MCU_SUB_FORCE_UART0_PCLK

Pclk for uart0

Definition at line 137 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_UART1_PCLK

#define LL_CGC_FRC_UART1_PCLK MCU_SUB_FORCE_UART1_PCLK

Pclk for uart1

Definition at line 138 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_UART2_PCLK

#define LL_CGC_FRC_UART2_PCLK MCU_SUB_FORCE_UART2_PCLK

Pclk for uart2

Definition at line 139 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_UART3_PCLK

#define LL_CGC_FRC_UART3_PCLK MCU_SUB_FORCE_UART3_PCLK

Pclk for uart3

Definition at line 140 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_VTTBL_PCLK

#define LL_CGC_FRC_VTTBL_PCLK MCU_SUB_FORCE_VTTBL_PCLK

Pclk for VTTBL

Definition at line 156 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_FRC_XQSPI_DIV4_PCLK

#define LL_CGC_FRC_XQSPI_DIV4_PCLK MCU_SUB_FORCE_XQSPI_DIV4_PCLK

Div4 clk for xf qspi

Definition at line 158 of file gr55xx_ll_cgc.h.