Macros
Clock source select
Peripheral Driver » LL Driver » CLK » Defines » CLK Exported Constants

## Macros
#define | LL_CLK_SEL_SOURCE_CPLL_CLK (0UL)
#define | LL_CLK_SEL_SOURCE_HF_OSC_CLK (1UL)
#define | LL_CLK_SEL_FAST_WAKEUP_CPLL_CLK (0UL)
#define | LL_CLK_SEL_FAST_WAKEUP_HF_OSC_CLK (AON_CTL_AON_CLK_WAKUP_FAST_CLK_SEL_Msk)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CLK_SEL_FAST_WAKEUP_CPLL_CLK

#define LL_CLK_SEL_FAST_WAKEUP_CPLL_CLK (0UL)

Select CPLL clk as fast wakeup clk

Definition at line 78 of file gr55xx_ll_clk.h.

## ◆ LL_CLK_SEL_FAST_WAKEUP_HF_OSC_CLK

#define LL_CLK_SEL_FAST_WAKEUP_HF_OSC_CLK (AON_CTL_AON_CLK_WAKUP_FAST_CLK_SEL_Msk)

Select hf osc clk as fast wakeup clk

Definition at line 79 of file gr55xx_ll_clk.h.

## ◆ LL_CLK_SEL_SOURCE_CPLL_CLK

#define LL_CLK_SEL_SOURCE_CPLL_CLK (0UL)

Select CPLL clk as the source of the 192MHz clock

Definition at line 76 of file gr55xx_ll_clk.h.

## ◆ LL_CLK_SEL_SOURCE_HF_OSC_CLK

#define LL_CLK_SEL_SOURCE_HF_OSC_CLK (1UL)

Select hf osc clk as the source of the 192MHz clock

Definition at line 77 of file gr55xx_ll_clk.h.