app_adc_dma.h
Go to the documentation of this file.
1 /**
2 ****************************************************************************************
3 *
4 * @file app_adc_dma.h
5 * @author BLE Driver Team
6 * @brief Header file containing functions prototypes of ADC app library.
7 *
8 ****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 ****************************************************************************************
36 */
37
38 /** @addtogroup PERIPHERAL Peripheral Driver
39 * @{
40 */
41
42 /** @addtogroup APP_DRIVER APP DRIVER
43 * @{
44 */
45
46 /** @defgroup APP_ADC ADC
47 * @brief ADC APP module driver.
48 * @{
49 */
50
51
52 #ifndef _APP_ADC_DMA_H_
53 #define _APP_ADC_DMA_H_
54
55 #include "grx_hal.h"
56 #include "app_io.h"
57 #include "app_drv_error.h"
58 #include "app_drv_config.h"
59 #include "app_adc.h"
60
61 #ifdef __cplusplus
62 extern "C" {
63 #endif
64
65 #ifdef HAL_ADC_MODULE_ENABLED
66
67 /** @addtogroup APP_ADC_DRIVER_MACRO Defines
68 * @{
69 */
70 /**
71 * @brief DMA for conversion.
72 */
73 #define app_adc_dma_conversion_async app_adc_conversion_async
74 /**
75 * @brief DMA for multi channel conversion.
76 */
77 #define app_adc_dma_multi_channel_conversion_async app_adc_multi_channel_conversion_async
78 /** @} */
79
80 /* Exported functions --------------------------------------------------------*/
81 /** @addtogroup APP_ADC_DRIVER_FUNCTIONS Functions
82 * @{
83 */
84
85 /**
86 ****************************************************************************************
87 * @brief Initialize the APP ADC DRIVER according to the specified parameters
88 * in the app_adc_params_t and app_adc_evt_handler_t.
89 * @note If DMA mode is set, you can use blocking mode. Conversely, if blocking mode
90 * is set, you can't use DMA mode.
91 *
92 * @param[in] p_params: Pointer to app_adc_params_t parameter which contains the
93 * configuration information for the specified ADC module.
94 *
95 * @return Result of initialization.
96 ****************************************************************************************
97 */
98 uint16_t app_adc_dma_init(app_adc_params_t *p_params);
99
100 /**
101 ****************************************************************************************
102 * @brief De-initialize the APP ADC DRIVER peripheral.
103 *
104 * @return Result of De-initialization.
105 ****************************************************************************************
106 */
107 uint16_t app_adc_dma_deinit(void);
108
109 /** @} */
110
111 #endif
112
113 #ifdef __cplusplus
114 }
115 #endif
116
117 #endif
118 /** @} */
119 /** @} */
120 /** @} */
app_adc_params_t
ADC parameters structure definition.
Definition: app_adc.h:186
app_io.h
Header file containing functions prototypes of GPIO app library.
app_adc_dma_deinit
uint16_t app_adc_dma_deinit(void)
De-initialize the APP ADC DRIVER peripheral.
grx_hal.h
This file contains all the functions prototypes for the HAL module driver.
app_adc.h
Header file containing functions prototypes of ADC app library.
app_adc_dma_init
uint16_t app_adc_dma_init(app_adc_params_t *p_params)
Initialize the APP ADC DRIVER according to the specified parameters in the app_adc_params_t and app_a...
app_drv_error.h
Header file of app driver error code.
app_drv_config.h
Header file of app driver config code.