Public Attributes | List of all members
ble_gap_evt_local_tx_pwr_read_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Local transmit power read indication info event for BLE_GAPC_EVT_LOCAL_TX_POWER_READ. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | phy
int8_t | curr_tx_pwr_lvl
int8_t | max_tx_pwr_lvl

## Detailed Description

Local transmit power read indication info event for BLE_GAPC_EVT_LOCAL_TX_POWER_READ.

Definition at line 952 of file ble_gapc.h.

## Member Data Documentation

## ◆ curr_tx_pwr_lvl

int8_t ble_gap_evt_local_tx_pwr_read_ind_t::curr_tx_pwr_lvl

Current transmit power level (dBm).

Definition at line 955 of file ble_gapc.h.

## ◆ max_tx_pwr_lvl

int8_t ble_gap_evt_local_tx_pwr_read_ind_t::max_tx_pwr_lvl

Max transmit power level (dBm).

Definition at line 956 of file ble_gapc.h.

## ◆ phy

uint8_t ble_gap_evt_local_tx_pwr_read_ind_t::phy

Phy see ble_gap_phy_type_t.

Definition at line 954 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h