Macros
PDM Exported Macros
Peripheral Driver » HAL Driver » PDM » Defines

PDM_default_config initStruct default configuartion. More...

## Macros
#define | __HAL_PDM_RESET_HANDLE_STATE(__HANDLE__) ((__HANDLE__)->state = HAL_PDM_STATE_RESET)
| Reset PDM handle states. More...
#define | __HAL_PDM_ENABLE_CLOCK(__HANDLE__) ll_pdm_enable_clk((__HANDLE__)->p_instance)
| Enable the specified PDM clock. More...
#define | __HAL_PDM_DISABLE_CLOCK(__HANDLE__) ll_pdm_disable_clk((__HANDLE__)->p_instance)
| Disable the specified ADC clock. More...

## Detailed Description

PDM_default_config initStruct default configuartion.

## Macro Definition Documentation

## ◆ __HAL_PDM_DISABLE_CLOCK

#define __HAL_PDM_DISABLE_CLOCK | ( |  | __HANDLE__ | ) | ll_pdm_disable_clk((__HANDLE__)->p_instance)

Disable the specified ADC clock.

Parameters

  __HANDLE__ | Specify the ADC Handle.

Return values

  None |

Definition at line 200 of file gr55xx_hal_pdm.h.

## ◆ __HAL_PDM_ENABLE_CLOCK

#define __HAL_PDM_ENABLE_CLOCK | ( |  | __HANDLE__ | ) | ll_pdm_enable_clk((__HANDLE__)->p_instance)

Enable the specified PDM clock.

Parameters

  __HANDLE__ | Specify the PDM Handle.

Return values

  None |

Definition at line 194 of file gr55xx_hal_pdm.h.

## ◆ __HAL_PDM_RESET_HANDLE_STATE

#define __HAL_PDM_RESET_HANDLE_STATE | ( |  | __HANDLE__ | ) | ((__HANDLE__)->state = HAL_PDM_STATE_RESET)

Reset PDM handle states.

Parameters

  __HANDLE__ | PDM handle.

Return values

  None |

Definition at line 188 of file gr55xx_hal_pdm.h.