ble_event.h
Go to the documentation of this file.
1 /**
2 ****************************************************************************************
3 *
4 * @file ble_event.h
5 *
6 * @brief BLE event header files
7 *
8 ****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE
40 * @{
41 */
42
43 /**
44 @addtogroup BLE_EVENT BLE Event
45 @{
46 @brief BLE Event interface.
47 */
48 #ifndef __BLE_EVENT_H__
49 #define __BLE_EVENT_H__
50
51 #include "ble_gapm.h"
52 #include "ble_gapc.h"
53 #include "ble_gatts.h"
54 #include "ble_gattc.h"
55 #include "ble_sec.h"
56 #include "ble_l2cap.h"
57
58 /** @addtogroup BLE_EVENT_DEFINES Defines
59 * @{
60 */
61 /** @defgroup BLE_EVENT_BASE BLE Event Base
62 * @{ */
63 #define BLE_COMMON_EVT_BASE 0x0100 /**< BLE Common Event base. */
64 #define BLE_GAPM_EVT_BASE 0x0200 /**< BLE GAP Management Event base. */
65 #define BLE_GAPC_EVT_BASE 0x0300 /**< BLE GAP Connection Control Event base. */
66 #define BLE_GATTS_EVT_BASE 0x0400 /**< BLE GATTS Event base. */
67 #define BLE_GATTC_EVT_BASE 0x0500 /**< BLE GATTC Event base. */
68 #define BLE_GATT_COMMON_EVT_BASE 0x0600 /**< BLE GATT Event base. */
69 #define BLE_SEC_EVT_BASE 0x0700 /**< BLE Security Event base. */
70 #define BLE_L2CAP_EVT_BASE 0x0800 /**< BLE L2CAP Event base. */
71 /** @} */
72 /** @} */
73 #define BLE_SEC_ERR_OFFSET 0x60
74
75 /**
76 * @defgroup BLE_EVENT_ENUM Enumerations
77 * @{
78 */
79 /**
80 * @brief BLE Common Events.
81 */
82 enum BLE_COMMON_EVTS
83 {
84 BLE_COMMON_EVT_STACK_INIT = BLE_COMMON_EVT_BASE, /**< BLE Stack init complete event. */
85 BLE_COMMON_EVT_MAX,
86 };
87
88 /**@brief BLE GAP Managerment Events. */
89 enum BLE_GAPM_EVTS
90 {
91 BLE_GAPM_EVT_CH_MAP_SET = BLE_GAPM_EVT_BASE, /**< Channel Map Set complete event. */
92 BLE_GAPM_EVT_WHITELIST_SET, /**< Whitelist Set complete event. */
93 BLE_GAPM_EVT_PER_ADV_LIST_SET, /**< Periodic Advertising List Set complete event. */
94 BLE_GAPM_EVT_PRIVACY_MODE_SET, /**< Privacy Mode for Peer Device Set complete event. */
95 BLE_GAPM_EVT_LEPSM_REGISTER, /**< LEPSM Register complete event. */
96 BLE_GAPM_EVT_LEPSM_UNREGISTER, /**< LEPSM Unregister complete event. */
97 BLE_GAPM_EVT_DEV_INFO_GOT, /**< Device Info Get event. */
98 BLE_GAPM_EVT_ADV_START, /**< Advertising Start complete event. */
99 BLE_GAPM_EVT_ADV_STOP, /**< Advertising Stop complete event. */
100 BLE_GAPM_EVT_SCAN_REQUEST, /**< Scan Request event. */
101 BLE_GAPM_EVT_ADV_DATA_UPDATE, /**< Advertising Data update event. */
102 BLE_GAPM_EVT_SCAN_START, /**< Scan Start complete event. */
103 BLE_GAPM_EVT_SCAN_STOP, /**< Scan Stop complete event. */
104 BLE_GAPM_EVT_ADV_REPORT, /**< Advertising Report event. */
105 BLE_GAPM_EVT_SYNC_ESTABLISH, /**< Periodic Advertising Synchronization Establish event. */
106 BLE_GAPM_EVT_SYNC_STOP, /**< Periodic Advertising Synchronization Stop event. */
107 BLE_GAPM_EVT_SYNC_LOST, /**< Periodic Advertising Synchronization Lost event. */
108 BLE_GAPM_EVT_READ_RSLV_ADDR, /**< Read Resolvable Address event. */
109 BLE_GAPM_EVT_RSLV_ADDR_REPORT, /**< Resolvable Address report event. */
110 BLE_GAPM_EVT_MAX,
111 };
112
113 /**@brief BLE GAP Connection Control Events. */
114 enum BLE_GAPC_EVTS
115 {
116 BLE_GAPC_EVT_PHY_UPDATED = BLE_GAPC_EVT_BASE, /**< PHY Update event. */
117 BLE_GAPC_EVT_CONNECTED, /**< Connected event. */
118 BLE_GAPC_EVT_DISCONNECTED, /**< Disconnected event. */
119 BLE_GAPC_EVT_CONNECT_CANCLE, /**< Connect Cancle event. */
120 BLE_GAPC_EVT_AUTO_CONN_TIMEOUT, /**< Auto Connect Timeout event. */
121 BLE_GAPC_EVT_CONN_PARAM_UPDATED, /**< Connect Parameter Updated event. */
122 BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ, /**< Connect Parameter Request event. */
123 BLE_GAPC_EVT_PEER_NAME_GOT, /**< peer Name Get event. */
124 BLE_GAPC_EVT_CONN_INFO_GOT, /**< Connect Info Get event. */
125 BLE_GAPC_EVT_PEER_INFO_GOT, /**< Peer Info Get event. */
126 BLE_GAPC_EVT_DATA_LENGTH_UPDATED, /**< Data Length Updated event. */
127 BLE_GAPC_EVT_DEV_INFO_SET, /**< Device Info Set event. */
128 BLE_GAPC_EVT_CONNECT_IQ_REPORT, /**< Connection IQ Report info event. */
129 BLE_GAPC_EVT_CONNECTLESS_IQ_REPORT, /**< Connectionless IQ Report info event. */
130 BLE_GAPC_EVT_LOCAL_TX_POWER_READ, /**< Local transmit power read indication info event. */
131 BLE_GAPC_EVT_REMOTE_TX_POWER_READ, /**< Remote transmit power read indication info event. */
132 BLE_GAPC_EVT_TX_POWER_CHANGE_REPORT, /**< Transmit power change reporting info event. */
133 BLE_GAPC_EVT_PATH_LOSS_THRESHOLD_REPORT, /**< Path loss threshold reporting info event. */
134 BLE_GAPC_EVT_RANGING_IND, /**< Ranging indication event. */
135 BLE_GAPC_EVT_RANGING_SAMPLE_REPORT, /**< Ranging sample report event. */
136 BLE_GAPC_EVT_RANGING_CMP_IND, /**< Ranging complete indication event. */
137 BLE_GAPC_EVT_DFT_SUBRATE_SET, /**< Default subrate param set complete event. */
138 BLE_GAPC_EVT_SUBRATE_CHANGE_IND, /**< Subrate change indication event. */
139
140 BLE_GAPC_EVT_MAX,
141 };
142
143 /**@brief BLE GATT Common Events. */
144 enum
145 {
146 BLE_GATT_COMMON_EVT_MTU_EXCHANGE = BLE_GATT_COMMON_EVT_BASE, /**< MTU Exchange event. */
147 BLE_GATT_COMMON_EVT_PRF_REGISTER, /**< Service Register event. */
148 BLE_GATT_COMMON_EVT_MAX,
149 };
150
151 /**@brief BLE GATTS Events. */
152 enum BLE_GATTS_EVTS
153 {
154 BLE_GATTS_EVT_READ_REQUEST = BLE_GATTS_EVT_BASE, /**< GATTS Read Request event .*/
155 BLE_GATTS_EVT_WRITE_REQUEST, /**< GATTS Write Request event .*/
156 BLE_GATTS_EVT_PREP_WRITE_REQUEST, /**< GATTS Prepare Write Request event .*/
157 BLE_GATTS_EVT_NTF_IND, /**< GATTS Notify or Indicate Complete event .*/
158 BLE_GATTS_EVT_CCCD_RECOVERY, /**< GATTS CCCD Recovery event .*/
159 BLE_GATTS_EVT_MULT_NTF, /**< GATTS Multiple Notify event .*/
160 BLE_GATTS_EVT_ENH_READ_REQUEST, /**< GATTS Enhance Read Request event .*/
161 BLE_GATTS_EVT_ENH_WRITE_REQUEST, /**< GATTS Enhance Write Request event .*/
162 BLE_GATTS_EVT_ENH_PREP_WRITE_REQUEST, /**< GATTS Enhance Prepare Write Request event .*/
163 BLE_GATTS_EVT_ENH_NTF_IND, /**< GATTS Enhance Notify or Indicate Complete event .*/
164 BLE_GATTS_EVT_ENH_CCCD_RECOVERY, /**< GATTS Enhance CCCD Recovery event .*/
165 BLE_GATTS_EVT_ENH_MULT_NTF, /**< GATTS Enhance Multiple Notifications event .*/
166 BLE_GATTS_EVT_DATABASE_INITED_IND,
167 BLE_GATTS_EVT_MAX,
168 };
169
170 enum BLE_GATTC_EVTS
171 {
172 BLE_GATTC_EVT_SRVC_BROWSE = BLE_GATTC_EVT_BASE, /**< GATTC Service Browse event .*/
173 BLE_GATTC_EVT_PRIMARY_SRVC_DISC, /**< GATTC Primary Service Discovery event .*/
174 BLE_GATTC_EVT_INCLUDE_SRVC_DISC, /**< GATTC Include Service Discovery event .*/
175 BLE_GATTC_EVT_CHAR_DISC, /**< GATTC Characteristic Discovery event .*/
176 BLE_GATTC_EVT_CHAR_DESC_DISC, /**< GATTC Characteristic Descriptor Discovery event .*/
177 BLE_GATTC_EVT_READ_RSP, /**< GATTC Read Response event. */
178 BLE_GATTC_EVT_WRITE_RSP, /**< GATTC Write Response event. */
179 BLE_GATTC_EVT_NTF_IND, /**< GATTC Notify or Indicate Receive event. */
180 BLE_GATTC_EVT_CACHE_UPDATE, /**< GATTC Cache Update event. */
181 BLE_GATTC_EVT_PRF_REGISTER, /**< GATTC Profile Register event. */
182 BLE_GATTC_EVT_ENH_SRVC_BROWSE, /**< GATTC Service Browse event .*/
183 BLE_GATTC_EVT_ENH_PRIMARY_SRVC_DISC, /**< GATTC Primary Service Discovery event .*/
184 BLE_GATTC_EVT_ENH_INCLUDE_SRVC_DISC, /**< GATTC Include Service Discovery event .*/
185 BLE_GATTC_EVT_ENH_CHAR_DISC, /**< GATTC Characteristic Discovery event .*/
186 BLE_GATTC_EVT_ENH_CHAR_DESC_DISC, /**< GATTC Characteristic Descriptor Discovery event .*/
187 BLE_GATTC_EVT_ENH_READ_RSP, /**< GATTC Read Response event. */
188 BLE_GATTC_EVT_ENH_WRITE_RSP, /**< GATTC Write Response event. */
189 BLE_GATTC_EVT_ENH_NTF_IND, /**< GATTC Notify or Indicate Receive event. */
190 BLE_GATTC_EVT_MAX,
191 };
192
193 enum BLE_SEC_EVTS
194 {
195 BLE_SEC_EVT_LINK_ENC_REQUEST = BLE_SEC_EVT_BASE, /**< Link Encrypte Request event. */
196 BLE_SEC_EVT_LINK_ENCRYPTED, /**< Link Encrypted event. */
197 BLE_SEC_EVT_LTK_REQ, /**< LTK Request event. */
198 BLE_SEC_EVT_KEY_PRESS_NTF, /**< Key Press event. */
199 BLE_SEC_EVT_KEY_MISSING, /**< Key Missing event. */
200 BLE_SEC_EVT_MAX,
201 };
202
203 enum BLE_L2CAP_EVTS
204 {
205 BLE_L2CAP_EVT_CONN_REQ = BLE_L2CAP_EVT_BASE, /**< L2cap Connect Request event. */
206 BLE_L2CAP_EVT_CONN_IND, /**< L2cap Connected Indicate event. */
207 BLE_L2CAP_EVT_ADD_CREDITS_IND, /**< L2cap Credits Add Indicate event. */
208 BLE_L2CAP_EVT_DISCONNECTED, /**< L2cap Disconnected event. */
209 BLE_L2CAP_EVT_SDU_RECV, /**< L2cap SDU Receive event. */
210 BLE_L2CAP_EVT_SDU_SEND, /**< L2cap SDU Send event. */
211 BLE_L2CAP_EVT_ADD_CREDITS_CPLT, /**< L2cap Credits Add Completed event. */
212 BLE_L2CAP_EVT_MAX,
213 };
214 /** @} */
215
216 /** @addtogroup BLE_COMMEN_STRUCTURES Structures
217 * @{
218 */
219 /**@brief BLE Event Information. */
220 typedef struct
221 {
222 uint16_t evt_id; /**< Event ID. */
223 uint16_t evt_status; /**< Event Status. */
224 union
225 {
226 ble_gapm_evt_t gapm_evt; /**< BLE GAP Management Event. */
227 ble_gapc_evt_t gapc_evt; /**< BLE GAP Connection Control Event. */
228 ble_gatts_evt_t gatts_evt; /**< BLE GATT Server Event. */
229 ble_gattc_evt_t gattc_evt; /**< BLE GATT Client Event. */
230 ble_gatt_common_evt_t gatt_common_evt; /**< BLE GATT Common Event. */
231 ble_sec_evt_t sec_evt; /**< BLE Security Event. */
232 ble_l2cap_evt_t l2cap_evt; /**< BLE L2CAP Event. */
233 } evt; /**< BLE Event parameter. */
234 } ble_evt_t;
235 /** @} */
236
237 /** @addtogroup BLE_EVENT_TYPEDEF Typedefs
238 * @{
239 */
240 /**@brief The BLE event handler type. */
241
242 typedef void (*ble_evt_handler_t)(const ble_evt_t *p_evt);
243 extern ble_evt_handler_t s_ble_evt_handler;
244
245 #define BLE_EVT_INIT(ble_evt, evt, status) \
246 ble_evt_t ble_evt; \
247 do \
248 { \
249 memset(&ble_evt, 0xff, sizeof(ble_evt_t)); \
250 ble_evt.evt_id = evt; \
251 ble_evt.evt_status = status; \
252 } while(0);
253
254 /** @} */
255 bool ble_event_handle(const ble_evt_t *p_evt);
256
257 #endif
258 /** @} */
259 /** @} */
260
261
262
263
BLE_GAPM_EVT_PRIVACY_MODE_SET
@ BLE_GAPM_EVT_PRIVACY_MODE_SET
Definition: ble_event.h:94
BLE_GAPC_EVT_PATH_LOSS_THRESHOLD_REPORT
@ BLE_GAPC_EVT_PATH_LOSS_THRESHOLD_REPORT
Definition: ble_event.h:133
BLE_GAPM_EVTS
BLE_GAPM_EVTS
BLE GAP Managerment Events.
Definition: ble_event.h:90
BLE_GATT_COMMON_EVT_MAX
@ BLE_GATT_COMMON_EVT_MAX
Definition: ble_event.h:148
BLE_GAPM_EVT_SCAN_REQUEST
@ BLE_GAPM_EVT_SCAN_REQUEST
Definition: ble_event.h:100
ble_event_handle
bool ble_event_handle(const ble_evt_t *p_evt)
BLE_GATTC_EVT_READ_RSP
@ BLE_GATTC_EVT_READ_RSP
Definition: ble_event.h:177
BLE_GAPM_EVT_ADV_START
@ BLE_GAPM_EVT_ADV_START
Definition: ble_event.h:98
BLE_GAPM_EVT_BASE
#define BLE_GAPM_EVT_BASE
Definition: ble_event.h:64
BLE_GATTC_EVT_MAX
@ BLE_GATTC_EVT_MAX
Definition: ble_event.h:190
BLE_GAPM_EVT_ADV_STOP
@ BLE_GAPM_EVT_ADV_STOP
Definition: ble_event.h:99
BLE_GATTC_EVT_ENH_NTF_IND
@ BLE_GATTC_EVT_ENH_NTF_IND
Definition: ble_event.h:189
BLE_GATTC_EVT_ENH_CHAR_DESC_DISC
@ BLE_GATTC_EVT_ENH_CHAR_DESC_DISC
Definition: ble_event.h:186
BLE_GATTS_EVT_PREP_WRITE_REQUEST
@ BLE_GATTS_EVT_PREP_WRITE_REQUEST
Definition: ble_event.h:156
BLE_SEC_EVT_MAX
@ BLE_SEC_EVT_MAX
Definition: ble_event.h:200
BLE_GAPC_EVT_CONN_INFO_GOT
@ BLE_GAPC_EVT_CONN_INFO_GOT
Definition: ble_event.h:124
BLE_GATTC_EVT_WRITE_RSP
@ BLE_GATTC_EVT_WRITE_RSP
Definition: ble_event.h:178
BLE_SEC_EVT_BASE
#define BLE_SEC_EVT_BASE
Definition: ble_event.h:69
BLE_GAPM_EVT_ADV_REPORT
@ BLE_GAPM_EVT_ADV_REPORT
Definition: ble_event.h:104
BLE_GAPM_EVT_RSLV_ADDR_REPORT
@ BLE_GAPM_EVT_RSLV_ADDR_REPORT
Definition: ble_event.h:109
BLE_GATTC_EVT_NTF_IND
@ BLE_GATTC_EVT_NTF_IND
Definition: ble_event.h:179
ble_evt_t::l2cap_evt
ble_l2cap_evt_t l2cap_evt
Definition: ble_event.h:232
BLE_GAPC_EVT_DISCONNECTED
@ BLE_GAPC_EVT_DISCONNECTED
Definition: ble_event.h:118
BLE_L2CAP_EVT_CONN_REQ
@ BLE_L2CAP_EVT_CONN_REQ
Definition: ble_event.h:205
BLE_GATTS_EVT_ENH_CCCD_RECOVERY
@ BLE_GATTS_EVT_ENH_CCCD_RECOVERY
Definition: ble_event.h:164
ble_evt_t::evt_status
uint16_t evt_status
Definition: ble_event.h:223
BLE_L2CAP_EVT_BASE
#define BLE_L2CAP_EVT_BASE
Definition: ble_event.h:70
BLE_GAPC_EVT_RANGING_SAMPLE_REPORT
@ BLE_GAPC_EVT_RANGING_SAMPLE_REPORT
Definition: ble_event.h:135
ble_evt_t::gatts_evt
ble_gatts_evt_t gatts_evt
Definition: ble_event.h:228
ble_gatts.h
BLE GATTS API.
ble_l2cap_evt_t
BLE L2CAP event structure.
Definition: ble_l2cap.h:232
BLE_GATTS_EVT_ENH_PREP_WRITE_REQUEST
@ BLE_GATTS_EVT_ENH_PREP_WRITE_REQUEST
Definition: ble_event.h:162
BLE_GATT_COMMON_EVT_PRF_REGISTER
@ BLE_GATT_COMMON_EVT_PRF_REGISTER
Definition: ble_event.h:147
BLE_GAPM_EVT_MAX
@ BLE_GAPM_EVT_MAX
Definition: ble_event.h:110
BLE_GATTS_EVT_WRITE_REQUEST
@ BLE_GATTS_EVT_WRITE_REQUEST
Definition: ble_event.h:155
ble_evt_t::sec_evt
ble_sec_evt_t sec_evt
Definition: ble_event.h:231
BLE_GAPC_EVT_SUBRATE_CHANGE_IND
@ BLE_GAPC_EVT_SUBRATE_CHANGE_IND
Definition: ble_event.h:138
BLE_GAPC_EVT_DEV_INFO_SET
@ BLE_GAPC_EVT_DEV_INFO_SET
Definition: ble_event.h:127
BLE_GAPC_EVT_CONN_PARAM_UPDATED
@ BLE_GAPC_EVT_CONN_PARAM_UPDATED
Definition: ble_event.h:121
BLE_GATT_COMMON_EVT_MTU_EXCHANGE
@ BLE_GATT_COMMON_EVT_MTU_EXCHANGE
Definition: ble_event.h:146
BLE_SEC_EVT_LINK_ENCRYPTED
@ BLE_SEC_EVT_LINK_ENCRYPTED
Definition: ble_event.h:196
BLE_GATTS_EVT_NTF_IND
@ BLE_GATTS_EVT_NTF_IND
Definition: ble_event.h:157
BLE_GAPC_EVT_CONNECTED
@ BLE_GAPC_EVT_CONNECTED
Definition: ble_event.h:117
BLE_GATTC_EVT_PRF_REGISTER
@ BLE_GATTC_EVT_PRF_REGISTER
Definition: ble_event.h:181
BLE_L2CAP_EVT_ADD_CREDITS_CPLT
@ BLE_L2CAP_EVT_ADD_CREDITS_CPLT
Definition: ble_event.h:211
ble_l2cap.h
BLE L2CAP API.
BLE_L2CAP_EVTS
BLE_L2CAP_EVTS
Definition: ble_event.h:204
BLE_GAPM_EVT_SYNC_STOP
@ BLE_GAPM_EVT_SYNC_STOP
Definition: ble_event.h:106
BLE_GAPM_EVT_PER_ADV_LIST_SET
@ BLE_GAPM_EVT_PER_ADV_LIST_SET
Definition: ble_event.h:93
BLE_GATT_COMMON_EVT_BASE
#define BLE_GATT_COMMON_EVT_BASE
Definition: ble_event.h:68
BLE_GATTC_EVT_CACHE_UPDATE
@ BLE_GATTC_EVT_CACHE_UPDATE
Definition: ble_event.h:180
BLE_GAPC_EVT_DFT_SUBRATE_SET
@ BLE_GAPC_EVT_DFT_SUBRATE_SET
Definition: ble_event.h:137
BLE_GAPC_EVT_BASE
#define BLE_GAPC_EVT_BASE
Definition: ble_event.h:65
BLE_GAPC_EVT_PEER_INFO_GOT
@ BLE_GAPC_EVT_PEER_INFO_GOT
Definition: ble_event.h:125
BLE_GATTS_EVT_MAX
@ BLE_GATTS_EVT_MAX
Definition: ble_event.h:167
ble_gapm_evt_t
BLE GAPM event structure.
Definition: ble_gapm.h:902
ble_sec.h
BLE SEC API.
BLE_GAPC_EVT_REMOTE_TX_POWER_READ
@ BLE_GAPC_EVT_REMOTE_TX_POWER_READ
Definition: ble_event.h:131
BLE_GATTC_EVTS
BLE_GATTC_EVTS
Definition: ble_event.h:171
BLE_GATTS_EVT_ENH_READ_REQUEST
@ BLE_GATTS_EVT_ENH_READ_REQUEST
Definition: ble_event.h:160
BLE_GAPM_EVT_LEPSM_UNREGISTER
@ BLE_GAPM_EVT_LEPSM_UNREGISTER
Definition: ble_event.h:96
BLE_COMMON_EVT_MAX
@ BLE_COMMON_EVT_MAX
Definition: ble_event.h:85
BLE_SEC_EVT_KEY_MISSING
@ BLE_SEC_EVT_KEY_MISSING
Definition: ble_event.h:199
ble_gapc.h
BLE GAPC API.
BLE_GATTC_EVT_ENH_SRVC_BROWSE
@ BLE_GATTC_EVT_ENH_SRVC_BROWSE
Definition: ble_event.h:182
BLE_L2CAP_EVT_SDU_RECV
@ BLE_L2CAP_EVT_SDU_RECV
Definition: ble_event.h:209
BLE_L2CAP_EVT_MAX
@ BLE_L2CAP_EVT_MAX
Definition: ble_event.h:212
BLE_GATTS_EVT_CCCD_RECOVERY
@ BLE_GATTS_EVT_CCCD_RECOVERY
Definition: ble_event.h:158
BLE_GATTC_EVT_ENH_CHAR_DISC
@ BLE_GATTC_EVT_ENH_CHAR_DISC
Definition: ble_event.h:185
BLE_GATTS_EVT_ENH_WRITE_REQUEST
@ BLE_GATTS_EVT_ENH_WRITE_REQUEST
Definition: ble_event.h:161
BLE_COMMON_EVTS
BLE_COMMON_EVTS
BLE Common Events.
Definition: ble_event.h:83
BLE_GAPM_EVT_WHITELIST_SET
@ BLE_GAPM_EVT_WHITELIST_SET
Definition: ble_event.h:92
BLE_GATTS_EVT_BASE
#define BLE_GATTS_EVT_BASE
Definition: ble_event.h:66
BLE_GAPM_EVT_DEV_INFO_GOT
@ BLE_GAPM_EVT_DEV_INFO_GOT
Definition: ble_event.h:97
BLE_COMMON_EVT_STACK_INIT
@ BLE_COMMON_EVT_STACK_INIT
Definition: ble_event.h:84
BLE_GAPM_EVT_SYNC_ESTABLISH
@ BLE_GAPM_EVT_SYNC_ESTABLISH
Definition: ble_event.h:105
BLE_GAPC_EVT_LOCAL_TX_POWER_READ
@ BLE_GAPC_EVT_LOCAL_TX_POWER_READ
Definition: ble_event.h:130
BLE_GAPC_EVTS
BLE_GAPC_EVTS
BLE GAP Connection Control Events.
Definition: ble_event.h:115
BLE_GATTC_EVT_CHAR_DESC_DISC
@ BLE_GATTC_EVT_CHAR_DESC_DISC
Definition: ble_event.h:176
BLE_GATTC_EVT_PRIMARY_SRVC_DISC
@ BLE_GATTC_EVT_PRIMARY_SRVC_DISC
Definition: ble_event.h:173
BLE_GATTS_EVT_DATABASE_INITED_IND
@ BLE_GATTS_EVT_DATABASE_INITED_IND
Definition: ble_event.h:166
BLE_L2CAP_EVT_ADD_CREDITS_IND
@ BLE_L2CAP_EVT_ADD_CREDITS_IND
Definition: ble_event.h:207
BLE_SEC_EVTS
BLE_SEC_EVTS
Definition: ble_event.h:194
BLE_COMMON_EVT_BASE
#define BLE_COMMON_EVT_BASE
Definition: ble_event.h:63
BLE_GAPC_EVT_CONNECT_IQ_REPORT
@ BLE_GAPC_EVT_CONNECT_IQ_REPORT
Definition: ble_event.h:128
ble_evt_t::gapc_evt
ble_gapc_evt_t gapc_evt
Definition: ble_event.h:227
BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ
@ BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ
Definition: ble_event.h:122
BLE_GAPM_EVT_ADV_DATA_UPDATE
@ BLE_GAPM_EVT_ADV_DATA_UPDATE
Definition: ble_event.h:101
BLE_L2CAP_EVT_SDU_SEND
@ BLE_L2CAP_EVT_SDU_SEND
Definition: ble_event.h:210
s_ble_evt_handler
ble_evt_handler_t s_ble_evt_handler
BLE_GATTS_EVTS
BLE_GATTS_EVTS
BLE GATTS Events.
Definition: ble_event.h:153
BLE_GAPM_EVT_SCAN_START
@ BLE_GAPM_EVT_SCAN_START
Definition: ble_event.h:102
ble_gapc_evt_t
BLE GAPC event structure.
Definition: ble_gapc.h:1014
BLE_GATTC_EVT_BASE
#define BLE_GATTC_EVT_BASE
Definition: ble_event.h:67
BLE_GATTS_EVT_ENH_MULT_NTF
@ BLE_GATTS_EVT_ENH_MULT_NTF
Definition: ble_event.h:165
BLE_GATTC_EVT_CHAR_DISC
@ BLE_GATTC_EVT_CHAR_DISC
Definition: ble_event.h:175
BLE_GATTC_EVT_ENH_INCLUDE_SRVC_DISC
@ BLE_GATTC_EVT_ENH_INCLUDE_SRVC_DISC
Definition: ble_event.h:184
ble_gatts_evt_t
BLE GATTS event structure.
Definition: ble_gatts.h:419
ble_gapm.h
BLE GAPM API.
BLE_GATTS_EVT_ENH_NTF_IND
@ BLE_GATTS_EVT_ENH_NTF_IND
Definition: ble_event.h:163
BLE_GATTS_EVT_MULT_NTF
@ BLE_GATTS_EVT_MULT_NTF
Definition: ble_event.h:159
BLE_SEC_EVT_KEY_PRESS_NTF
@ BLE_SEC_EVT_KEY_PRESS_NTF
Definition: ble_event.h:198
BLE_GATTC_EVT_INCLUDE_SRVC_DISC
@ BLE_GATTC_EVT_INCLUDE_SRVC_DISC
Definition: ble_event.h:174
BLE_SEC_EVT_LTK_REQ
@ BLE_SEC_EVT_LTK_REQ
Definition: ble_event.h:197
BLE_GATTC_EVT_SRVC_BROWSE
@ BLE_GATTC_EVT_SRVC_BROWSE
Definition: ble_event.h:172
ble_gatt_common_evt_t
GATT Common structure.
Definition: ble_gatt.h:104
BLE_L2CAP_EVT_CONN_IND
@ BLE_L2CAP_EVT_CONN_IND
Definition: ble_event.h:206
BLE_GATTC_EVT_ENH_READ_RSP
@ BLE_GATTC_EVT_ENH_READ_RSP
Definition: ble_event.h:187
BLE_SEC_EVT_LINK_ENC_REQUEST
@ BLE_SEC_EVT_LINK_ENC_REQUEST
Definition: ble_event.h:195
BLE_GAPC_EVT_PHY_UPDATED
@ BLE_GAPC_EVT_PHY_UPDATED
Definition: ble_event.h:116
ble_evt_handler_t
void(* ble_evt_handler_t)(const ble_evt_t *p_evt)
The BLE event handler type.
Definition: ble_event.h:242
BLE_GAPC_EVT_CONNECT_CANCLE
@ BLE_GAPC_EVT_CONNECT_CANCLE
Definition: ble_event.h:119
BLE_GAPC_EVT_MAX
@ BLE_GAPC_EVT_MAX
Definition: ble_event.h:140
ble_evt_t
BLE Event Information.
Definition: ble_event.h:221
ble_gattc.h
BLE GATTC API.
BLE_GAPC_EVT_RANGING_IND
@ BLE_GAPC_EVT_RANGING_IND
Definition: ble_event.h:134
BLE_GAPC_EVT_RANGING_CMP_IND
@ BLE_GAPC_EVT_RANGING_CMP_IND
Definition: ble_event.h:136
BLE_GAPC_EVT_AUTO_CONN_TIMEOUT
@ BLE_GAPC_EVT_AUTO_CONN_TIMEOUT
Definition: ble_event.h:120
BLE_GAPM_EVT_SCAN_STOP
@ BLE_GAPM_EVT_SCAN_STOP
Definition: ble_event.h:103
ble_evt_t::gattc_evt
ble_gattc_evt_t gattc_evt
Definition: ble_event.h:229
BLE_GATTS_EVT_READ_REQUEST
@ BLE_GATTS_EVT_READ_REQUEST
Definition: ble_event.h:154
ble_evt_t::gapm_evt
ble_gapm_evt_t gapm_evt
Definition: ble_event.h:226
BLE_GAPM_EVT_READ_RSLV_ADDR
@ BLE_GAPM_EVT_READ_RSLV_ADDR
Definition: ble_event.h:108
BLE_GAPM_EVT_CH_MAP_SET
@ BLE_GAPM_EVT_CH_MAP_SET
Definition: ble_event.h:91
BLE_GAPC_EVT_CONNECTLESS_IQ_REPORT
@ BLE_GAPC_EVT_CONNECTLESS_IQ_REPORT
Definition: ble_event.h:129
BLE_GAPC_EVT_TX_POWER_CHANGE_REPORT
@ BLE_GAPC_EVT_TX_POWER_CHANGE_REPORT
Definition: ble_event.h:132
ble_sec_evt_t
BLE Security event structure.
Definition: ble_sec.h:234
BLE_GATTC_EVT_ENH_WRITE_RSP
@ BLE_GATTC_EVT_ENH_WRITE_RSP
Definition: ble_event.h:188
BLE_GAPC_EVT_PEER_NAME_GOT
@ BLE_GAPC_EVT_PEER_NAME_GOT
Definition: ble_event.h:123
BLE_GATTC_EVT_ENH_PRIMARY_SRVC_DISC
@ BLE_GATTC_EVT_ENH_PRIMARY_SRVC_DISC
Definition: ble_event.h:183
BLE_L2CAP_EVT_DISCONNECTED
@ BLE_L2CAP_EVT_DISCONNECTED
Definition: ble_event.h:208
BLE_GAPC_EVT_DATA_LENGTH_UPDATED
@ BLE_GAPC_EVT_DATA_LENGTH_UPDATED
Definition: ble_event.h:126
BLE_GAPM_EVT_LEPSM_REGISTER
@ BLE_GAPM_EVT_LEPSM_REGISTER
Definition: ble_event.h:95
BLE_GAPM_EVT_SYNC_LOST
@ BLE_GAPM_EVT_SYNC_LOST
Definition: ble_event.h:107
ble_evt_t::gatt_common_evt
ble_gatt_common_evt_t gatt_common_evt
Definition: ble_event.h:230
ble_evt_t::evt_id
uint16_t evt_id
Definition: ble_event.h:222
ble_gattc_evt_t
BLE GATTC event structure.
Definition: ble_gattc.h:401