Macros
Power States Defines
Peripheral Driver » HAL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | HAL_ISO7816_PWR_STATE_OFF LL_ISO7816_PWR_STATE_OFF
#define | HAL_ISO7816_PWR_STATE_PWRUP_VCC LL_ISO7816_PWR_STATE_PWRUP_VCC
#define | HAL_ISO7816_PWR_STATE_PWRUP_RST LL_ISO7816_PWR_STATE_PWRUP_RST
#define | HAL_ISO7816_PWR_STATE_PWRDN_RST LL_ISO7816_PWR_STATE_PWRDN_RST
#define | HAL_ISO7816_PWR_STATE_PWRDN_VCC LL_ISO7816_PWR_STATE_PWRDN_VCC
#define | HAL_ISO7816_PWR_STATE_STOP_PRE LL_ISO7816_PWR_STATE_STOP_PRE
#define | HAL_ISO7816_PWR_STATE_STOP LL_ISO7816_PWR_STATE_STOP
#define | HAL_ISO7816_PWR_STATE_STOP_POST LL_ISO7816_PWR_STATE_STOP_POST
#define | HAL_ISO7816_PWR_STATE_IDLE LL_ISO7816_PWR_STATE_IDLE
#define | HAL_ISO7816_PWR_STATE_RX_TS0 LL_ISO7816_PWR_STATE_RX_TS0
#define | HAL_ISO7816_PWR_STATE_RX_TS1 LL_ISO7816_PWR_STATE_RX_TS1
#define | HAL_ISO7816_PWR_STATE_RX LL_ISO7816_PWR_STATE_RX
#define | HAL_ISO7816_PWR_STATE_TX LL_ISO7816_PWR_STATE_TX
#define | HAL_ISO7816_PWR_STATE_TX_RX LL_ISO7816_PWR_STATE_TX_RX

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_ISO7816_PWR_STATE_IDLE

#define HAL_ISO7816_PWR_STATE_IDLE LL_ISO7816_PWR_STATE_IDLE

Idle

Definition at line 236 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_OFF

#define HAL_ISO7816_PWR_STATE_OFF LL_ISO7816_PWR_STATE_OFF

Off

Definition at line 228 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRDN_RST

#define HAL_ISO7816_PWR_STATE_PWRDN_RST LL_ISO7816_PWR_STATE_PWRDN_RST

Power Down reset

Definition at line 231 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRDN_VCC

#define HAL_ISO7816_PWR_STATE_PWRDN_VCC LL_ISO7816_PWR_STATE_PWRDN_VCC

Power Down VCC

Definition at line 232 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRUP_RST

#define HAL_ISO7816_PWR_STATE_PWRUP_RST LL_ISO7816_PWR_STATE_PWRUP_RST

Power up reset

Definition at line 230 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRUP_VCC

#define HAL_ISO7816_PWR_STATE_PWRUP_VCC LL_ISO7816_PWR_STATE_PWRUP_VCC

Power up VCC

Definition at line 229 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_RX

#define HAL_ISO7816_PWR_STATE_RX LL_ISO7816_PWR_STATE_RX

Receive

Definition at line 239 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_RX_TS0

#define HAL_ISO7816_PWR_STATE_RX_TS0 LL_ISO7816_PWR_STATE_RX_TS0

RX TS Character

Definition at line 237 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_RX_TS1

#define HAL_ISO7816_PWR_STATE_RX_TS1 LL_ISO7816_PWR_STATE_RX_TS1

RX TS Character

Definition at line 238 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_STOP

#define HAL_ISO7816_PWR_STATE_STOP LL_ISO7816_PWR_STATE_STOP

Clock Stopped

Definition at line 234 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_STOP_POST

#define HAL_ISO7816_PWR_STATE_STOP_POST LL_ISO7816_PWR_STATE_STOP_POST

Exiting Clock Stop

Definition at line 235 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_STOP_PRE

#define HAL_ISO7816_PWR_STATE_STOP_PRE LL_ISO7816_PWR_STATE_STOP_PRE

Preparing Clock Stop

Definition at line 233 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_TX

#define HAL_ISO7816_PWR_STATE_TX LL_ISO7816_PWR_STATE_TX

Transmit

Definition at line 240 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_TX_RX

#define HAL_ISO7816_PWR_STATE_TX_RX LL_ISO7816_PWR_STATE_TX_RX

Transmit and Receive

Definition at line 241 of file gr55xx_hal_iso7816.h.