Macros
Sleep Timer Clock Source
Peripheral Driver » HAL Driver » PWR | Peripheral Driver » HAL Driver » SLP_TIM » Defines » PWR Exported Constants

## Macros
#define | SLEEP_TIMER_CLK_SEL_RNG_OSC LL_SLEEP_TIMER_CLK_SEL_RNG_OSC
#define | SLEEP_TIMER_CLK_SEL_XO LL_SLEEP_TIMER_CLK_SEL_XO
#define | SLEEP_TIMER_CLK_SEL_RNG2_OSC LL_SLEEP_TIMER_CLK_SEL_RNG2_OSC
#define | SLEEP_TIMER_CLK_SEL_RTC_OSC LL_SLEEP_TIMER_CLK_SEL_RTC_OSC

## Detailed Description

## Macro Definition Documentation

## ◆ SLEEP_TIMER_CLK_SEL_RNG2_OSC

#define SLEEP_TIMER_CLK_SEL_RNG2_OSC LL_SLEEP_TIMER_CLK_SEL_RNG2_OSC

Set Sleep Timer Clock Source as RNG2.

Definition at line 117 of file gr55xx_hal_sleep_timer.h.

## ◆ SLEEP_TIMER_CLK_SEL_RNG_OSC

#define SLEEP_TIMER_CLK_SEL_RNG_OSC LL_SLEEP_TIMER_CLK_SEL_RNG_OSC

Set Sleep Timer Clock Source as RNG.

Definition at line 115 of file gr55xx_hal_sleep_timer.h.

## ◆ SLEEP_TIMER_CLK_SEL_RTC_OSC

#define SLEEP_TIMER_CLK_SEL_RTC_OSC LL_SLEEP_TIMER_CLK_SEL_RTC_OSC

Set Sleep Timer Clock Source as RTC.

Definition at line 118 of file gr55xx_hal_sleep_timer.h.

## ◆ SLEEP_TIMER_CLK_SEL_XO

#define SLEEP_TIMER_CLK_SEL_XO LL_SLEEP_TIMER_CLK_SEL_XO

Set Sleep Timer Clock Source as XO.

Definition at line 116 of file gr55xx_hal_sleep_timer.h.