Public Attributes | List of all members
app_pdm_pin_t Struct Reference
Peripheral Driver » APP DRIVER » PDM » Structures

PDM IO configuration Structures. More...

`#include <app_pdm.h>`

## Public Attributes
app_io_type_t | type
app_io_mux_t | mux
uint32_t | pin
app_io_pull_t | pull

## Detailed Description

PDM IO configuration Structures.

Definition at line 91 of file app_pdm.h.

## Member Data Documentation

## ◆ mux

app_io_mux_t app_pdm_pin_t::mux

Specifies the Peripheral to be connected to the selected pins.

Definition at line 94 of file app_pdm.h.

## ◆ pin

uint32_t app_pdm_pin_t::pin

Specifies the IO pins to be configured.

Definition at line 95 of file app_pdm.h.

## ◆ pull

app_io_pull_t app_pdm_pin_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

Definition at line 96 of file app_pdm.h.

## ◆ type

app_io_type_t app_pdm_pin_t::type

Specifies the type of PDM IO.

Definition at line 93 of file app_pdm.h.

The documentation for this struct was generated from the following file:

- app_pdm.h