Macros
RX FIFO Threshold
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_RX_FIFO_TH_CHAR_1 0x00000000U
#define | LL_I2C_RX_FIFO_TH_CHAR_2 0x00000001U
#define | LL_I2C_RX_FIFO_TH_CHAR_3 0x00000002U
#define | LL_I2C_RX_FIFO_TH_CHAR_4 0x00000003U
#define | LL_I2C_RX_FIFO_TH_CHAR_5 0x00000004U
#define | LL_I2C_RX_FIFO_TH_CHAR_6 0x00000005U
#define | LL_I2C_RX_FIFO_TH_CHAR_7 0x00000006U
#define | LL_I2C_RX_FIFO_TH_CHAR_8 0x00000007U
#define | LL_I2C_RX_FIFO_TH_CHAR_9 0x00000008U
#define | LL_I2C_RX_FIFO_TH_CHAR_10 0x00000009U
#define | LL_I2C_RX_FIFO_TH_CHAR_11 0x0000000AU
#define | LL_I2C_RX_FIFO_TH_CHAR_12 0x0000000BU
#define | LL_I2C_RX_FIFO_TH_CHAR_13 0x0000000CU
#define | LL_I2C_RX_FIFO_TH_CHAR_14 0x0000000DU
#define | LL_I2C_RX_FIFO_TH_CHAR_15 0x0000000EU
#define | LL_I2C_RX_FIFO_TH_CHAR_16 0x0000000FU
#define | LL_I2C_RX_FIFO_TH_CHAR_17 0x00000010U
#define | LL_I2C_RX_FIFO_TH_CHAR_18 0x00000011U
#define | LL_I2C_RX_FIFO_TH_CHAR_19 0x00000012U
#define | LL_I2C_RX_FIFO_TH_CHAR_20 0x00000013U
#define | LL_I2C_RX_FIFO_TH_CHAR_21 0x00000014U
#define | LL_I2C_RX_FIFO_TH_CHAR_22 0x00000015U
#define | LL_I2C_RX_FIFO_TH_CHAR_23 0x00000016U
#define | LL_I2C_RX_FIFO_TH_CHAR_24 0x00000017U
#define | LL_I2C_RX_FIFO_TH_CHAR_25 0x00000018U
#define | LL_I2C_RX_FIFO_TH_CHAR_26 0x00000019U
#define | LL_I2C_RX_FIFO_TH_CHAR_27 0x0000001AU
#define | LL_I2C_RX_FIFO_TH_CHAR_28 0x0000001BU
#define | LL_I2C_RX_FIFO_TH_CHAR_29 0x0000001CU
#define | LL_I2C_RX_FIFO_TH_CHAR_30 0x0000001DU
#define | LL_I2C_RX_FIFO_TH_CHAR_31 0x0000001EU
#define | LL_I2C_RX_FIFO_TH_CHAR_32 0x0000001FU
#define | LL_I2C_RX_FIFO_TH_FULL 0x00000020U

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_RX_FIFO_TH_CHAR_1

#define LL_I2C_RX_FIFO_TH_CHAR_1 0x00000000U

1 character in RX FIFO

Definition at line 253 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_10

#define LL_I2C_RX_FIFO_TH_CHAR_10 0x00000009U

10 characters in RX FIFO

Definition at line 262 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_11

#define LL_I2C_RX_FIFO_TH_CHAR_11 0x0000000AU

11 characters in RX FIFO

Definition at line 263 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_12

#define LL_I2C_RX_FIFO_TH_CHAR_12 0x0000000BU

12 characters in RX FIFO

Definition at line 264 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_13

#define LL_I2C_RX_FIFO_TH_CHAR_13 0x0000000CU

13 characters in RX FIFO

Definition at line 265 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_14

#define LL_I2C_RX_FIFO_TH_CHAR_14 0x0000000DU

14 characters in RX FIFO

Definition at line 266 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_15

#define LL_I2C_RX_FIFO_TH_CHAR_15 0x0000000EU

15 character in RX FIFO

Definition at line 267 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_16

#define LL_I2C_RX_FIFO_TH_CHAR_16 0x0000000FU

16 characters in RX FIFO

Definition at line 268 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_17

#define LL_I2C_RX_FIFO_TH_CHAR_17 0x00000010U

17 characters in RX FIFO

Definition at line 269 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_18

#define LL_I2C_RX_FIFO_TH_CHAR_18 0x00000011U

18 characters in RX FIFO

Definition at line 270 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_19

#define LL_I2C_RX_FIFO_TH_CHAR_19 0x00000012U

19 characters in RX FIFO

Definition at line 271 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_2

#define LL_I2C_RX_FIFO_TH_CHAR_2 0x00000001U

2 characters in RX FIFO

Definition at line 254 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_20

#define LL_I2C_RX_FIFO_TH_CHAR_20 0x00000013U

20 characters in RX FIFO

Definition at line 272 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_21

#define LL_I2C_RX_FIFO_TH_CHAR_21 0x00000014U

21 characters in RX FIFO

Definition at line 273 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_22

#define LL_I2C_RX_FIFO_TH_CHAR_22 0x00000015U

22 character in RX FIFO

Definition at line 274 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_23

#define LL_I2C_RX_FIFO_TH_CHAR_23 0x00000016U

23 characters in RX FIFO

Definition at line 275 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_24

#define LL_I2C_RX_FIFO_TH_CHAR_24 0x00000017U

24 characters in RX FIFO

Definition at line 276 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_25

#define LL_I2C_RX_FIFO_TH_CHAR_25 0x00000018U

25 characters in RX FIFO

Definition at line 277 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_26

#define LL_I2C_RX_FIFO_TH_CHAR_26 0x00000019U

26 characters in RX FIFO

Definition at line 278 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_27

#define LL_I2C_RX_FIFO_TH_CHAR_27 0x0000001AU

27 characters in RX FIFO

Definition at line 279 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_28

#define LL_I2C_RX_FIFO_TH_CHAR_28 0x0000001BU

28 characters in RX FIFO

Definition at line 280 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_29

#define LL_I2C_RX_FIFO_TH_CHAR_29 0x0000001CU

29 character in RX FIFO

Definition at line 281 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_3

#define LL_I2C_RX_FIFO_TH_CHAR_3 0x00000002U

3 characters in RX FIFO

Definition at line 255 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_30

#define LL_I2C_RX_FIFO_TH_CHAR_30 0x0000001DU

30 characters in RX FIFO

Definition at line 282 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_31

#define LL_I2C_RX_FIFO_TH_CHAR_31 0x0000001EU

31 characters in RX FIFO

Definition at line 283 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_32

#define LL_I2C_RX_FIFO_TH_CHAR_32 0x0000001FU

32 characters in RX FIFO

Definition at line 284 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_4

#define LL_I2C_RX_FIFO_TH_CHAR_4 0x00000003U

4 characters in RX FIFO

Definition at line 256 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_5

#define LL_I2C_RX_FIFO_TH_CHAR_5 0x00000004U

5 characters in RX FIFO

Definition at line 257 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_6

#define LL_I2C_RX_FIFO_TH_CHAR_6 0x00000005U

6 characters in RX FIFO

Definition at line 258 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_7

#define LL_I2C_RX_FIFO_TH_CHAR_7 0x00000006U

7 characters in RX FIFO

Definition at line 259 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_8

#define LL_I2C_RX_FIFO_TH_CHAR_8 0x00000007U

8 character in RX FIFO

Definition at line 260 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_9

#define LL_I2C_RX_FIFO_TH_CHAR_9 0x00000008U

9 characters in RX FIFO

Definition at line 261 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_FULL

#define LL_I2C_RX_FIFO_TH_FULL 0x00000020U

RX FIFO full

Definition at line 285 of file gr55xx_ll_i2c.h.