Enumerations
Enumerations
BLE Services » Link Loss Service Client (LLS_C)

## Enumerations
enum | lls_c_alert_level_t { LLS_C_ALERT_LEVEL_NO_ALERT, LLS_C_ALERT_LEVEL_MILD_ALERT, LLS_C_ALERT_LEVEL_HIGH_ALERT }
| Link Loss Service Client alert levels. More...
enum | lls_c_evt_type_t { LLS_C_EVT_INVALID, LLS_C_EVT_DISCOVERY_COMPLETE, LLS_C_EVT_DISCOVERY_FAIL, LLS_C_EVT_ALERT_LEVEL_SET_SUCCESS, LLS_C_EVT_ALERT_LEVEL_SET_ERR, LLS_C_EVT_ALERT_LEVEL_RECEIVE }
| Link Loss Service Client event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ lls_c_alert_level_t

enum lls_c_alert_level_t

Link Loss Service Client alert levels.

Enumerator
LLS_C_ALERT_LEVEL_NO_ALERT | No alert.
LLS_C_ALERT_LEVEL_MILD_ALERT | Mild alert.
LLS_C_ALERT_LEVEL_HIGH_ALERT | High alert.

Definition at line 77 of file lls_c.h.

## ◆ lls_c_evt_type_t

enum lls_c_evt_type_t

Link Loss Service Client event type.

Enumerator
LLS_C_EVT_INVALID | LLS Client invalid event.
LLS_C_EVT_DISCOVERY_COMPLETE | LLS Client has found LLS service and its characteristics.
LLS_C_EVT_DISCOVERY_FAIL | LLS Client found LLS service failed because of invalid operation or no found at the peer.
LLS_C_EVT_ALERT_LEVEL_SET_SUCCESS | LLS Client has set Alert Level characteristics.
LLS_C_EVT_ALERT_LEVEL_SET_ERR | Error occured when LLS Client set Alert Level characteristics.
LLS_C_EVT_ALERT_LEVEL_RECEIVE | LLS Client has received Alert Level value.

Definition at line 85 of file lls_c.h.