Enumerations
Enumerations
BLE » Light Communication Protocol (LCP)

## Enumerations
enum | LCP_RATE { LCP_RATE_1MBPS = 0, LCP_RATE_2MBPS }
enum | PROTOCOL_MODE { BLE_ADV = 0, BLE_SCAN = 1, LCP_TRX_MODE_SW_TX = 2, LCP_TRX_MODE_SW_RX = 3, LCP_TRX_MODE_TIMER_TX = 4, LCP_TRX_MODE_TIMER_RX = 5 }
| Protocol Mode. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ LCP_RATE

enum LCP_RATE

Enumerator
LCP_RATE_1MBPS |
LCP_RATE_2MBPS |

Definition at line 65 of file ble_lcp.h.

## ◆ PROTOCOL_MODE

enum PROTOCOL_MODE

Protocol Mode.

Enumerator
BLE_ADV | BLE ADV mode.
BLE_SCAN | BLE SCAN mode.
LCP_TRX_MODE_SW_TX |
LCP_TRX_MODE_SW_RX |
LCP_TRX_MODE_TIMER_TX |
LCP_TRX_MODE_TIMER_RX |

Definition at line 72 of file ble_lcp.h.