gr55xx_hal_aon_gpio_ex.h
Go to the documentation of this file.
1
51 /* Define to prevent recursive inclusion -------------------------------------*/
52 #ifndef __GR55xx_HAL_AON_GPIO_EX_H__
53 #define __GR55xx_HAL_AON_GPIO_EX_H__
54
55 #ifdef __cplusplus
56 extern "C" {
57 #endif
58
59 /* Includes ------------------------------------------------------------------*/
60 #include "gr55xx_hal_def.h"
61 #include "gr55xx_ll_gpio.h"
62
63 /* Exported types ------------------------------------------------------------*/
64
70 /* Exported constants --------------------------------------------------------*/
78 #define AON_GPIO_MUX_0 LL_AON_GPIO_MUX_0
79 #define AON_GPIO_MUX_1 LL_AON_GPIO_MUX_1
80 #define AON_GPIO_MUX_2 LL_AON_GPIO_MUX_2
81 #define AON_GPIO_MUX_3 LL_AON_GPIO_MUX_3
82 #define AON_GPIO_MUX_4 LL_AON_GPIO_MUX_4
83 #define AON_GPIO_MUX_5 LL_AON_GPIO_MUX_5
84 #define AON_GPIO_MUX_6 LL_AON_GPIO_MUX_6
85 #define AON_GPIO_MUX_7 LL_AON_GPIO_MUX_7
92 #if defined (GR551xx)
93 /*---------------------------------- GR551xx ------------------------------*/
94
99 #define AON_GPIO_PIN_MUX_GPIO AON_GPIO_MUX_7
106 #define AON_GPIO_PIN1_MUX_QSPIM0_CS_N AON_GPIO_MUX_5
107 #define AON_GPIO_PIN1_MUX_COEX_BLE_TX AON_GPIO_MUX_6
113 #define AON_GPIO_PIN2_MUX_SIM_PRESENCE AON_GPIO_MUX_0
114 #define AON_GPIO_PIN2_MUX_QSPIM1_CS_N AON_GPIO_MUX_1
115 #define AON_GPIO_PIN2_MUX_I2S_WS AON_GPIO_MUX_2
116 #define AON_GPIO_PIN2_MUX_I2S_S_WS AON_GPIO_MUX_3
117 #define AON_GPIO_PIN2_MUX_PWM0_C AON_GPIO_MUX_5
118 #define AON_GPIO_PIN2_MUX_COEX_BLE_PROC AON_GPIO_MUX_6
124 #define AON_GPIO_PIN3_MUX_SIM_RST_N AON_GPIO_MUX_0
125 #define AON_GPIO_PIN3_MUX_QSPIM1_IO_0 AON_GPIO_MUX_1
126 #define AON_GPIO_PIN3_MUX_I2S_TX_SDO AON_GPIO_MUX_2
127 #define AON_GPIO_PIN3_MUX_I2S_S_TX_SDO AON_GPIO_MUX_3
128 #define AON_GPIO_PIN3_MUX_PWM1_A AON_GPIO_MUX_5
129 #define AON_GPIO_PIN3_MUX_COEX_WLAN_RX AON_GPIO_MUX_6
135 #define AON_GPIO_PIN4_MUX_SIM_IO AON_GPIO_MUX_0
136 #define AON_GPIO_PIN4_MUX_QSPIM1_IO_1 AON_GPIO_MUX_1
137 #define AON_GPIO_PIN4_MUX_I2S_RX_SDI AON_GPIO_MUX_2
138 #define AON_GPIO_PIN4_MUX_I2S_S_RX_SDI AON_GPIO_MUX_3
139 #define AON_GPIO_PIN4_MUX_PWM1_B AON_GPIO_MUX_5
140 #define AON_GPIO_PIN4_MUX_COEX_BLE_RX AON_GPIO_MUX_6
146 #define AON_GPIO_PIN5_MUX_SIM_CLK AON_GPIO_MUX_0
147 #define AON_GPIO_PIN5_MUX_QSPIM1_CLK AON_GPIO_MUX_1
148 #define AON_GPIO_PIN5_MUX_I2S_SCLK AON_GPIO_MUX_2
149 #define AON_GPIO_PIN5_MUX_I2S_S_SCLK AON_GPIO_MUX_3
150 #define AON_GPIO_PIN5_MUX_PWM1_C AON_GPIO_MUX_5
151 #define AON_GPIO_PIN5_MUX_COEX_WLAN_TX AON_GPIO_MUX_6
159 #define IS_AON_GPIO_MUX(__MUX__) (((__MUX__) <= AON_GPIO_MUX_7))
160
161 /*------------------------------------------------------------------------------------------*/
162 #endif /* GR551xx */
163
170 #ifdef __cplusplus
171 }
172 #endif
173
174 #endif /* __GR55xx_HAL_AON_GPIO_EX_H__ */
175
gr55xx_ll_gpio.h
Header file containing functions prototypes of GPIO LL library.
gr55xx_hal_def.h
This file contains HAL common definitions, enumeration, macros and structures definitions.