Data Fields
gattc_browse_attr_char_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Client » Structures

GATTC Browse information about Characteristic. More...

`#include <ble_gattc.h>`

## Data Fields
uint8_t | attr_type
uint8_t | prop
uint16_t | handle
uint8_t | uuid_len
uint8_t | uuid [BLE_ATT_UUID_128_LEN]

## Detailed Description

GATTC Browse information about Characteristic.

## Field Documentation

## ◆ attr_type

uint8_t gattc_browse_attr_char_t::attr_type

Attribute type. See BLE_GATTC_BROWSE_ATTR_CHAR for Characteristic Declaration.

## ◆ handle

uint16_t gattc_browse_attr_char_t::handle

Value handle.

## ◆ prop

uint8_t gattc_browse_attr_char_t::prop

Value property.

## ◆ uuid

uint8_t gattc_browse_attr_char_t::uuid[BLE_ATT_UUID_128_LEN]

Characteristic UUID.

## ◆ uuid_len

uint8_t gattc_browse_attr_char_t::uuid_len

Characteristic UUID length.

The documentation for this struct was generated from the following file:

- ble_gattc.h